----- timezone:GMT
10-17 14:43:30.254943   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:30.254970   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:30.255020   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:30.255109   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:30.255178   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:43:30.255275   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:43:30.255371   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:30.255408   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:30.255462   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:30.255498   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:30.255550   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:30.255596   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:30.255786   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:30.262939   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:43:30.263070   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:30.263161   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:43:30.263213   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:30.263280   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:43:30.263325   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:30.263379   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:43:30.263419   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:30.263587   721   768 I AT      : AT read end: 46
10-17 14:43:30.263650   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:30.263679   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:30.263725   721   768 D AT      : AT< OK
10-17 14:43:30.263755   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:43:30.263797   721   768 I AT      : AT read start
10-17 14:43:30.265235   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:43:30.265328   721   751 D RIL     : requestQueryThermal success
10-17 14:43:30.265367   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:30.265403   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:43:30.265450   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:43:30.265519   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f97856690 
10-17 14:43:30.265563   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:43:30.265597   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:32.447447   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 184963/0
10-17 14:43:33.892044   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:43:33.892142   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:43:33.892227   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:43:33.892286   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:33.892421   721   765 I AT      : AT read end: 37
10-17 14:43:33.892474   721   765 D AT      : AT< +ECSQ: 38,99,-291,1,1,1,1,3,32767
10-17 14:43:33.892508   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 38,99,-291,1,1,1,1,3,32767
10-17 14:43:33.892558   721   765 D RIL     : Nw URC:+ECSQ: 38,99,-291,1,1,1,1,3,32767
10-17 14:43:33.892636   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:43:33.892675   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:43:33.892703   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:33.892780   721   765 I AT      : AT read start
10-17 14:43:33.893186  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:43:33.893470  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -285 1 1
10-17 14:43:33.893579  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -291 1 1
10-17 14:43:33.893617  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:34.245821  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:43:34.247317  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:43:34.247466  1450  1450 D RILJ    : [9459]> SCREEN_STATE: false [SUB0]
10-17 14:43:34.253428  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:43:34.254017   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:43:34.254099   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9300, pRI=0x7f9784c360, p=0x7f97856930, pUCI=0x0
10-17 14:43:34.254134   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97856930 dispatched to RIL_CMD_PROXY_3
10-17 14:43:34.254244   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.254252   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.254275   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.254300   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.254361   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.254391   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.254436   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.254499   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.254526   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.254590   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.254602   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.254660   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.254694   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:34.254736   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.254762   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.254806   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.254817  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:43:34.254833   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.254873   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.254900   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.254924  1450  1450 D RILJ    : [9460]> SCREEN_STATE: false [SUB1]
10-17 14:43:34.254939   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:34.254971   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:34.255006   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97856930 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:34.255040   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.255072   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:34.255101   721   749 D RIL     : radioState:10
10-17 14:43:34.255163   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.255194   721   749 D AT      : AT> AT+CREG=1
10-17 14:43:34.255218   721   749 I AT      : AT write start
10-17 14:43:34.255316   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.255351   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.256267   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.256397   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.256494   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.256563   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.256651   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:34.257640   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:43:34.257724   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cdaa00, pRI=0x7f9784c510, p=0x7f978569a0, pUCI=0x0
10-17 14:43:34.257761   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c510 p=0x7f978569a0 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:34.257912   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.257912   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.257943   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.257963   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.257995   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.258020   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.258063   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.258070   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.258120   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.258146   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.258182   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.258226   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.258327   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.258366   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:34.258399   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c510 p=0x7f978569a0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:34.258431   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.258462   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:34.258489   721   755 D RIL     : radioState:0
10-17 14:43:34.258527   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.258554   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.258593   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.258644   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.258674   721   755 D AT      : AT> AT+CREG=1
10-17 14:43:34.258698   721   755 I AT      : AT write start
10-17 14:43:34.258791   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.258819   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.258863   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.258888   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.258924   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.258948   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.258985   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.259011   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.259466   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.259532   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.259579   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.259656   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:34.264258   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.264315   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.264476   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.264542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.264642   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.264650   721   766 I AT      : AT read end: 6
10-17 14:43:34.264691   721   766 D AT      : AT< OK
10-17 14:43:34.264695   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.264761   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.264803   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.264721   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.264901   721   772 I AT      : AT read end: 6
10-17 14:43:34.264943   721   772 D AT      : AT< OK
10-17 14:43:34.264963   721   766 I AT      : AT read start
10-17 14:43:34.264980   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.265027   721   772 I AT      : AT read start
10-17 14:43:34.265094   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.265145   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.265171   721   749 D AT      : AT> AT+CGREG=1
10-17 14:43:34.265193   721   749 I AT      : AT write start
10-17 14:43:34.265435   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.265451   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.265486   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.265505   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.265512   721   755 D AT      : AT> AT+CGREG=1
10-17 14:43:34.265538   721   755 I AT      : AT write start
10-17 14:43:34.265556   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.265636   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:34.265658   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.265705   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.265753   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.265827   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:34.266899   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.266968   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.267034   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.267082   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.267170   721   766 I AT      : AT read end: 6
10-17 14:43:34.267206   721   766 D AT      : AT< OK
10-17 14:43:34.267234   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.267271   721   766 I AT      : AT read start
10-17 14:43:34.267316   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.267428   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.267459   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:43:34.267482   721   749 I AT      : AT write start
10-17 14:43:34.267601   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.267649   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.267694   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.267767   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:34.267838   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.267883   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.267943   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.267986   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.268085   721   772 I AT      : AT read end: 6
10-17 14:43:34.268124   721   772 D AT      : AT< OK
10-17 14:43:34.268152   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.268193   721   772 I AT      : AT read start
10-17 14:43:34.268256   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.268299   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.268325   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:43:34.268348   721   755 I AT      : AT write start
10-17 14:43:34.268465   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.268516   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.268562   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.268654   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:34.268943   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.268996   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.269062   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.269104   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.269195   721   766 I AT      : AT read end: 6
10-17 14:43:34.269233   721   766 D AT      : AT< OK
10-17 14:43:34.269261   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.269295   721   766 I AT      : AT read start
10-17 14:43:34.269335   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.269379   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.269406   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:43:34.269433   721   749 I AT      : AT write start
10-17 14:43:34.269553   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.269598   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.269641   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.269716   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:43:34.270016   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.270071   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.270137   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.270180   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.270272   721   772 I AT      : AT read end: 6
10-17 14:43:34.270311   721   772 D AT      : AT< OK
10-17 14:43:34.270339   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.270378   721   772 I AT      : AT read start
10-17 14:43:34.270440   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.270477   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.270502   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:43:34.270524   721   755 I AT      : AT write start
10-17 14:43:34.270640   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.270689   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.270735   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.271043   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.271086   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:43:34.271112   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.271172   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.271211   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.271309   721   766 I AT      : AT read end: 6
10-17 14:43:34.271345   721   766 D AT      : AT< OK
10-17 14:43:34.271373   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.271409   721   766 I AT      : AT read start
10-17 14:43:34.271449   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.271494   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.271520   721   749 D AT      : AT> AT+CEREG=1
10-17 14:43:34.271542   721   749 I AT      : AT write start
10-17 14:43:34.271661   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.271704   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.271747   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.271825   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:34.271966   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.272011   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.272068   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.272106   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.272198   721   772 I AT      : AT read end: 6
10-17 14:43:34.272231   721   772 D AT      : AT< OK
10-17 14:43:34.272260   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.272296   721   772 I AT      : AT read start
10-17 14:43:34.272337   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.272384   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.272409   721   755 D AT      : AT> AT+CEREG=1
10-17 14:43:34.272433   721   755 I AT      : AT write start
10-17 14:43:34.272557   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.272601   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.272645   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.272721   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:34.273141   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.273191   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.273253   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.273300   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.273384   721   766 I AT      : AT read end: 6
10-17 14:43:34.273418   721   766 D AT      : AT< OK
10-17 14:43:34.273447   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.273485   721   766 I AT      : AT read start
10-17 14:43:34.273520   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.273560   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:34.273600   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:34.273675   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97856930 
10-17 14:43:34.273705   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9300
10-17 14:43:34.273730   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:34.273848  1450  1606 D RILJ    : [9459]< SCREEN_STATE  [SUB0]
10-17 14:43:34.275776   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.275857   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.275931   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.275976   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.276088   721   772 I AT      : AT read end: 6
10-17 14:43:34.276130   721   772 D AT      : AT< OK
10-17 14:43:34.276160   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.276209   721   772 I AT      : AT read start
10-17 14:43:34.276262   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.276305   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:34.276344   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:34.276416   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f978569a0 
10-17 14:43:34.276446   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaa00
10-17 14:43:34.276470   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:34.276599  1450  1609 D RILJ    : [9460]< SCREEN_STATE  [SUB1]
10-17 14:43:34.494354  1450  1450 D RILJ    : [9461]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:43:34.496532   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:43:34.496619   721   760 I RILC-MTK: create request 59: pRequest=0x7f94ce6a60, pRI=0x7f9784c6f0, p=0x7f978572d0, pUCI=0x0
10-17 14:43:34.496656   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978572d0 dispatched to RIL_ATCI_PROXY
10-17 14:43:34.496785   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.496785   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.496799   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.496819   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.496835   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.496862   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.496864   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.496886   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:34.496890   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.496925   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978572d0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:34.496927   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.496944   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.496956   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:34.496958   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.496982   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.496992   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:43:34.497007   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.497007   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.497016   721   753 D RIL     : radioState:10
10-17 14:43:34.497045   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.497057   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:43:34.497089   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:34.497092   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.497116   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:43:34.497121   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.497139   721   753 I AT      : AT write start
10-17 14:43:34.497157   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.497168   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:34.497197   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.497288   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.497336   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.497350   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:34.497385   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:34.497396   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.497443   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.497490   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:43:34.507972   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:34.508034   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:34.508112   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:34.508154   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.508252   721   770 I AT      : AT read end: 6
10-17 14:43:34.508295   721   770 D AT      : AT< OK
10-17 14:43:34.508324   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:34.508364   721   770 I AT      : AT read start
10-17 14:43:34.508412   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:34.508452   721   753 D RIL     : p_response->success = 1
10-17 14:43:34.508479   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:34.508507   721   753 D RIL     : strLength = 6
10-17 14:43:34.508563   721   753 D RIL     : line = <
10-17 14:43:34.508563   721   753 D RIL     : OK
10-17 14:43:34.508563   721   753 D RIL     : >
10-17 14:43:34.508593   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:34.508638   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:34.508710   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f978572d0 
10-17 14:43:34.508743   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a60
10-17 14:43:34.508778   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.508920  1450  1606 D RILJ    : [9461]< OEM_HOOK_RAW [B@c305e66 [SUB0]
10-17 14:43:34.681649  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.683068  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.683546  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.703939  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:34.704396  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:34.716793  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:34.724224  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:43:34.731062  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:34.816039  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.818590  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.818956  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.843314  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.845147  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.854631  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:43:34.856981  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:34.857080  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:43:34.850858  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.860461   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:34.860752   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:34.861806  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:34.861944  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:43:34.864633   909  1190 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:34.864911   909  1190 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:34.899480  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:34.899591  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:43:34.899712  1450  1450 D RILJ    : [9462]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:43:34.904281  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:43:34.905156   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:43:34.905246   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cf93a0, pRI=0x7f9784c240, p=0x7f97857420, pUCI=0x0
10-17 14:43:34.905281   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c240 p=0x7f97857420 dispatched to RIL_CMD_PROXY_3
10-17 14:43:34.905502   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.905572   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.905647   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.905685   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:34.905738   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.905771   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.905813   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.905839   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.905879   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.905906   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.905947   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.905973   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.906012   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.906037   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.906077   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:34.906107   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:34.906140   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c240 p=0x7f97857420 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:34.906171   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.906203   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:43:34.906230   721   749 D RIL     : radioState:10
10-17 14:43:34.906271   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:43:34.906304   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:43:34.906336   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.906361   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:43:34.906388   721   749 I AT      : AT write start
10-17 14:43:34.906496   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.906527   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.906569   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.906593   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.906719   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.906748   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.907667   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.907755   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.907811   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.907917   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:34.908087   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.908145   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.915528   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.915632   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.915714   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.915760   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.916092   721   766 I AT      : AT read end: 6
10-17 14:43:34.916153   721   766 D AT      : AT< OK
10-17 14:43:34.916188   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.916234   721   766 I AT      : AT read start
10-17 14:43:34.916288   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.916331   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:34.916378   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:34.916456   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97857420 
10-17 14:43:34.916497   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf93a0
10-17 14:43:34.916525   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:34.916743  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:43:34.916864  1450  1606 D RILJ    : [9462]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:43:34.921460  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.922712  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.923166  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.928647  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:43:34.928847  1450  1450 D RILJ    : [9463]> SCREEN_STATE: true [SUB0]
10-17 14:43:34.932995  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:43:34.933260   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:43:34.933335   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6a20, pRI=0x7f9784c300, p=0x7f97857d50, pUCI=0x0
10-17 14:43:34.933368   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c300 p=0x7f97857d50 dispatched to RIL_CMD_PROXY_3
10-17 14:43:34.933583   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.933625   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.933987   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.934038   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.934082   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.934109   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:34.934152   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.934180   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.934223   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.934248   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.934288   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.934313   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.934351   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.934375   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.934418   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.934443   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.934485   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.934511   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.934551   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.934576   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.934614   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.934640   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.934681   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:34.934711   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:34.934745   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c300 p=0x7f97857d50 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:34.934776   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.934810   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:34.934835   721   749 D RIL     : radioState:10
10-17 14:43:34.934892   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.934921   721   749 D AT      : AT> AT+CREG=3
10-17 14:43:34.934948   721   749 I AT      : AT write start
10-17 14:43:34.935599  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:43:34.935792  1450  1450 D RILJ    : [9464]> SCREEN_STATE: true [SUB1]
10-17 14:43:34.938636  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:43:34.940759  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:34.940872  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:43:34.941094  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:34.941171  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:34.941815   909  1651 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:34.941995   909  1651 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:34.942209   909  1651 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:34.944753  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:34.944944  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:43:34.945077  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:34.945143  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:34.945692   909  1551 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:34.945822   909  1551 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:34.946086   909  1551 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:34.952005   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:43:34.952002   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.952095   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9540, pRI=0x7f9784c870, p=0x7f97857e30, pUCI=0x0
10-17 14:43:34.952100   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.952132   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c870 p=0x7f97857e30 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:34.952155   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.952275   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:34.952301   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.952332   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.952331   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.952363   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.952402   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.952427   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.952471   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.952496   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.952538   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.952563   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.952600   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.952623   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.952663   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.952690   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.952730   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.952757   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.952798   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.952822   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.952859   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.952884   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.952923   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:34.952952   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:34.952984   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c870 p=0x7f97857e30 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:34.953018   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:34.953051   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:34.953078   721   755 D RIL     : radioState:0
10-17 14:43:34.953116   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.953143   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.953168   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:34.953220   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.953254   721   755 D AT      : AT> AT+CREG=3
10-17 14:43:34.953278   721   755 I AT      : AT write start
10-17 14:43:34.953578   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.953660   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.953715   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.953803   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:34.957827  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.958701  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.959046  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.960265   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:43:34.960366   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:43:34.960440   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:43:34.960483   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.960534   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.960575   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.960628   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.960669   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.961226   721   766 I AT      : AT read end: 6
10-17 14:43:34.961301   721   766 D AT      : AT< OK
10-17 14:43:34.961334   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.961389   721   766 I AT      : AT read start
10-17 14:43:34.961526   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.961595   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.961622   721   749 D AT      : AT> AT+CGREG=3
10-17 14:43:34.961648   721   749 I AT      : AT write start
10-17 14:43:34.961769   721   765 I AT      : AT read end: 36
10-17 14:43:34.961802   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:34.961829   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:34.961864   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:34.961898   721   765 D RIL     : NW state changed: normal case
10-17 14:43:34.961927   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:43:34.961958   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:34.961991   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:43:34.962043   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:43:34.962075   721   765 D RIL     : bCREGType3Support=1
10-17 14:43:34.962102   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:43:34.962128   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:43:34.962210   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:43:34.962240   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:34.962306   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e434e0
10-17 14:43:34.962341   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e434f0
10-17 14:43:34.962436   721   765 I AT      : AT read start
10-17 14:43:34.962711  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:43:34.970708  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:34.971117  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:43:34.971249  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:43:34.971374  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:43:34.972170  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:34.974714  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:34.976073   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.976167   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.976222   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.976318   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:34.976758   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:43:34.976842   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:43:34.976936   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:43:34.976982   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.977036   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.977077   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.977133   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.977172   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.977341   721   771 I AT      : AT read end: 36
10-17 14:43:34.977397   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:34.977432   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:34.977477   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:34.977519   721   771 D RIL     : NW state changed: normal case
10-17 14:43:34.977553   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:43:34.977587   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:43:34.977617   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:43:34.977676   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:43:34.977711   721   771 D RIL     : bCREGType3Support=1
10-17 14:43:34.977742   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:43:34.977769   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:43:34.977860   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:43:34.977896   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:34.977974   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e434e0, cancel
10-17 14:43:34.978010   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e437e0
10-17 14:43:34.978044   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e437f0
10-17 14:43:34.978120   721   771 I AT      : AT read start
10-17 14:43:34.981291   721   772 I AT      : AT read end: 6
10-17 14:43:34.981348   721   772 D AT      : AT< OK
10-17 14:43:34.981375   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.981417   721   772 I AT      : AT read start
10-17 14:43:34.982240  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:43:34.982514   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.982579   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.982608   721   755 D AT      : AT> AT+CGREG=3
10-17 14:43:34.982632   721   755 I AT      : AT write start
10-17 14:43:34.983005   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.983059   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.983110   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.983189   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:34.983485  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:43:34.983587  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:43:34.983689  1450  1450 D RILJ    : [9465]> OPERATOR [SUB0]
10-17 14:43:34.984882   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.984970   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.985052   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.985108   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.985238   721   766 I AT      : AT read end: 6
10-17 14:43:34.985296   721   766 D AT      : AT< OK
10-17 14:43:34.985344   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.985388   721   766 I AT      : AT read start
10-17 14:43:34.985464   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.985504   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.985530   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:43:34.985551   721   749 I AT      : AT write start
10-17 14:43:34.985875   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.985924   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.985974   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.986054   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:34.986144   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.986190   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.986257   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.986297   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.986317  1450  1450 D RILJ    : [9466]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:43:34.988808   721   772 I AT      : AT read end: 6
10-17 14:43:34.988883   721   772 D AT      : AT< OK
10-17 14:43:34.988924   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.988976   721   772 I AT      : AT read start
10-17 14:43:34.989139  1450  1450 D RILJ    : [9467]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:43:34.989667   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.989734   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:34.989740   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:43:34.989766   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:43:34.989803   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9b80, pRI=0x7f9784c9c0, p=0x7f97857f10, pUCI=0x0
10-17 14:43:34.989794   721   755 I AT      : AT write start
10-17 14:43:34.989844   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784c9c0 p=0x7f97857f10 dispatched to RIL_CMD_PROXY_3
10-17 14:43:34.989965   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:43:34.989984   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:34.990015   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:34.990026   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cdaac0, pRI=0x7f9784ca50, p=0x7f97857f80, pUCI=0x0
10-17 14:43:34.990060   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c9c0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.990091   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:34.990128   721   760 D RILC-MTK: Request pRI=0x7f9784ca50 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:43:34.990267   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:34.990302   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:34.990368   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:34.990397   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:34.990441   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:34.990468   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:34.990511   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:34.990537   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:34.990579   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:34.990621   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:34.990667   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:34.990696   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:34.990732   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:34.990737   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:34.990771   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:34.990969  1450  1450 D RILJ    : [9468]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:43:34.991252   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:34.991270   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.991335   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.991343   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:34.991373   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:34.991398   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:34.991501   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:34.991874   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:43:34.991982   721   760 I RILC-MTK: create request 20: pRequest=0x7f94ce6aa0, pRI=0x7f9784cb10, p=0x7f97857ff0, pUCI=0x0
10-17 14:43:34.992022   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c9c0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.992064   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784ca50 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.992095   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:34.992128   721   760 D RILC-MTK: Request pRI=0x7f9784cb10 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:43:34.992876  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:34.993044   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:34.993100  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:34.993112   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:34.993212  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:43:34.993244   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:34.993296   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.993417   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:43:34.993486   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9240, pRI=0x7f9784cb40, p=0x7f97858140, pUCI=0x0
10-17 14:43:34.993541   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c9c0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.993574   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784ca50 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.993608   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857ff0 is queued in RIL_CMD_PROXY_3
10-17 14:43:34.993610  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:43:34.993649   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:34.993684   721   760 D RILC-MTK: Request pRI=0x7f9784cb40 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:43:34.993705  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:43:34.993782  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:43:34.993837  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:43:34.994615   721   766 I AT      : AT read end: 6
10-17 14:43:34.994672   721   766 D AT      : AT< OK
10-17 14:43:34.994708   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:34.994777   721   766 I AT      : AT read start
10-17 14:43:34.995164   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.995231   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:34.995259   721   749 D AT      : AT> AT+ECSQ
10-17 14:43:34.995282   721   749 I AT      : AT write start
10-17 14:43:34.995480   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:34.995591   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:34.995648   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:34.995744   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:43:34.999182   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:34.999269   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:34.999353   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:34.999491   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:34.999781   721   772 I AT      : AT read end: 6
10-17 14:43:34.999840   721   772 D AT      : AT< OK
10-17 14:43:34.999876   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:34.999919   721   772 I AT      : AT read start
10-17 14:43:34.999931   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:43:34.999989   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.000059   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:43:35.000101   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.000195   721   766 I AT      : AT read end: 37
10-17 14:43:35.000225   721   766 D AT      : AT< +ECSQ: 38,99,-291,1,1,1,1,3,32767
10-17 14:43:35.000251   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 38,99,-291,1,1,1,1,3,32767
10-17 14:43:35.000287   721   766 I AT      : AT read start
10-17 14:43:35.000312   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.000382   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.000410   721   755 D AT      : AT> AT+ECSQ
10-17 14:43:35.000436   721   755 I AT      : AT write start
10-17 14:43:35.000628   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.000681   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.000734   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:35.000820   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:43:35.002409   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.002503   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.002570   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.002610   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.002658   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:43:35.002699   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.002748   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:43:35.002786   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.002827   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:35.002869   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.002911   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:35.002949   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.003053   721   766 I AT      : AT read end: 6
10-17 14:43:35.003093   721   766 D AT      : AT< OK
10-17 14:43:35.003123   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.003165   721   766 I AT      : AT read start
10-17 14:43:35.003211   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.003220   721   772 I AT      : AT read end: 42
10-17 14:43:35.003250   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:43:35.003279   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:43:35.003293   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:43:35.003307   721   772 D AT      : AT< OK
10-17 14:43:35.003333   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:35.003333   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:43:35.003376   721   772 I AT      : AT read start
10-17 14:43:35.003387   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.003463   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.003492   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:43:35.003518   721   749 I AT      : AT write start
10-17 14:43:35.003671   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.003687   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.003744   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.003731   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:43:35.003798   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.003799   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:43:35.003834   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.003865   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:43:35.003888   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:43:35.003889   721   755 I AT      : AT write start
10-17 14:43:35.004102   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.004175   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.004235   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:35.004334   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:43:35.005245   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.005351   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.005502   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.005542   721   766 I AT      : AT read end: 6
10-17 14:43:35.005679   721   766 D AT      : AT< OK
10-17 14:43:35.005690   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.005721   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.005761   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:35.005789   721   766 I AT      : AT read start
10-17 14:43:35.005808   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.005895   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.005944   721   772 I AT      : AT read end: 6
10-17 14:43:35.005982   721   772 D AT      : AT< OK
10-17 14:43:35.006003   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.006013   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:35.006068   721   772 I AT      : AT read start
10-17 14:43:35.006041   721   749 D AT      : AT> AT+CEREG=3
10-17 14:43:35.006099   721   749 I AT      : AT write start
10-17 14:43:35.006178   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:35.006251   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.006298   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.006287   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.006352   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.006380   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.006402   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.006408   721   755 D AT      : AT> AT+CEREG=3
10-17 14:43:35.006433   721   755 I AT      : AT write start
10-17 14:43:35.006489   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:35.006576   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.006616   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.006664   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:35.006741   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:35.007141   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.007186   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.007268   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.007279   721   766 I AT      : AT read end: 6
10-17 14:43:35.007309   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.007314   721   766 D AT      : AT< OK
10-17 14:43:35.007350   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.007390   721   766 I AT      : AT read start
10-17 14:43:35.007438   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.007478   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.007527   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.007599   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f97857d50 
10-17 14:43:35.007641   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:43:35.007673   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:35.007703   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784c9c0 p=0x7f97857f10 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:35.007734   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.007764   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:43:35.007792   721   749 D RIL     : radioState:10
10-17 14:43:35.007796  1450  1606 D RILJ    : [9463]< SCREEN_STATE  [SUB0]
10-17 14:43:35.007831   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.007860   721   749 D AT      : AT> AT+COPS?
10-17 14:43:35.007883   721   749 I AT      : AT write start
10-17 14:43:35.008073   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.008137   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.008186   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.008265   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:43:35.008339   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:35.008387   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.008477   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:35.008499   721   772 I AT      : AT read end: 6
10-17 14:43:35.008521   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.008541   721   772 D AT      : AT< OK
10-17 14:43:35.008574   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:35.008626   721   772 I AT      : AT read start
10-17 14:43:35.008693   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.008747   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:35.008804   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:35.008903   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c870 p=0x7f97857e30 
10-17 14:43:35.008944   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9540
10-17 14:43:35.008977   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:35.009181  1450  1609 D RILJ    : [9464]< SCREEN_STATE  [SUB1]
10-17 14:43:35.009665   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:43:35.009812   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.009944   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:43:35.009976   721   766 I AT      : AT read end: 24
10-17 14:43:35.010001   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.010043   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:43:35.010065   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.010076   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:43:35.010107   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.010111   721   766 I AT      : AT read start
10-17 14:43:35.010202   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.010246   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.010282   721   766 I AT      : AT read end: 6
10-17 14:43:35.010316   721   766 D AT      : AT< OK
10-17 14:43:35.010343   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.010385   721   766 I AT      : AT read start
10-17 14:43:35.010438   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.010480   721   749 D RIL     : Get operator code 25020
10-17 14:43:35.010513   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:43:35.010552   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:43:35.010581   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.010637   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.010713   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c9c0 p=0x7f97857f10 
10-17 14:43:35.010743   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:43:35.010775   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:35.010805   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ca50 p=0x7f97857f80 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:35.010836   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.010864   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:43:35.011031  1450  1606 D RILJ    : [9465]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:43:35.010889   721   749 D RIL     : radioState:10
10-17 14:43:35.011224   721   749 D RIL     : request gprs reg state: normal case
10-17 14:43:35.011264   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.011290   721   749 D AT      : AT> AT+CGREG?
10-17 14:43:35.011312   721   749 I AT      : AT write start
10-17 14:43:35.011495   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.011548   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.011597   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.011679   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:35.012334   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:43:35.012391   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.012479   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:43:35.012496   721   766 I AT      : AT read end: 44
10-17 14:43:35.012522   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.012538   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:43:35.012569   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:43:35.012604   721   766 I AT      : AT read start
10-17 14:43:35.012854   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.012904   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.012983   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.012982   721   766 I AT      : AT read end: 6
10-17 14:43:35.013018   721   766 D AT      : AT< OK
10-17 14:43:35.013030   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.013044   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.013081   721   766 I AT      : AT read start
10-17 14:43:35.013123   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.013166   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:35.013195   721   749 E RIL     : The value in the field <lac> :0
10-17 14:43:35.013221   721   749 D RIL     : cid: 3583
10-17 14:43:35.013245   721   749 E RIL     : The value of act: 3
10-17 14:43:35.013270   721   749 D RIL     : cause_type: 0
10-17 14:43:35.013295   721   749 D RIL     : reject_cause: 0
10-17 14:43:35.013337   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.013365   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:43:35.013388   721   749 I AT      : AT write start
10-17 14:43:35.013522   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.013568   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.013612   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.013693   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:43:35.014400   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:43:35.014452   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.014534   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:43:35.014541   721   766 I AT      : AT read end: 19
10-17 14:43:35.014573   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:43:35.014577   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.014608   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:43:35.014644   721   766 I AT      : AT read start
10-17 14:43:35.014915   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.014964   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.015051   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.015053   721   766 I AT      : AT read end: 6
10-17 14:43:35.015090   721   766 D AT      : AT< OK
10-17 14:43:35.015100   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.015121   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.015161   721   766 I AT      : AT read start
10-17 14:43:35.015211   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.015275   721   749 E RIL     : rid: 0
10-17 14:43:35.015303   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:43:35.015336   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:43:35.015366   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:43:35.015392   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:43:35.015420   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.015475   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.015551   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784ca50 p=0x7f97857f80 
10-17 14:43:35.015583   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:43:35.015614   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:35.015645   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857ff0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:35.015676   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.015704   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:43:35.015730   721   749 D RIL     : radioState:10
10-17 14:43:35.015767   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.015793   721   749 D AT      : AT> AT+CREG?
10-17 14:43:35.015781  1450  1606 D RILJ    : [9466]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:43:35.015821   721   749 I AT      : AT write start
10-17 14:43:35.015976   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.016026   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.016077   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.016163   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:43:35.016281   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.016328   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.016384   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.016478   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 1
10-17 14:43:35.017810   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:43:35.017915   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.018062   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:43:35.018092   721   766 I AT      : AT read end: 38
10-17 14:43:35.018131   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.018151   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:43:35.018188   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:43:35.018191   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.018237   721   766 I AT      : AT read start
10-17 14:43:35.018242   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.018383   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.018404   721   766 I AT      : AT read end: 6
10-17 14:43:35.018439   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.018443   721   766 D AT      : AT< OK
10-17 14:43:35.018478   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.018529   721   766 I AT      : AT read start
10-17 14:43:35.018599   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.018658   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:35.018700   721   749 E RIL     : The value in the field <lac> :127
10-17 14:43:35.018734   721   749 D RIL     : cid: 3583
10-17 14:43:35.018763   721   749 E RIL     : The value of act: 3
10-17 14:43:35.018795   721   749 D RIL     : cause_type: 0
10-17 14:43:35.018823   721   749 D RIL     : reject_cause: 0
10-17 14:43:35.018891   721   749 E RIL     : rid: 0
10-17 14:43:35.018928   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:43:35.018964   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:43:35.018997   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:43:35.019026   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:43:35.019062   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:43:35.019108   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.019190   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.019311   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f97857ff0 
10-17 14:43:35.019362   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:43:35.019399   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:35.019435   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cb40 p=0x7f97858140 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:35.019471   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.019507   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:43:35.019540   721   749 D RIL     : radioState:10
10-17 14:43:35.019589   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.019624   721   749 D AT      : AT> AT+COPS?
10-17 14:43:35.019651   721   749 I AT      : AT write start
10-17 14:43:35.019639  1450  1606 D RILJ    : [9467]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:43:35.019895   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.019994   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.020059   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.020165   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:43:35.020405   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.020483   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.020540   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.021473   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 1
10-17 14:43:35.028066   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:43:35.028151   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.028226   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:43:35.028290   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.028343   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.028387   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.028435   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.028475   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.028587   721   766 I AT      : AT read end: 30
10-17 14:43:35.028627   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:43:35.028657   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:43:35.028693   721   766 D AT      : AT< OK
10-17 14:43:35.028718   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.028760   721   766 I AT      : AT read start
10-17 14:43:35.031205   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.031344   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.031458   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.031570   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb40 p=0x7f97858140 
10-17 14:43:35.031628   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:43:35.031672   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:35.031849  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:43:35.031997  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:43:35.032151  1450  1606 D RILJ    : [9468]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:43:35.068977  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.069069  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.069138  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:43:35.069199  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:43:35.069328  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:43:35.069382  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:43:35.069449  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:43:35.069486  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:43:35.069522  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:43:35.069571  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:43:35.069609  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:43:35.069751  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:43:35.069873  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:43:35.069945  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:43:35.070002  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:43:35.070352  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:43:35.076938  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.077320  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.077385  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:43:35.082301  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:43:35.082446  1450  1450 D RILJ    : [9469]> OPERATOR [SUB1]
10-17 14:43:35.088215  1450  1450 D RILJ    : [9470]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:43:35.088534   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:43:35.088637   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9bc0, pRI=0x7f9784cba0, p=0x7f97856930, pUCI=0x0
10-17 14:43:35.088680   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cba0 p=0x7f97856930 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:35.088828   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:35.088828   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:35.088883   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:35.088933   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:35.088982   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:35.089008   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:35.090133   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:35.090209   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:35.090269   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:35.090280  1450  1450 D RILJ    : [9471]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:43:35.090298   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:35.090343   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:35.090368   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:35.090414   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:35.090442   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:35.090483   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:35.090529   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:35.090583   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:35.090611   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:35.090652   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:35.090678   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:35.090721   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:35.090748   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:35.090789   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:35.090827   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:35.090865   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784cba0 p=0x7f97856930 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:35.090979   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.091032   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:43:35.091060   721   755 D RIL     : radioState:0
10-17 14:43:35.091102   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.091128   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.091155   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.091181   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.091222   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:35.091250   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:35.091299   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:35.091384   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f97856930 
10-17 14:43:35.091419   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9bc0
10-17 14:43:35.091449   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:35.092047  1450  1609 D RilRequest: [9469]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:35.093088  1450  1450 D RILJ    : [9472]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:43:35.093463   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:43:35.093545   721   760 I RILC-MTK: create request 21: pRequest=0x7f94ce6a20, pRI=0x7f9784c240, p=0x7f97857110, pUCI=0x0
10-17 14:43:35.093579   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97857110 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:35.093712   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:43:35.093716   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:35.093759   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:35.093775   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9100, pRI=0x7f9784c300, p=0x7f978571f0, pUCI=0x0
10-17 14:43:35.093810   721   760 D RILC-MTK: 1:DATA_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97857110 is queued in RIL_CMD2_PROXY_3
10-17 14:43:35.093841   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD2_PROXY_3 is OPERATOR ****
10-17 14:43:35.093876   721   760 D RILC-MTK: Request pRI=0x7f9784c300 to RIL_CMD2_PROXY_3 is busy. total:2 requests pending
10-17 14:43:35.093978   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:35.094008   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:35.094053   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:35.094077   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:35.094117   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:35.094147   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:35.094191   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:35.094237   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:35.094280   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:35.094306   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:35.094348   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:35.094376   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:35.094510   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:35.094537   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:35.094584   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:35.094610   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:35.094650   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:35.094680   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:35.094713   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97857110 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:35.094747   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.094778   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:43:35.094771   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:35.094807   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:35.094807   721   755 D RIL     : radioState:0
10-17 14:43:35.094853   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.094854   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:35.094881   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:35.094882   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.094909   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.094935   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.094972   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:35.095002   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:35.095047   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:35.095125   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97857110 
10-17 14:43:35.095159   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:43:35.095149  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:35.095196   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:35.095228   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c300 p=0x7f978571f0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:35.095244  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:43:35.095258   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.095289   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:43:35.095314   721   755 D RIL     : radioState:0
10-17 14:43:35.095345   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.095370   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.095372  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -285 1 1
10-17 14:43:35.095398   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.095423   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:35.095442  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -291 1 1
10-17 14:43:35.095456   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:35.095480  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:35.095484   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:35.095524   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:35.095543  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:43:35.095575   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f978571f0 
10-17 14:43:35.095609   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9100
10-17 14:43:35.095634   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:35.095666  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:43:35.095711  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:43:35.096206  1450  1609 D RilRequest: [9470]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:35.096360   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:43:35.096422   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9120, pRI=0x7f9784c360, p=0x7f97857340, pUCI=0x0
10-17 14:43:35.096454   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c360 p=0x7f97857340 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:35.096535  1450  1609 D RilRequest: [9471]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:35.096608   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:35.096643   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:35.096678   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:35.096711   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:35.096763   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:35.096790   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:35.096849   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:35.096882   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:35.096933   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:35.096958   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:35.097011   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:35.097036   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:35.097089   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:35.097116   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:35.097158   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:35.097184   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:35.097227   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:35.097251   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:35.097419   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:35.097470   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:35.097525   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:35.097558   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:35.097939   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:35.097987   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:35.098021   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c360 p=0x7f97857340 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:35.098050   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.098081   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:43:35.098106   721   755 D RIL     : radioState:0
10-17 14:43:35.098153   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.098182   721   755 D AT      : AT> AT+COPS?
10-17 14:43:35.098205   721   755 I AT      : AT write start
10-17 14:43:35.098370  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.098388   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.098443   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.098467  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:43:35.098493   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:35.098550  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:43:35.098585   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:43:35.098599  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:43:35.100067  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.100183  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:43:35.100263  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:43:35.100314  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:43:35.100388  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:43:35.100441  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:43:35.100499  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:43:35.100551  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:43:35.100679  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:43:35.103412  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:35.103988  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:35.107575   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:43:35.107678   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.107770   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:43:35.107823   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.107876   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:35.107922   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:35.107992   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:35.108036   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.108572   721   772 I AT      : AT read end: 18
10-17 14:43:35.108648   721   772 D AT      : AT< +COPS: 0
10-17 14:43:35.108739   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:43:35.108784   721   772 D AT      : AT< OK
10-17 14:43:35.108814   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:35.108856   721   772 I AT      : AT read start
10-17 14:43:35.109213   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:35.109300   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:35.109354   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:35.109447   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97857340 
10-17 14:43:35.109482   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9120
10-17 14:43:35.109510   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:35.109666  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:43:35.109765  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:43:35.109882  1450  1609 D RILJ    : [9472]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:43:35.119810  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:35.119995  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:43:35.120081  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:43:35.120128  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:43:35.120205  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:43:35.120254  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:43:35.120317  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:43:35.120354  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:35.120434  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:43:35.120496  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:43:35.120567  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:43:35.120656  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:43:35.120697  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:43:35.120873  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:43:35.121035  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:43:35.121089  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:35.121193  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:43:35.121259  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:43:35.124097  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.126708  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:43:35.126794  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:43:35.126843  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:43:35.126990  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:43:35.127143  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:43:35.127442  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:43:35.127538  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:43:35.127605  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:43:35.127670  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:43:35.127833  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:43:35.127908  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:43:35.127977  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:43:35.128072  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128154  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128229  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128274  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128317  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128373  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128417  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128459  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128503  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128551  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:35.128594  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:43:35.128649  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:43:35.128686  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:43:35.128749  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:43:35.130761  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:43:35.131784  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.131894  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:43:35.132666  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:43:35.135096  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:43:35.134
10-17 14:43:35.135322  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:43:35.136163  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.136332  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.136467  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:43:35.136539  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:43:35.136599  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.136937  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:43:35.137623   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.137730   909  2707 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:35.137928   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=0
10-17 14:43:35.138253   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143913Europe/Samara(1,290,14400,0,1476700753) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.138548   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143934Europe/Samara(1,290,14400,0,1476700774) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.138833   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.139101   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.139361   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.139416   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:43:35.139464   909  2707 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:35.139600   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.139708   909  2707 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:35.139845   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.140085   909  2707 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:35.140290   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.140860   909  2707 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:35.141529   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.141654   909  2707 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:35.141652  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:35.141794  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:35.141852  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:35.141891  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:35.141941  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=20
10-17 14:43:35.141971  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:35.141819   909  2707 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:35.142833   909  2707 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:35.179154  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:35.180112   909  2707 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:35.194890  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:43:35.195014  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:35.197434  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:35.198319  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:35.200514  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:43:35.200631  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:43:35.200678  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:35.200748  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:43:35.200792  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:35.200832  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:35.200890  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:43:35.201006  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:35.201041  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:35.201097  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:43:35.201132  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:35.201161  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:35.201288  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:43:35.204627  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.205529  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:43:35.205620  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:43:35.233701  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:43:35.233778  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:43:35.233834  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:43:35.233874  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:43:35.266335  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.267054  1450  1752 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:43:35.274872  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:35.276062  1450  1752 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:43:35.277819  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:35.280626   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:43:35.365055  1450 23534 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:43:35.373709  1450 23534 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:43:35.388043  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:35.391247  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:35.400010  1450  1634 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.400200  1450  1634 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.406491  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.453785  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.455716  1450 20008 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.455876  1450 20008 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.456916  1450  1515 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:35.457109  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:43:35.466645  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:43:35.466997  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:35.475199  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.494134  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:35.494623  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:35.537338  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:35.540591  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:35.552220  1450  1807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.569076  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:43:35.571855  1450  1634 D DCT     : [0]phoneSubId = 1
10-17 14:43:35.572353  1450  1634 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:35.573017  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:35.573112  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:43:35.574924   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:35.575268   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:35.576387  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:35.576538  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:43:35.581176   909  1946 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:35.581538   909  1946 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:35.584467  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:35.584632  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:43:35.584883  1450  1450 D RILJ    : [9473]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:43:35.586606  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:35.589926   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:43:35.590041   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cc36c0, pRI=0x7f9784c840, p=0x7f97856e70, pUCI=0x0
10-17 14:43:35.590090   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c840 p=0x7f97856e70 dispatched to RIL_CMD_PROXY_3
10-17 14:43:35.590358   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:35.590435   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:35.590506   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:35.590538   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:35.590594   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:35.590624   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:35.590672   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:35.590701   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:35.590744   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:35.590769   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:35.590811   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:35.590838   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:35.590879   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:35.590979   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:35.591033   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:35.591061   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:35.591106   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:35.591132   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:35.591723   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:35.591807   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:35.592084   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:35.592159   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:35.592201   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c840 p=0x7f97856e70 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:35.592235   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:35.592268   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:43:35.592296   721   749 D RIL     : radioState:10
10-17 14:43:35.592343   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:43:35.592379   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:43:35.592414   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.592443   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:43:35.592469   721   749 I AT      : AT write start
10-17 14:43:35.592653   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:35.592714   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:35.592765   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:35.592851   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:35.593712   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:35.593845   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:35.596534  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:43:35.598894  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:35.599035  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:43:35.599301  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.599300  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:35.599493  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.600491   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:35.600582   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:35.600660   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:35.600708   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:35.600699   909  7315 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:35.600843   909  7315 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:35.600869   721   766 I AT      : AT read end: 6
10-17 14:43:35.600987   721   766 D AT      : AT< OK
10-17 14:43:35.601021   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:35.601073   721   766 I AT      : AT read start
10-17 14:43:35.601235   909  7315 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:35.601477   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:35.601553   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:35.601608   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:35.602261  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:43:35.602266  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:35.602396  1450  1606 D RILJ    : [9473]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:43:35.602579  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:35.602697  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:43:35.602834  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:35.602916  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:35.603520   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c840 p=0x7f97856e70 
10-17 14:43:35.603641   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:43:35.603682   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:35.605300   909  2707 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:35.605445   909  2707 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:35.605712   909  2707 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:35.607908  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:35.608019  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:43:35.622455  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:35.623983  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:35.635262  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:35.658222  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:43:35.658426  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:35.962821   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e437e0 
10-17 14:43:35.962901   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e434e0
10-17 14:43:35.962929   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e434f0
10-17 14:43:35.978224   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e437e0 reset to NULL
10-17 14:43:35.978292   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e437e0
10-17 14:43:35.978322   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e437f0
10-17 14:43:37.425376  1450  1450 D RILJ    : [9474]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:43:37.432814   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:43:37.432945   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9460, pRI=0x7f9784c4b0, p=0x7f97856ee0, pUCI=0x0
10-17 14:43:37.432996   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c4b0 p=0x7f97856ee0 dispatched to RIL_ATCI_PROXY
10-17 14:43:37.433106   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:37.433157   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:37.433157   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:37.433201   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:37.433294   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:37.433336   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:37.433396   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:37.433422   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:37.433470   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:37.433508   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:37.433553   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:37.433578   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:37.433626   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:37.433655   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:37.433702   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:37.433727   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:37.433778   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:37.433812   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:37.434045   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:37.434094   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:37.434139   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:37.434173   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:37.434210   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c4b0 p=0x7f97856ee0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:37.434251   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:37.434285   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:43:37.434314   721   753 D RIL     : radioState:10
10-17 14:43:37.434359   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:43:37.434393   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:37.434420   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:43:37.434443   721   753 I AT      : AT write start
10-17 14:43:37.434877   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:37.434973   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:37.435034   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:37.435142   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:43:37.433860   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:37.435865   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:37.436818   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:37.436937   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:37.437079   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:37.437176   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:37.437811   721   770 I AT      : AT read end: 6
10-17 14:43:37.437941   721   770 D AT      : AT< OK
10-17 14:43:37.437981   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:37.438044   721   770 I AT      : AT read start
10-17 14:43:37.439005   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:37.439073   721   753 D RIL     : p_response->success = 1
10-17 14:43:37.439104   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:37.439129   721   753 D RIL     : strLength = 6
10-17 14:43:37.439156   721   753 D RIL     : line = <
10-17 14:43:37.439156   721   753 D RIL     : OK
10-17 14:43:37.439156   721   753 D RIL     : >
10-17 14:43:37.439188   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:37.439240   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:37.439320   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f97856ee0 
10-17 14:43:37.439363   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9460
10-17 14:43:37.439397   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:37.439646  1450  1606 D RILJ    : [9474]< OEM_HOOK_RAW [B@63f75a7 [SUB0]
10-17 14:43:37.447698   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185006/0
10-17 14:43:37.477852  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:37.485238  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:37.485664  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:37.491450  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:37.491741  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:37.502831  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:37.507371  1450 29539 D DCT     : [0]phoneSubId = 1
10-17 14:43:37.507666  1450 29539 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:38.298448  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:38.309488  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:38.326097  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:38.437387  1431 15705 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:38.514251  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:38.514731  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:38.531054  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:38.535717  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:43:38.535915  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:39.046741   909  6090 D TelephonyRegistry: listen: E pkg=com.alibaba.aliexpresshd events=0x40 notifyNow=true subId=2147483647 myUserId=0 callerUserId=0
10-17 14:43:39.046859   909  6090 D TelephonyRegistry: listen: add new record
10-17 14:43:39.049132  1450  1807 D SubscriptionController: [getPhoneId] asked for default subId=1
10-17 14:43:39.049867   909  6090 D TelephonyRegistry: listen:  Register r={callingPackage=com.alibaba.aliexpresshd binder=android.os.BinderProxy@4e28068 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@8c81 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=40 canReadPhoneState=false} r.subId=2147483647 phoneId=0
10-17 14:43:39.049990   909  6090 D TelephonyRegistry: listen: logSSC.length=5 next=0
10-17 14:43:39.050415   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143913Europe/Samara(1,290,14400,0,1476700753) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:39.050829   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143934Europe/Samara(1,290,14400,0,1476700774) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:39.051313   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:39.051707   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:39.052114   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:39.052202   909  6090 D TelephonyRegistry: listen: ----------------
10-17 14:43:39.052271   909  6090 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:39.052361   909  6090 D TelephonyRegistry: validateEventsAndUserLocked: valid=false r.callerUserId=0 foregroundUser=0 r.events=64 events=16
10-17 14:43:39.052727   909  6090 D TelephonyRegistry: validateEventsAndUserLocked: valid=false r.callerUserId=0 foregroundUser=0 r.events=64 events=1024
10-17 14:43:39.069552  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:39.070078 25234 25253 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:39.077537 25234 25253 D TelephonyManager: getNetworkOperatorName phoneId= 0
10-17 14:43:39.119818 25234 25257 D TelephonyManager: getNetworkOperatorName phoneId= 0
10-17 14:43:40.272278   721   760 I RILC    : NUMBER:1
10-17 14:43:40.272360   721   760 I RILC    : arg len:14
10-17 14:43:40.272398   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:43:40.272502   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:43:40.272596   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c8d0 p=0x7f97856fc0 dispatched to RIL_CMD_PROXY_1
10-17 14:43:40.272704   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:40.272718   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:40.272747   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:40.272785   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:40.272794   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:40.272820   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:40.272861   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:40.272888   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:40.272928   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:40.272959   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:43:40.272991   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c8d0 p=0x7f97856fc0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:43:40.273028   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:43:40.273058   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:43:40.273084   721   751 D RIL     : radioState:10
10-17 14:43:40.273128   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:43:40.273174   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:43:40.273185   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:40.273204   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:43:40.273240   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:43:40.273263   721   751 I AT      : AT write start
10-17 14:43:40.273261   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:40.273292   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:40.273347   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:40.273383   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:40.273408   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:40.273407   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:40.273437   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:40.273472   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:40.273496   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:40.273494   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:40.273523   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:40.273568   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:40.273594   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:40.273621   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:40.273706   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:40.273760   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:43:40.273851   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:43:40.281513   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:43:40.281582   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:40.281679   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:43:40.281733   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:40.281791   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:43:40.281833   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:40.281887   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:43:40.281942   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:40.282091   721   768 I AT      : AT read end: 46
10-17 14:43:40.282145   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:40.282178   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:40.282363   721   768 D AT      : AT< OK
10-17 14:43:40.282394   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:43:40.282446   721   768 I AT      : AT read start
10-17 14:43:40.282525   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:43:40.282574   721   751 D RIL     : requestQueryThermal success
10-17 14:43:40.282612   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:40.282648   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:43:40.282697   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:43:40.282775   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c8d0 p=0x7f97856fc0 
10-17 14:43:40.282827   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9300
10-17 14:43:40.282860   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:42.366184   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:43:42.366237   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:43:42.366304   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:43:42.366345   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.366460   721   765 I AT      : AT read end: 37
10-17 14:43:42.366503   721   765 D AT      : AT< +ECSQ: 39,99,-286,1,1,1,1,3,32767
10-17 14:43:42.366533   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 39,99,-286,1,1,1,1,3,32767
10-17 14:43:42.366578   721   765 D RIL     : Nw URC:+ECSQ: 39,99,-286,1,1,1,1,3,32767
10-17 14:43:42.366644   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:43:42.366682   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:43:42.366710   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:42.366806   721   765 I AT      : AT read start
10-17 14:43:42.367258  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:43:42.367520  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -285 1 1
10-17 14:43:42.367636  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -286 1 1
10-17 14:43:42.367679  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:42.448302   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185009/0
10-17 14:43:42.584420  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:43:42.596075  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:43:42.596269  1450  1450 D RILJ    : [9475]> SCREEN_STATE: false [SUB0]
10-17 14:43:42.600359  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:43:42.602149  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:43:42.602268  1450  1450 D RILJ    : [9476]> SCREEN_STATE: false [SUB1]
10-17 14:43:42.603003   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:43:42.603057   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cda740, pRI=0x7f9784c930, p=0x7f97857420, pUCI=0x0
10-17 14:43:42.603089   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97857420 dispatched to RIL_CMD_PROXY_3
10-17 14:43:42.603901   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:42.603940   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:42.603982   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:42.604010   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:42.604050   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:42.604074   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:42.604112   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:42.604141   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:42.604144   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:42.604176   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:42.604177   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97857420 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:42.604211   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:42.604216   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:42.604240   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:42.604241   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:42.604268   721   749 D RIL     : radioState:10
10-17 14:43:42.604283   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:42.604309   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:42.604321   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.604346   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:42.604350   721   749 D AT      : AT> AT+CREG=1
10-17 14:43:42.604372   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:42.604376   721   749 I AT      : AT write start
10-17 14:43:42.604410   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:42.604435   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:42.604467   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:42.604496   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:42.604533   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:42.604557   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:42.604670   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.604721   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.604772   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:42.604857   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:42.606046   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:42.606099   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:42.606627   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:42.606705   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:42.606774   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:42.606814   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.606852   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:43:42.606940   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cda760, pRI=0x7f9784cb70, p=0x7f97856540, pUCI=0x0
10-17 14:43:42.606972   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb70 p=0x7f97856540 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:42.607068   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:42.607098   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:42.607116   721   766 I AT      : AT read end: 6
10-17 14:43:42.607133   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:42.607142   721   766 D AT      : AT< OK
10-17 14:43:42.607157   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:42.607172   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:42.607192   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:42.607208   721   766 I AT      : AT read start
10-17 14:43:42.607227   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:42.607254   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:42.607265   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:42.607279   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:42.607310   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:42.607319   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:42.607335   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:42.607366   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:42.607371   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:42.607413   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:42.607418   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:42.607437   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:42.607475   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:42.607488   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.607502   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:42.607535   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:42.607536   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.607568   721   749 D AT      : AT> AT+CGREG=1
10-17 14:43:42.607571   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:42.607594   721   749 I AT      : AT write start
10-17 14:43:42.607701   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:42.607736   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb70 p=0x7f97856540 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:42.607767   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:42.607796   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:42.607819   721   755 D RIL     : radioState:0
10-17 14:43:42.607847   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:42.607873   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:42.607897   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:42.607937   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.607961   721   755 D AT      : AT> AT+CREG=1
10-17 14:43:42.607985   721   755 I AT      : AT write start
10-17 14:43:42.608116   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.608163   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.608208   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:42.608289   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:42.608355   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.608390   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.608430   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:42.608496   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:42.609244   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:42.609298   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:42.609359   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:42.609400   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.609492   721   772 I AT      : AT read end: 6
10-17 14:43:42.609523   721   772 D AT      : AT< OK
10-17 14:43:42.609550   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:42.609597   721   772 I AT      : AT read start
10-17 14:43:42.609659   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.609704   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.609734   721   755 D AT      : AT> AT+CGREG=1
10-17 14:43:42.609762   721   755 I AT      : AT write start
10-17 14:43:42.609956   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.610006   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.610050   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:42.610124   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:42.612394   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:42.612474   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:42.612541   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:42.612582   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.612629   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:42.612671   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:42.612719   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:42.612754   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.612860   721   766 I AT      : AT read end: 6
10-17 14:43:42.612860   721   772 I AT      : AT read end: 6
10-17 14:43:42.612904   721   766 D AT      : AT< OK
10-17 14:43:42.612904   721   772 D AT      : AT< OK
10-17 14:43:42.612935   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:42.612935   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:42.612974   721   766 I AT      : AT read start
10-17 14:43:42.612981   721   772 I AT      : AT read start
10-17 14:43:42.613044   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.613077   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.613102   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:43:42.613123   721   749 I AT      : AT write start
10-17 14:43:42.613242   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.613286   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.613329   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:42.613406   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:42.613471   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.613511   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.613535   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:43:42.613558   721   755 I AT      : AT write start
10-17 14:43:42.613666   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.613705   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.613748   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:42.613817   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:42.614942   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:42.615008   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:42.615154   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:42.615165   721   766 I AT      : AT read end: 6
10-17 14:43:42.615201   721   766 D AT      : AT< OK
10-17 14:43:42.615199   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.615233   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:42.615254   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:42.615279   721   766 I AT      : AT read start
10-17 14:43:42.615301   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:42.615356   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:42.615398   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.615476   721   772 I AT      : AT read end: 6
10-17 14:43:42.615506   721   772 D AT      : AT< OK
10-17 14:43:42.615533   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:42.615570   721   772 I AT      : AT read start
10-17 14:43:42.615629   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.615663   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.615689   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:43:42.615716   721   749 I AT      : AT write start
10-17 14:43:42.615835   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.615881   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.615926   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:42.616003   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:43:42.616067   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.616102   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.616126   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:43:42.616147   721   755 I AT      : AT write start
10-17 14:43:42.616253   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.616292   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.616336   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:42.616403   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:43:42.617568   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:42.617631   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:42.617694   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:42.617735   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.617831   721   766 I AT      : AT read end: 6
10-17 14:43:42.617870   721   766 D AT      : AT< OK
10-17 14:43:42.617897   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:42.617934   721   766 I AT      : AT read start
10-17 14:43:42.618058   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.618118   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.618144   721   749 D AT      : AT> AT+CEREG=1
10-17 14:43:42.618166   721   749 I AT      : AT write start
10-17 14:43:42.618286   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.618331   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.618376   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:42.618449   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:42.618518   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:42.618559   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:42.618617   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:42.618656   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.618735   721   772 I AT      : AT read end: 6
10-17 14:43:42.618767   721   772 D AT      : AT< OK
10-17 14:43:42.618795   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:42.618833   721   772 I AT      : AT read start
10-17 14:43:42.618894   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.618933   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.618957   721   755 D AT      : AT> AT+CEREG=1
10-17 14:43:42.618982   721   755 I AT      : AT write start
10-17 14:43:42.619089   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.619130   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.619172   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:42.619652   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:42.619707   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:42.619767   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:42.619806   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.619898   721   766 I AT      : AT read end: 6
10-17 14:43:42.619934   721   766 D AT      : AT< OK
10-17 14:43:42.619961   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:42.619997   721   766 I AT      : AT read start
10-17 14:43:42.620037   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:42.620080   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:42.620120   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:42.620186   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c930 p=0x7f97857420 
10-17 14:43:42.620215   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda740
10-17 14:43:42.620239   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:42.620452  1450  1606 D RILJ    : [9475]< SCREEN_STATE  [SUB0]
10-17 14:43:42.622049   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:42.622574   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:42.622631   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:42.622693   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:42.622733   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.622824   721   772 I AT      : AT read end: 6
10-17 14:43:42.622859   721   772 D AT      : AT< OK
10-17 14:43:42.622890   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:42.622942   721   772 I AT      : AT read start
10-17 14:43:42.623006   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:42.623041   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:42.623081   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:42.623149   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb70 p=0x7f97856540 
10-17 14:43:42.623180   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:43:42.623204   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:42.623412  1450  1609 D RILJ    : [9476]< SCREEN_STATE  [SUB1]
10-17 14:43:42.854102  1450  1450 D RILJ    : [9477]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:43:42.856048   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:43:42.856132   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda960, pRI=0x7f9784c3f0, p=0x7f978567e0, pUCI=0x0
10-17 14:43:42.856168   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f978567e0 dispatched to RIL_ATCI_PROXY
10-17 14:43:42.856303   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:42.856338   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:42.856343   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:42.856376   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:42.856408   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:42.856418   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:42.856434   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:42.856460   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:42.856476   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:42.856485   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:42.856529   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:42.856553   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:42.856593   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:42.856592   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:42.856621   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:42.856659   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:42.856707   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:42.856731   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:42.856831   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:42.856873   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f978567e0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:42.856902   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:42.856933   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:43:42.856957   721   753 D RIL     : radioState:10
10-17 14:43:42.856995   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:43:42.857026   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:42.857052   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:43:42.857075   721   753 I AT      : AT write start
10-17 14:43:42.857463   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:42.857530   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:42.857580   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:42.857660   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:43:42.857736   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:42.857769   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:42.857818   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:42.857842   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:42.857877   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:42.865102   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:42.865187   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:42.865256   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:42.865296   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:42.865407   721   770 I AT      : AT read end: 6
10-17 14:43:42.865453   721   770 D AT      : AT< OK
10-17 14:43:42.865483   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:42.865520   721   770 I AT      : AT read start
10-17 14:43:42.865643   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:42.865692   721   753 D RIL     : p_response->success = 1
10-17 14:43:42.865721   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:42.865746   721   753 D RIL     : strLength = 6
10-17 14:43:42.865769   721   753 D RIL     : line = <
10-17 14:43:42.865769   721   753 D RIL     : OK
10-17 14:43:42.865769   721   753 D RIL     : >
10-17 14:43:42.865796   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:42.865841   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:42.865906   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c3f0 p=0x7f978567e0 
10-17 14:43:42.865941   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda960
10-17 14:43:42.865967   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:42.866124  1450  1606 D RILJ    : [9477]< OEM_HOOK_RAW [B@5082a54 [SUB0]
10-17 14:43:43.054470  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:43:43.057771  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:43:43.057949  1450  1450 D RILJ    : [9478]> SCREEN_STATE: true [SUB0]
10-17 14:43:43.061307  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:43:43.062194   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:43:43.062283   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9340, pRI=0x7f9784c810, p=0x7f978570a0, pUCI=0x0
10-17 14:43:43.062320   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c810 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_3
10-17 14:43:43.062474   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.062508   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.062559   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.062586   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.062626   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.062654   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.062694   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.062718   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.062758   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.062784   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.062855   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.062891   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.062933   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.062959   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.063001   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.063025   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.063065   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.063090   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.063141   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:43.063175   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.063209   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c810 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.063245   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.063278   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:43.063304   721   749 D RIL     : radioState:10
10-17 14:43:43.063362   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.063392   721   749 D AT      : AT> AT+CREG=3
10-17 14:43:43.063416   721   749 I AT      : AT write start
10-17 14:43:43.063524   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.063554   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.063596   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.063625   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.063743   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.063799   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.063851   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.063948   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:43.064207  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:43:43.064337  1450  1450 D RILJ    : [9479]> SCREEN_STATE: true [SUB1]
10-17 14:43:43.067324   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:43:43.067412   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9160, pRI=0x7f9784cab0, p=0x7f97857490, pUCI=0x0
10-17 14:43:43.067451   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cab0 p=0x7f97857490 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:43.067594   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.067627   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.067670   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.067699   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.067737   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.067763   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.067804   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.067839   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.067959   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.067990   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.068176   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.068221   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.068263   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.068287   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.068326   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.068350   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.068389   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.068414   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.068452   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.068482   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:43.068515   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cab0 p=0x7f97857490 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:43.068549   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.068579   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:43:43.068605   721   755 D RIL     : radioState:0
10-17 14:43:43.068645   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.068671   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.068695   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.068745   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.068771   721   755 D AT      : AT> AT+CREG=3
10-17 14:43:43.068794   721   755 I AT      : AT write start
10-17 14:43:43.068974   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.069039   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.069091   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.069183   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:43.069271   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.069313   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.072632   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:43:43.072725   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:43:43.072801   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:43:43.072844   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.072895   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.072937   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.072989   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.073030   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.073072   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:43:43.073114   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:43:43.073164   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:43:43.073204   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.073329   721   765 I AT      : AT read end: 36
10-17 14:43:43.073372   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:43.073405   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:43.073448   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:43:43.073482   721   765 D RIL     : NW state changed: normal case
10-17 14:43:43.073511   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:43:43.073541   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:43.073570   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:43:43.073625   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:43:43.073658   721   765 D RIL     : bCREGType3Support=1
10-17 14:43:43.073688   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:43:43.073714   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:43:43.073795   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:43:43.073824   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.073891   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43540
10-17 14:43:43.073928   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43550
10-17 14:43:43.073993   721   765 I AT      : AT read start
10-17 14:43:43.074252  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:43:43.074457  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:43:43.074556  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:43:43.074712  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:43:43.075191   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.075276   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.075367   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.075413   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.075849   721   772 I AT      : AT read end: 6
10-17 14:43:43.075896   721   772 D AT      : AT< OK
10-17 14:43:43.075926   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.075977   721   772 I AT      : AT read start
10-17 14:43:43.076295   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.076387   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.076415   721   755 D AT      : AT> AT+CGREG=3
10-17 14:43:43.076439   721   755 I AT      : AT write start
10-17 14:43:43.076638   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.076704   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.076758   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.076847   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:43.077717   721   771 I AT      : AT read end: 36
10-17 14:43:43.077793   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:43.077825   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:43.077876   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:43:43.077910   721   771 D RIL     : NW state changed: normal case
10-17 14:43:43.077947   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:43:43.077978   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:43:43.078009   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:43:43.078064   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:43:43.078100   721   771 D RIL     : bCREGType3Support=1
10-17 14:43:43.078130   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:43:43.078156   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:43:43.078246   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:43:43.078278   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.078338   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e43540, cancel
10-17 14:43:43.078376   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e433c0
10-17 14:43:43.078410   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e433d0
10-17 14:43:43.078478   721   771 I AT      : AT read start
10-17 14:43:43.078728   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.078753  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:43:43.078795   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.078875   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.078921   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.079293   721   766 I AT      : AT read end: 6
10-17 14:43:43.079361   721   766 D AT      : AT< OK
10-17 14:43:43.079391   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.079442   721   766 I AT      : AT read start
10-17 14:43:43.079575   721   772 I AT      : AT read end: 6
10-17 14:43:43.079618   721   772 D AT      : AT< OK
10-17 14:43:43.079648   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.079696   721   772 I AT      : AT read start
10-17 14:43:43.079776   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.079834   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.079865   721   749 D AT      : AT> AT+CGREG=3
10-17 14:43:43.079890   721   749 I AT      : AT write start
10-17 14:43:43.080068   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.080122   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.080173   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.080277   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:43.080659   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.080753   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.080783   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:43:43.080807   721   755 I AT      : AT write start
10-17 14:43:43.081144   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.081212   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.081357   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.081444   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:43:43.081579  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:43:43.081684  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:43:43.081802  1450  1450 D RILJ    : [9480]> OPERATOR [SUB0]
10-17 14:43:43.082248   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.082352   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.082429   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.082474   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.084674  1450  1450 D RILJ    : [9481]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:43:43.085049   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:43:43.085129   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf91e0, pRI=0x7f9784cae0, p=0x7f978565b0, pUCI=0x0
10-17 14:43:43.085165   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cae0 p=0x7f978565b0 dispatched to RIL_CMD_PROXY_3
10-17 14:43:43.085303   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.085332   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.085372   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.085397   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.085435   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.085459   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.085498   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.085523   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.085561   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.085584   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.086836   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.086891   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.086936   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.086963   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.087003   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.087030   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.087070   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.087096   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.087134   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.087159   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.087252   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:43:43.087312   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9c00, pRI=0x7f9784cd80, p=0x7f97856bd0, pUCI=0x0
10-17 14:43:43.087345   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cae0 p=0x7f978565b0 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.087375   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:43.087408   721   760 D RILC-MTK: Request pRI=0x7f9784cd80 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:43:43.087784  1450  1450 D RILJ    : [9482]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:43:43.091564   721   766 I AT      : AT read end: 6
10-17 14:43:43.091643   721   766 D AT      : AT< OK
10-17 14:43:43.091675   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.091730   721   766 I AT      : AT read start
10-17 14:43:43.091904   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.091972   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.092014   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:43:43.092044   721   749 I AT      : AT write start
10-17 14:43:43.092130   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.092197   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.092265   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.092312   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.092647   721   772 I AT      : AT read end: 6
10-17 14:43:43.092707   721   772 D AT      : AT< OK
10-17 14:43:43.092740   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.092786   721   772 I AT      : AT read start
10-17 14:43:43.092874   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.092921   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.092966   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.093058   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:43.098014   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.098084   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.098111   721   755 D AT      : AT> AT+ECSQ
10-17 14:43:43.098135   721   755 I AT      : AT write start
10-17 14:43:43.098295   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.098345   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.098397   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.098479   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:43:43.100649   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:43:43.100713   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9c20, pRI=0x7f9784cde0, p=0x7f97856c40, pUCI=0x0
10-17 14:43:43.100747   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cae0 p=0x7f978565b0 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.100874   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cd80 p=0x7f97856bd0 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.101055   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:43.101097   721   760 D RILC-MTK: Request pRI=0x7f9784cde0 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:43:43.101175   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.101235   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.101305   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.101344   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.101394   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:43:43.101435   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.101490   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:43:43.101527   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.101631   721   766 I AT      : AT read end: 6
10-17 14:43:43.101663   721   766 D AT      : AT< OK
10-17 14:43:43.101692   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.101737   721   766 I AT      : AT read start
10-17 14:43:43.101648   721   772 I AT      : AT read end: 36
10-17 14:43:43.101774   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:43:43.101804   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:43:43.101833   721   772 I AT      : AT read start
10-17 14:43:43.101842   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.101888   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.101892   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.101933   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.101951   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.101956   721   749 D AT      : AT> AT+ECSQ
10-17 14:43:43.101981   721   749 I AT      : AT write start
10-17 14:43:43.101991   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.102078   721   772 I AT      : AT read end: 6
10-17 14:43:43.102103   721   772 D AT      : AT< OK
10-17 14:43:43.102128   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.102167   721   772 I AT      : AT read start
10-17 14:43:43.102230   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.102269   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.102310   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.102384   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:43:43.102454   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.102501   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:43:43.102538   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:43:43.102566   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.102602   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:43:43.102626   721   755 I AT      : AT write start
10-17 14:43:43.103103   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.103255   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.103312   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.103391   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:43:43.104008   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:43:43.104090   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.104161   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:43:43.104203   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.104276   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.104316   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.104363   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.104400   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.105134   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.105217   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.105285   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.105325   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.105469   721   772 I AT      : AT read end: 6
10-17 14:43:43.105509   721   772 D AT      : AT< OK
10-17 14:43:43.105537   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.105589   721   772 I AT      : AT read start
10-17 14:43:43.105868   721   766 I AT      : AT read end: 43
10-17 14:43:43.105916   721   766 D AT      : AT< +ECSQ: 39,99,-286,1,1,1,1,3,32767
10-17 14:43:43.105944   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 39,99,-286,1,1,1,1,3,32767
10-17 14:43:43.105977   721   766 D AT      : AT< OK
10-17 14:43:43.106001   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.106034   721   766 I AT      : AT read start
10-17 14:43:43.106087   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.106161   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:43:43.106197   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:43:43.109208   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.109342   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.109373   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:43:43.109398   721   749 I AT      : AT write start
10-17 14:43:43.109782   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.109880   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.109937   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.110037   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:43:43.110093   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.110169   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.110198   721   755 D AT      : AT> AT+CEREG=3
10-17 14:43:43.110222   721   755 I AT      : AT write start
10-17 14:43:43.110391   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.110454   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.110506   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.110592   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:43:43.111304  1450  1450 D RILJ    : [9483]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:43:43.114321   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:43:43.114407   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9c40, pRI=0x7f9784ce10, p=0x7f97856cb0, pUCI=0x0
10-17 14:43:43.114445   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cae0 p=0x7f978565b0 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.114478   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cd80 p=0x7f97856bd0 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.114507   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cde0 p=0x7f97856c40 is queued in RIL_CMD_PROXY_3
10-17 14:43:43.114537   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:43:43.114569   721   760 D RILC-MTK: Request pRI=0x7f9784ce10 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:43:43.114721  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.114828  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:43:43.114905  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:43:43.114988  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:43:43.115031  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:43:43.117593  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.117707  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.117769  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:43:43.117913  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:43:43.117904   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.117967   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.118039  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:43:43.118044   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.118091   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.118109  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:43:43.118148   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.118193   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.118195  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:43:43.118237  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:43:43.118252   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.118275  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:43:43.118290   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.118313  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:43:43.118346  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:43:43.118449   721   766 I AT      : AT read end: 6
10-17 14:43:43.118449   721   772 I AT      : AT read end: 6
10-17 14:43:43.118494   721   766 D AT      : AT< OK
10-17 14:43:43.118495   721   772 D AT      : AT< OK
10-17 14:43:43.118528   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.118529   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.118581   721   766 I AT      : AT read start
10-17 14:43:43.118591   721   772 I AT      : AT read start
10-17 14:43:43.118672   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.118712   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:43.118752   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.118834   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cab0 p=0x7f97857490 
10-17 14:43:43.118876   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9160
10-17 14:43:43.118905   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.118974   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.119021   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.119049   721   749 D AT      : AT> AT+CEREG=3
10-17 14:43:43.119072   721   749 I AT      : AT write start
10-17 14:43:43.119356  1450  1609 D RILJ    : [9479]< SCREEN_STATE  [SUB1]
10-17 14:43:43.119749   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.119832   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.119892   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.119983   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:43.121264  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:43:43.121442  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:43:43.121514  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:43:43.121564  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:43:43.121825  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:43:43.122689  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.122812  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.122865  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:43:43.124813  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:43:43.125024  1450  1450 D RILJ    : [9484]> OPERATOR [SUB1]
10-17 14:43:43.127763   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.127858   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.127948   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.127995   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.128032   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:43:43.128117   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9c60, pRI=0x7f9784ce40, p=0x7f97856930, pUCI=0x0
10-17 14:43:43.128133   721   766 I AT      : AT read end: 6
10-17 14:43:43.128153   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784ce40 p=0x7f97856930 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:43.128166   721   766 D AT      : AT< OK
10-17 14:43:43.128199   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.128242   721   766 I AT      : AT read start
10-17 14:43:43.128266   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.128297   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.128339   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.128341   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.128371   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.128421   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.128421   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.128449   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.128487   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.128523   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.128546   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.128552   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.128595   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.128621   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.128648   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.128659   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.128692   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.128703   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.128744   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.128827   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c810 p=0x7f978570a0 
10-17 14:43:43.128860   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:43:43.128909   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.128947   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784cae0 p=0x7f978565b0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.128977   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.129008   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:43:43.129034   721   749 D RIL     : radioState:10
10-17 14:43:43.129076   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.129085  1450  1606 D RILJ    : [9478]< SCREEN_STATE  [SUB0]
10-17 14:43:43.129107   721   749 D AT      : AT> AT+COPS?
10-17 14:43:43.129134   721   749 I AT      : AT write start
10-17 14:43:43.129289   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.129331   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:43.129364   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784ce40 p=0x7f97856930 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:43.129395   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.129424   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:43:43.129448   721   755 D RIL     : radioState:0
10-17 14:43:43.129489   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.129519   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.129545   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.129571   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.129613   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:43.129645   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:43.129696   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.129804   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce40 p=0x7f97856930 
10-17 14:43:43.129840   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c60
10-17 14:43:43.129866   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.130007   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.130054   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.130105   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.130132   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.130600  1450  1609 D RilRequest: [9484]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:43.131078   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.131181   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.131239   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.131335   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:43:43.133317  1450  1450 D RILJ    : [9485]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:43:43.135554  1450  1450 D RILJ    : [9486]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:43:43.136932   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:43:43.137033   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cda8a0, pRI=0x7f9784c510, p=0x7f978569a0, pUCI=0x0
10-17 14:43:43.137069   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f978569a0 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:43.137246   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.137296   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.137342   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.137369   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.137411   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.137438   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.137479   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.137505   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.137587   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.137616   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.137956   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.138008   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.138055   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.138080   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.138118   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.138143   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.138181   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.138212   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:43.138245   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f978569a0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:43.138273   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.138304   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:43:43.138328   721   755 D RIL     : radioState:0
10-17 14:43:43.138365   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.138390   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.138415   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.138441   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.138474   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:43.138515   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:43.138565   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.138629   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f978569a0 
10-17 14:43:43.138662   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda8a0
10-17 14:43:43.138688   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.138745   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.138789   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.138975   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.139001   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.139119  1450  1609 D RilRequest: [9485]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:43.139620   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:43:43.139713   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.139805   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:43:43.139859   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.139992   721   766 I AT      : AT read end: 24
10-17 14:43:43.140047   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:43:43.140078   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:43:43.140115   721   766 I AT      : AT read start
10-17 14:43:43.140390   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.140457   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.140543   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.140602   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.140832   721   766 I AT      : AT read end: 6
10-17 14:43:43.140879   721   766 D AT      : AT< OK
10-17 14:43:43.140996   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.141045   721   766 I AT      : AT read start
10-17 14:43:43.141307   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.141373   721   749 D RIL     : Get operator code 25020
10-17 14:43:43.141408   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:43:43.141448   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:43:43.141481   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.141540   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.141618   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cae0 p=0x7f978565b0 
10-17 14:43:43.141659   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf91e0
10-17 14:43:43.141689   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.141722   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cd80 p=0x7f97856bd0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.141751   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.141783   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:43:43.141808   721   749 D RIL     : radioState:10
10-17 14:43:43.141852   721   749 D RIL     : request gprs reg state: normal case
10-17 14:43:43.141888   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.141914   721   749 D AT      : AT> AT+CGREG?
10-17 14:43:43.141938   721   749 I AT      : AT write start
10-17 14:43:43.142253  1450  1606 D RILJ    : [9480]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:43:43.142625   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:43:43.142719   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cdaa00, pRI=0x7f9784c870, p=0x7f978573b0, pUCI=0x0
10-17 14:43:43.142756   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c870 p=0x7f978573b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:43.142943   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.142990   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.143039   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.143065   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.143107   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.143132   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.143173   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.143199   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.143187   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.143244   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.143250   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.143272   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.143306   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.143313   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.143347   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:43.143380   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c870 p=0x7f978573b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:43.143396   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:43:43.143409   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.143439   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:43:43.143454   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.143465   721   755 D RIL     : radioState:0
10-17 14:43:43.143484   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.143508   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.143525   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.143534   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.143550   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.143560   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.143587   721   755 I RIL     : isWfcSupport: 0
10-17 14:43:43.143590   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.143620   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.143626   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:43:43.143655   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:43.143661   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.143685   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.143701   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.143722   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.143749   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.143764   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c870 p=0x7f978573b0 
10-17 14:43:43.143797   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaa00
10-17 14:43:43.143821   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.143997  1450  1450 D RILJ    : [9487]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:43:43.144026  1450  1609 D RilRequest: [9486]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:43:43.148169  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:43.148291  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:43:43.148455  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -285 1 1
10-17 14:43:43.148565  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -286 1 1
10-17 14:43:43.148606  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.148672  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:43:43.148718  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:43:43.148760  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:43.148812  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:43:43.148848  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:43.148879  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:43.148921  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:43:43.149048  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:43:43.149092  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:43:43.150050   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:43:43.150145   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cdaac0, pRI=0x7f9784c9c0, p=0x7f97857ab0, pUCI=0x0
10-17 14:43:43.150178   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c9c0 p=0x7f97857ab0 dispatched to RIL_CMD2_PROXY_3
10-17 14:43:43.151197   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.151311   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.151363   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.151389   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.151430   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.151456   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.151526   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.151552   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.151601   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.151606   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.151630   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.151668   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.151697   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.151738   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.151764   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.151806   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.151807   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:43:43.151834   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.151870   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.151875   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.151906   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.151946   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.151950   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:43:43.151980   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:43:43.151995   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.152012   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c9c0 p=0x7f97857ab0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:43:43.152042   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.152043   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.152076   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:43:43.152086   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.152104   721   755 D RIL     : radioState:0
10-17 14:43:43.152130   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.152143   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.152170   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.152171   721   755 D AT      : AT> AT+COPS?
10-17 14:43:43.152200   721   755 I AT      : AT write start
10-17 14:43:43.152277   721   766 I AT      : AT read end: 50
10-17 14:43:43.152315   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:43:43.152347   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:43:43.152363   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.152382   721   766 D AT      : AT< OK
10-17 14:43:43.152409   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.152408   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.152455   721   766 I AT      : AT read start
10-17 14:43:43.152474   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:43:43.152577   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:43:43.152671   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.152724   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:43.152754   721   749 E RIL     : The value in the field <lac> :0
10-17 14:43:43.152786   721   749 D RIL     : cid: 3583
10-17 14:43:43.152812   721   749 E RIL     : The value of act: 3
10-17 14:43:43.152837   721   749 D RIL     : cause_type: 0
10-17 14:43:43.152860   721   749 D RIL     : reject_cause: 0
10-17 14:43:43.152898   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.152925   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:43:43.152949   721   749 I AT      : AT write start
10-17 14:43:43.153495   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.153520   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.153574   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.153627   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.153716   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:43:43.154564   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:43:43.154653   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.154734   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:43:43.154780   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.154769  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.154839   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:43:43.154853  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:43:43.154880   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:43:43.154926   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:43:43.154927  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:43:43.154968   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.154975  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:43:43.155245   721   772 I AT      : AT read end: 18
10-17 14:43:43.155302   721   772 D AT      : AT< +COPS: 0
10-17 14:43:43.155336   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:43:43.155369   721   772 D AT      : AT< OK
10-17 14:43:43.155543   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:43:43.155568   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:43:43.155588   721   772 I AT      : AT read start
10-17 14:43:43.155625   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.155658   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:43:43.155698   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:43:43.155695   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:43:43.155743   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.155749   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:43:43.155804   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.155822   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c9c0 p=0x7f97857ab0 
10-17 14:43:43.155845   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.155863   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:43:43.155893   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.155891   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.155936   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.156041   721   766 I AT      : AT read end: 25
10-17 14:43:43.156079   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:43:43.156110   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:43:43.156152   721   766 D AT      : AT< OK
10-17 14:43:43.156178   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.156213  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:43:43.156229   721   766 I AT      : AT read start
10-17 14:43:43.156288  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:43:43.156386  1450  1609 D RILJ    : [9487]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:43:43.156677   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.156767   721   749 E RIL     : rid: 0
10-17 14:43:43.156795   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:43:43.156825   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:43:43.156853   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:43:43.156881   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:43:43.156913   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.156972   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.157054   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cd80 p=0x7f97856bd0 
10-17 14:43:43.157085   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c00
10-17 14:43:43.157114   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.157145   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cde0 p=0x7f97856c40 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.157176   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.157204   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:43:43.157230   721   749 D RIL     : radioState:10
10-17 14:43:43.157266   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.157270  1450  1606 D RILJ    : [9481]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:43:43.157293   721   749 D AT      : AT> AT+CREG?
10-17 14:43:43.157316   721   749 I AT      : AT write start
10-17 14:43:43.157543   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.157607   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.157660   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.157745   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:43:43.160213  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.160320  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:43:43.160399  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:43:43.160444  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:43:43.160486  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:43:43.160543  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:43:43.160581  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:43:43.160621  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:43:43.160736  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:43:43.165823   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:43:43.165898   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.165969   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:43:43.166011   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.166059   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.166109   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.166154   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.166191   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.166522   721   766 I AT      : AT read end: 44
10-17 14:43:43.166578   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:43:43.166611   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:43:43.166649   721   766 D AT      : AT< OK
10-17 14:43:43.166674   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.166723   721   766 I AT      : AT read start
10-17 14:43:43.167770   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.167834   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:43:43.167864   721   749 E RIL     : The value in the field <lac> :127
10-17 14:43:43.167890   721   749 D RIL     : cid: 3583
10-17 14:43:43.167916   721   749 E RIL     : The value of act: 3
10-17 14:43:43.167940   721   749 D RIL     : cause_type: 0
10-17 14:43:43.167966   721   749 D RIL     : reject_cause: 0
10-17 14:43:43.168023   721   749 E RIL     : rid: 0
10-17 14:43:43.168050   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:43:43.168080   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:43:43.168106   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:43:43.168131   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:43:43.168160   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:43:43.168194   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.168256   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.168343   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cde0 p=0x7f97856c40 
10-17 14:43:43.168373   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c20
10-17 14:43:43.168407   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.168439   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784ce10 p=0x7f97856cb0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.168468   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.168496   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:43:43.168522   721   749 D RIL     : radioState:10
10-17 14:43:43.168558   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.168589   721   749 D AT      : AT> AT+COPS?
10-17 14:43:43.168583  1450  1606 D RILJ    : [9482]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:43:43.168621   721   749 I AT      : AT write start
10-17 14:43:43.169223   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.169299   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.169354   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.169441   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:43:43.172071  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.172211  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:43:43.172258  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:43.172289  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:43.172361  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:43:43.172409  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:43:43.172443  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:43:43.172494  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:43:43.172543  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:43:43.172581  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:43:43.172648  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:43:43.172684  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:43:43.172730  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:43:43.172761  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.172811  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:43:43.172866  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:43:43.172927  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:43:43.172983  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:43:43.173013  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:43:43.173160  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:43:43.173195  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:43:43.173229  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.177367   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:43:43.177455   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.177529   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:43:43.177573   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.177711   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.177705   721   766 I AT      : AT read end: 24
10-17 14:43:43.177758   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:43:43.177767   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.177794   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:43:43.177830   721   766 I AT      : AT read start
10-17 14:43:43.177829   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.177875   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.177961   721   766 I AT      : AT read end: 6
10-17 14:43:43.177993   721   766 D AT      : AT< OK
10-17 14:43:43.178022   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.178073   721   766 I AT      : AT read start
10-17 14:43:43.178144   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.178200   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.178245   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.178315   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce10 p=0x7f97856cb0 
10-17 14:43:43.178348   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c40
10-17 14:43:43.178373   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:43.178804  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:43:43.178891  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:43:43.178969  1450  1606 D RILJ    : [9483]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:43:43.179154  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:43:43.179251  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:43:43.183650  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:43:43.183705  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:43:43.183745  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:43:43.183881  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:43:43.184000  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:43:43.184245  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:43:43.184300  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:43:43.184355  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:43:43.184415  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:43:43.184583  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:43:43.184640  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:43:43.184710  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:43:43.184795  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.184844  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.184886  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.184931  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.184982  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185054  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185102  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185143  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185187  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185229  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:43:43.185269  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:43:43.185393  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:43:43.185435  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:43:43.185671  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:43:43.186812  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:43:43.187610  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.187717  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:43:43.188419  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:43:43.189321  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:43:43.189
10-17 14:43:43.189453  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:43:43.190153  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.190355  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.190439  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:43:43.190494  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:43:43.190545  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.190798  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:43:43.191494   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.191582   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.191771   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=1
10-17 14:43:43.192163   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143934Europe/Samara(1,290,14400,0,1476700774) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.192562   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.192938   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.193304   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.193650   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.193745   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:43:43.193795   909   923 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:43.193946   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.194283   909   923 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:43.194483   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.194689   909   923 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:43.194850   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.195450   909   923 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:43.195669   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.195787   909   923 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:43.195944   909   923 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:43.198062  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:43.198151   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.198206  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:43.198253  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:43.198288  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:43.198329  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=20
10-17 14:43:43.198355  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:43.202777  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.205277   909   923 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.233737  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:43:43.233867  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:43.234068  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:43:43.237787  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.245038  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.247308   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:43:43.247554  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.247969  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.257721  1450  4234 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:43:43.259637  1450  4234 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:43:43.264573  1450  1515 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:43:43.265568  1450  1515 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:43:43.279826  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.281168  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.285219  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.289155  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:43.290718  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:43.464244  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.465551  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.465839  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.473803  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.482087  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.482513  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.512101  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.513618  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.514244  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.523640  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.525568  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.526123  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.547716  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.549008  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.549728  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.558942  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.559820  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.564264  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.569665  1450  1511 D DCT     : [0]phoneSubId = 1
10-17 14:43:43.569919  1450  1511 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:43.577873  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.579231  1450  4234 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.579765  1450  4234 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.583614  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:43:43.587844  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:43.587959  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:43:43.589689   909  1553 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.590060   909  1553 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.592090  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:43.592373  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:43:43.594807   909  1946 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.595470   909  1946 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.598768  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:43.599014  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:43:43.599323  1450  1450 D RILJ    : [9488]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:43:43.604097   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:43:43.604189   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cc36c0, pRI=0x7f9784ca50, p=0x7f97856540, pUCI=0x0
10-17 14:43:43.604223   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784ca50 p=0x7f97856540 dispatched to RIL_CMD_PROXY_3
10-17 14:43:43.604371   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.604402   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.604442   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.604467   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.604504   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.604528   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.604569   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.604592   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.604630   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.604654   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.604697   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.604722   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.604761   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:43.604790   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.604820   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784ca50 p=0x7f97856540 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.604850   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.604883   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:43:43.604910   721   749 D RIL     : radioState:10
10-17 14:43:43.604954   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:43:43.604990   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:43:43.605021   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.605048   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:43:43.605073   721   749 I AT      : AT write start
10-17 14:43:43.605741   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.605736  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.605828   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.605893   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.605923   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.605973   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.606001   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.606053   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.606086   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.606135   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.606167   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.606314   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.606384   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.606447   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.606600   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:43.608326   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.608412   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.608502   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.608552   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.609346   721   766 I AT      : AT read end: 6
10-17 14:43:43.609421   721   766 D AT      : AT< OK
10-17 14:43:43.609456   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.609514   721   766 I AT      : AT read start
10-17 14:43:43.611421   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.611500   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.611561   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.611662   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784ca50 p=0x7f97856540 
10-17 14:43:43.611720   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:43:43.611752   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:43.612278  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:43:43.613056  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:43:43.613250  1450  1606 D RILJ    : [9488]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:43:43.614442  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.619977  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:43.620129  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:43:43.620307  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.620391  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.621334   909  1631 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:43.621509   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.621896   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.622898  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:43.623045  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:43:43.623223  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.623313  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.624069   909  1946 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:43.624223  1450  1752 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.624249   909  1946 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.624297  1450  1752 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.624530   909  1946 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.631161  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:43:43.631388  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:43:43.651894  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:43:43.652010  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:43:43.652205  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:43:43.652281  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:43:43.652337  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:43:43.652376  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:43:43.653337  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.664952  1450  1515 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.665047  1450  1515 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.669904  1450  2351 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:43.670059  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:43:43.699121  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.703007  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:43:43.703200  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:43.707253  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.708528  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.709209  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.716509  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.717315  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.723829  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.735620  1450  1752 D DCT     : [0]phoneSubId = 1
10-17 14:43:43.735788  1450  1752 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:43.777067  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:43.823809  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:43.824320  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:43.862635  1450  1450 D RILJ    : [9489]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:43:43.865138   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:43:43.865227   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda760, pRI=0x7f9784c240, p=0x7f97857110, pUCI=0x0
10-17 14:43:43.865265   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f97857110 dispatched to RIL_ATCI_PROXY
10-17 14:43:43.865351   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.865387   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.865427   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.865452   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.865489   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.865514   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.865553   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.865576   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.865613   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.865637   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.865672   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.865696   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.865736   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.865744   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:43.865775   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:43.865778   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:43.865812   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f97857110 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:43.865843   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.865874   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:43:43.865897   721   753 D RIL     : radioState:10
10-17 14:43:43.865940   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:43:43.865970   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:43.865995   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:43:43.866017   721   753 I AT      : AT write start
10-17 14:43:43.866115   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.866158   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.866198   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.866222   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.866259   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.866282   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.866355   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.866385   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.866407   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.866467   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.866518   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:43.866629   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:43:43.872203  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:43.873256  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:43.875230   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:43.875320   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:43.875414   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:43.875466   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.875678   721   770 I AT      : AT read end: 6
10-17 14:43:43.875741   721   770 D AT      : AT< OK
10-17 14:43:43.875773   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:43.875822   721   770 I AT      : AT read start
10-17 14:43:43.876098   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:43.876191   721   753 D RIL     : p_response->success = 1
10-17 14:43:43.876224   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:43.876249   721   753 D RIL     : strLength = 6
10-17 14:43:43.876278   721   753 D RIL     : line = <
10-17 14:43:43.876278   721   753 D RIL     : OK
10-17 14:43:43.876278   721   753 D RIL     : >
10-17 14:43:43.876309   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.876363   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.876466   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97857110 
10-17 14:43:43.876502   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:43:43.876541   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.876884  1450  1606 D RILJ    : [9489]< OEM_HOOK_RAW [B@257cdfd [SUB0]
10-17 14:43:43.883981  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:43.907853  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:43:43.914355  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:43.914478  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:43:43.916757   909  1553 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.917150   909  1553 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.919253  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:43.919407  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:43:43.920092  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:43:43.920285  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:43.926020   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.926389   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.928149  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:43.928324  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:43:43.928583  1450  1450 D RILJ    : [9490]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:43:43.933485   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:43:43.933574   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cda900, pRI=0x7f9784c300, p=0x7f978571f0, pUCI=0x0
10-17 14:43:43.933623   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c300 p=0x7f978571f0 dispatched to RIL_CMD_PROXY_3
10-17 14:43:43.933742   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:43.933741   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:43.933794   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:43.933850   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:43.933877   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:43.933925   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:43.933950   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:43.934124   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:43.934164   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:43.934215   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:43.934254   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:43.934293   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:43.934305   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:43.934332   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:43.934375   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:43.934384   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:43.934404   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:43.934456   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:43.934485   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:43.934517   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:43.934944   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:43.935035   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:43:43.935075   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c300 p=0x7f978571f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:43:43.935109   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:43:43.935143   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:43:43.935171   721   749 D RIL     : radioState:10
10-17 14:43:43.935216   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:43:43.935251   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:43:43.935282   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.935310   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:43:43.935335   721   749 I AT      : AT write start
10-17 14:43:43.935557   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:43.935651   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:43.935780   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:43.935841   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:43.935894   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:43:43.935982   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:43:43.936350  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:43:43.937713  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:43.937990  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:43:43.938222  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.938341  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.938921   909   923 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:43.939024   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.939279   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.940125  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:43:43.940259  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:43:43.940387  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:43:43.940457  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:43:43.941237   909  6089 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:43:43.941894   909  6089 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:43.942957   909  6089 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:43.943507   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:43:43.943600   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:43:43.943692   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:43:43.943746   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:43.944912  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:43:43.945063  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:43:43.945452   721   766 I AT      : AT read end: 6
10-17 14:43:43.945533   721   766 D AT      : AT< OK
10-17 14:43:43.945569   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:43:43.945623   721   766 I AT      : AT read start
10-17 14:43:43.945905   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:43:43.945985   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:43.946041   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:43.946127   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f978571f0 
10-17 14:43:43.946167   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda900
10-17 14:43:43.946218   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:43.948534  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:43:43.948672  1450  1606 D RILJ    : [9490]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:43:44.074178   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e433c0 
10-17 14:43:44.074248   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43540
10-17 14:43:44.074279   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43550
10-17 14:43:44.078607   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e433c0 reset to NULL
10-17 14:43:44.078676   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e433c0
10-17 14:43:44.078705   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e433d0
10-17 14:43:44.798852  1450  1450 D RILJ    : [9491]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:43:44.801265   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:43:44.801336   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9100, pRI=0x7f9784c360, p=0x7f97857340, pUCI=0x0
10-17 14:43:44.801369   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97857340 dispatched to RIL_ATCI_PROXY
10-17 14:43:44.801465   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:44.801469   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:44.801498   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:44.801536   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:44.801543   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:44.801545   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:44.801575   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:44.801609   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:44.801621   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:44.801635   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:44.801665   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:44.801805   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:44.802476   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:44.802503   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:44.802520   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:44.802532   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:44.802565   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:44.802591   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97857340 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:44.802623   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:44.802619   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:44.802656   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:44.802658   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:43:44.802686   721   753 D RIL     : radioState:10
10-17 14:43:44.802692   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:44.802726   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:43:44.802742   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:44.802760   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:44.802767   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:44.802787   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:43:44.802802   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:44.802811   721   753 I AT      : AT write start
10-17 14:43:44.802825   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:44.805365   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:44.805430   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:44.805480   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:44.805564   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:43:44.813039   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:44.813116   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:44.813186   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:44.813234   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:44.813355   721   770 I AT      : AT read end: 6
10-17 14:43:44.813397   721   770 D AT      : AT< OK
10-17 14:43:44.813428   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:44.813466   721   770 I AT      : AT read start
10-17 14:43:44.813506   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:44.813543   721   753 D RIL     : p_response->success = 1
10-17 14:43:44.813570   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:44.813593   721   753 D RIL     : strLength = 6
10-17 14:43:44.813616   721   753 D RIL     : line = <
10-17 14:43:44.813616   721   753 D RIL     : OK
10-17 14:43:44.813616   721   753 D RIL     : >
10-17 14:43:44.813644   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:44.813698   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:44.813778   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97857340 
10-17 14:43:44.813809   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9100
10-17 14:43:44.813835   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:44.814098  1450  1606 D RILJ    : [9491]< OEM_HOOK_RAW [B@ed3faf2 [SUB0]
10-17 14:43:44.831313  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:44.832360  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:44.834701  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:44.848029  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:44.848393  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:44.859036  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:44.863149  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:43:44.863353  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:45.125137  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:43:45.130140  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:43:45.419179  1450  1450 D RILJ    : [9492]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:43:45.429314   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:43:45.429395   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9140, pRI=0x7f9784c810, p=0x7f97856e70, pUCI=0x0
10-17 14:43:45.429433   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f97856e70 dispatched to RIL_ATCI_PROXY
10-17 14:43:45.429550   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:45.429594   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:45.429604   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:45.429622   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:45.429638   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f97856e70 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:45.429661   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:45.429671   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:45.429685   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:45.429706   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:43:45.429722   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:45.429733   721   753 D RIL     : radioState:10
10-17 14:43:45.429747   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:45.429771   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:43:45.429782   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:45.429800   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:45.429806   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:45.429827   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:43:45.429849   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:45.429853   721   753 I AT      : AT write start
10-17 14:43:45.429877   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:45.429914   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:45.429940   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:45.430010   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:45.430038   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:45.430039   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:45.430076   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:45.430088   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:45.430099   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:45.430136   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:45.430220   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:43:45.431421   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:45.431485   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:45.431531   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:45.431558   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:45.431596   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:45.431620   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:45.437799   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:45.437887   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:45.437959   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:45.438003   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:45.438131   721   770 I AT      : AT read end: 6
10-17 14:43:45.438184   721   770 D AT      : AT< OK
10-17 14:43:45.438220   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:45.438272   721   770 I AT      : AT read start
10-17 14:43:45.438437   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:45.438482   721   753 D RIL     : p_response->success = 1
10-17 14:43:45.438510   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:45.438534   721   753 D RIL     : strLength = 6
10-17 14:43:45.438557   721   753 D RIL     : line = <
10-17 14:43:45.438557   721   753 D RIL     : OK
10-17 14:43:45.438557   721   753 D RIL     : >
10-17 14:43:45.438586   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:45.438637   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:45.438712   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c810 p=0x7f97856e70 
10-17 14:43:45.438744   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9140
10-17 14:43:45.438774   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:45.439065  1450  1606 D RILJ    : [9492]< OEM_HOOK_RAW [B@fe3c543 [SUB0]
10-17 14:43:45.828328  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:45.830275  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:45.843291  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:46.009827  1431 15705 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:46.013341  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:46.032805  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:46.067885  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:46.090825  1450  1752 D DCT     : [0]phoneSubId = 1
10-17 14:43:46.091104  1450  1752 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.448540   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185053/0
10-17 14:43:47.518494  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.520346  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.520887  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.559503  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.565101  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.576409  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.579220  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.579733  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.612833  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.614615  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.615078  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.661031  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.662976  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.663442  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.674774  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.676003  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.676501  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.696143  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.697259  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.697663  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.715383  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.717261  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.717800  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.732149  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.732608  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.737995  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.743463  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.743828  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.752043  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.753285  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.753726  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.767296  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.767985  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.775015  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.784249  1450  2351 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.784446  1450  2351 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.790007  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.791125  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.791541  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.801834  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.802112  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.805428  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.812650  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.812901  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.818043  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.820207  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.820607  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.825790  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.826045  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.835824  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.838443  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.838619  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:47.842340  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:47.843069  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:47.843420  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:47.847498  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:47.847725  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:47.852885  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:47.857892  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:47.858592  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:48.839279  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:48.840036  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:48.840348  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:48.846511  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:48.846902  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:48.850179  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:48.854310  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:48.854470  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:49.803143  1450  1450 D RILJ    : onDisplayChanged: displayId = 2 [SUB0]
10-17 14:43:49.803286  1450  1450 D RILJ    : onDisplayChanged: displayId = 2 [SUB1]
10-17 14:43:50.139191  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:50.140728  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:50.141695  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:50.154040  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:50.155264  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:50.158254  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:50.161269  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:43:50.161510  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:50.295990   721   760 I RILC    : NUMBER:1
10-17 14:43:50.296111   721   760 I RILC    : arg len:14
10-17 14:43:50.296155   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:43:50.296290   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:43:50.296352   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c150 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_1
10-17 14:43:50.296792   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:50.296817   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:50.296854   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:50.296898   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:50.296906   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:50.296926   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:50.296963   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:50.296979   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:50.297001   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:50.297053   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:50.297117   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:50.297162   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:50.297188   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:50.297647   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:50.297710   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:50.297761   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:50.297906   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:50.297982   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:50.298996   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:50.299049   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:50.299101   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:50.299131   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:43:50.299164   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c150 p=0x7f978570a0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:43:50.299202   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:43:50.299236   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:43:50.299262   721   751 D RIL     : radioState:10
10-17 14:43:50.299302   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:43:50.299375   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:43:50.299408   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:43:50.299435   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:43:50.299457   721   751 I AT      : AT write start
10-17 14:43:50.299561   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:50.299604   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:50.300601   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:50.300717   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:50.300784   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:43:50.301095   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:43:50.312035   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:43:50.312119   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:50.312196   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:43:50.312239   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:50.312290   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:43:50.312331   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:43:50.312381   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:43:50.312419   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:50.312571   721   768 I AT      : AT read end: 46
10-17 14:43:50.312636   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:50.312669   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:43:50.312711   721   768 D AT      : AT< OK
10-17 14:43:50.312741   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:43:50.312790   721   768 I AT      : AT read start
10-17 14:43:50.313425   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:43:50.313488   721   751 D RIL     : requestQueryThermal success
10-17 14:43:50.313519   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:50.313552   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:43:50.313595   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:43:50.313659   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f978570a0 
10-17 14:43:50.313699   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:43:50.313728   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:50.401884  1431  1481 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:52.448828   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185055/0
10-17 14:43:54.486445  1450  1450 D RILJ    : [9493]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:43:54.492627   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:43:54.492754   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda960, pRI=0x7f9784c540, p=0x7f97857420, pUCI=0x0
10-17 14:43:54.492794   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c540 p=0x7f97857420 dispatched to RIL_ATCI_PROXY
10-17 14:43:54.492953   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:54.492972   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:54.493010   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:54.493055   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:54.493060   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:54.493087   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:54.493142   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:54.493170   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:54.493214   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:54.493242   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:54.493290   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:54.493315   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:54.493370   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:54.493396   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:54.493436   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:54.493601   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:54.493665   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:54.493714   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:54.494119   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:54.494191   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:54.494229   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c540 p=0x7f97857420 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:54.494263   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:54.494296   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:43:54.494324   721   753 D RIL     : radioState:10
10-17 14:43:54.494371   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:43:54.494406   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:54.494434   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:43:54.494459   721   753 I AT      : AT write start
10-17 14:43:54.496821   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:54.496973   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:54.497036   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:54.497132   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:43:54.499067   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:54.499333   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:54.499455   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:54.499490   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:54.504920   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:54.505053   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:54.505154   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:54.505208   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:54.505824   721   770 I AT      : AT read end: 6
10-17 14:43:54.505927   721   770 D AT      : AT< OK
10-17 14:43:54.505964   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:54.506012   721   770 I AT      : AT read start
10-17 14:43:54.506171   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:54.506245   721   753 D RIL     : p_response->success = 1
10-17 14:43:54.506277   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:54.506305   721   753 D RIL     : strLength = 6
10-17 14:43:54.506333   721   753 D RIL     : line = <
10-17 14:43:54.506333   721   753 D RIL     : OK
10-17 14:43:54.506333   721   753 D RIL     : >
10-17 14:43:54.506365   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:54.506477   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:54.506710   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c540 p=0x7f97857420 
10-17 14:43:54.507476  1450  1606 D RILJ    : [9493]< OEM_HOOK_RAW [B@ee797c0 [SUB0]
10-17 14:43:54.506778   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda960
10-17 14:43:54.509235   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:55.120664  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:43:55.121208  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:43:57.449040   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185056/0
10-17 14:43:57.656105  1450  1450 D RILJ    : [9494]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:43:57.658155   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:43:57.658266   721   760 I RILC-MTK: create request 59: pRequest=0x7f94ce6a20, pRI=0x7f9784c660, p=0x7f97857c00, pUCI=0x0
10-17 14:43:57.658303   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c660 p=0x7f97857c00 dispatched to RIL_ATCI_PROXY
10-17 14:43:57.658447   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:43:57.658478   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:43:57.658519   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:43:57.658545   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:43:57.658584   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:43:57.658608   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:43:57.658644   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:43:57.658672   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:43:57.658703   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c660 p=0x7f97857c00 execute on RIL_ATCI_PROXY using channel 5
10-17 14:43:57.658734   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:43:57.658765   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:43:57.658790   721   753 D RIL     : radioState:10
10-17 14:43:57.658831   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:43:57.658862   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:43:57.658888   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:43:57.658910   721   753 I AT      : AT write start
10-17 14:43:57.658958   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:43:57.658990   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:43:57.659040   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:43:57.659065   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:43:57.659101   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:43:57.659125   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:43:57.659170   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:43:57.659194   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:43:57.659230   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:43:57.659253   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:43:57.659287   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:43:57.659311   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:43:57.659347   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:43:57.659370   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:43:57.659406   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:43:57.659429   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:43:57.659503   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:43:57.659550   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:43:57.659596   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:43:57.659698   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:43:57.661418   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:43:57.661495   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:43:57.661558   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:43:57.661599   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:57.661696   721   770 I AT      : AT read end: 6
10-17 14:43:57.661736   721   770 D AT      : AT< OK
10-17 14:43:57.661764   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:43:57.661807   721   770 I AT      : AT read start
10-17 14:43:57.662097   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:43:57.662132   721   753 D RIL     : p_response->success = 1
10-17 14:43:57.662160   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:43:57.662183   721   753 D RIL     : strLength = 6
10-17 14:43:57.662208   721   753 D RIL     : line = <
10-17 14:43:57.662208   721   753 D RIL     : OK
10-17 14:43:57.662208   721   753 D RIL     : >
10-17 14:43:57.662236   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:43:57.662283   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:57.662352   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c660 p=0x7f97857c00 
10-17 14:43:57.662384   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:43:57.662417   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:43:57.662599  1450  1606 D RILJ    : [9494]< OEM_HOOK_RAW [B@7584cf9 [SUB0]
10-17 14:43:59.093725  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.095480  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.096744  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.151000  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.151669  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.158108  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.166153  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.166522  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:59.176930  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.178522  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.179013  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.186501  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.187411  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.187815  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.194608  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.195596  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.196016  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.201992  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.204227  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.204639  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.212338  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.213299  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.213680  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.218899  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.219213  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.222275  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.225646  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.226129  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:59.230247  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.231226  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.231613  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.236971  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.237250  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.240234  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.243647  1450  2351 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.243867  1450  2351 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:59.248234  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.249280  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.249745  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.254841  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.255113  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.258091  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.261193  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.261375  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:59.265450  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.266498  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.266858  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.271963  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.272251  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.275082  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.278246  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.278487  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:43:59.285820   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:43:59.285909   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:43:59.285982   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:43:59.286036   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:43:59.286195   721   765 I AT      : AT read end: 37
10-17 14:43:59.286256   721   765 D AT      : AT< +ECSQ: 40,99,-281,1,1,1,1,3,32767
10-17 14:43:59.286289   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 40,99,-281,1,1,1,1,3,32767
10-17 14:43:59.286333   721   765 D RIL     : Nw URC:+ECSQ: 40,99,-281,1,1,1,1,3,32767
10-17 14:43:59.286408   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:43:59.286448   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:43:59.286475   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:43:59.286540   721   765 I AT      : AT read start
10-17 14:43:59.287093  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:43:59.287310  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 20 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -285 1 1
10-17 14:43:59.287419  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -281 1 1
10-17 14:43:59.287600  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.287731  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.287789  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.287823  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.287863  1450  1450 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.287903  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.287944  1450  1450 D GsmSST  : [GsmSST0] notifySignalStrength: mSignalStrength.getLevel=4
10-17 14:43:59.288198  1450  1450 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -281 1 1 sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad}
10-17 14:43:59.288816   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: subId=1 signalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -281 1 1
10-17 14:43:59.288928   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: logSSC.length=5 next=1
10-17 14:43:59.289328   909  1512 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T143934Europe/Samara(1,290,14400,0,1476700774) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:59.289769   909  1512 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:59.290188   909  1512 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:59.290620   909  1512 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:59.291215   909  1512 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:43:59.291311   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: ----------------
10-17 14:43:59.292765   909  1512 D TelephonyRegistry: validatePhoneId: true
10-17 14:43:59.292883   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: valid phoneId=0
10-17 14:43:59.292946   909  1512 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:59.293141   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -281 1 1
10-17 14:43:59.293278   909  1512 D TelephonyRegistry: idMatch: rlt=true
10-17 14:43:59.293446   909  1512 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -281 1 1
10-17 14:43:59.293698   909  1512 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:43:59.293971   909  1512 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.294156   909  1512 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.294245   909  1512 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.294290   909  1512 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.294338   909  1512 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.294365   909  1512 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295007  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295201  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.295285  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.295324  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295386  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.295419  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295600  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295660  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=20
10-17 14:43:59.295768  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295841  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.295894  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.295930  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.295973  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=20
10-17 14:43:59.296002  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296107  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296184  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.296234  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.296267  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296307  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.296335  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296364  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296407  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.296878  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.296965  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:43:59.297020  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:43:59.297052  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.297099  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:43:59.297127  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:43:59.299854  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:43:59.873565  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:43:59.874881  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:43:59.875701  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.887524  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.887969  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.891554  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.894879  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.895071  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:00.320988   721   760 I RILC    : NUMBER:1
10-17 14:44:00.321047   721   760 I RILC    : arg len:14
10-17 14:44:00.321081   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:44:00.321169   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:44:00.321238   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c7b0 p=0x7f97856ee0 dispatched to RIL_CMD_PROXY_1
10-17 14:44:00.321356   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:44:00.321384   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:44:00.321422   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:44:00.321446   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:44:00.321482   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:44:00.321510   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:44:00.321540   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c7b0 p=0x7f97856ee0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:44:00.321573   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:44:00.321598   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:44:00.321606   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:44:00.321629   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:44:00.321634   721   751 D RIL     : radioState:10
10-17 14:44:00.321670   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:44:00.321677   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:44:00.321695   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:44:00.321719   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:44:00.321731   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:44:00.321747   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:44:00.321755   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:44:00.321771   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:44:00.321789   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:44:00.321793   721   751 I AT      : AT write start
10-17 14:44:00.321816   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:44:00.321852   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:44:00.321876   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:44:00.321877   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:44:00.321906   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:44:00.321944   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:44:00.321976   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:44:00.322015   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:44:00.322040   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:44:00.322054   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:44:00.322074   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:44:00.322098   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:44:00.322104   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:44:00.322153   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:44:00.322254   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:44:00.329777   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:44:00.329932   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:44:00.330005   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:44:00.330049   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:00.330097   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:44:00.330140   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:44:00.330185   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:44:00.330222   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:00.330344   721   768 I AT      : AT read end: 46
10-17 14:44:00.330392   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:44:00.330425   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:44:00.330457   721   768 D AT      : AT< OK
10-17 14:44:00.330481   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:44:00.330519   721   768 I AT      : AT read start
10-17 14:44:00.331104   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:44:00.331172   721   751 D RIL     : requestQueryThermal success
10-17 14:44:00.331204   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:44:00.331235   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:44:00.331281   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:44:00.331340   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97856ee0 
10-17 14:44:00.331379   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:44:00.331874   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:44:00.883701  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:00.884649  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:00.885153  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:00.892971  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:00.893460  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:00.896447  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:00.900301  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:44:00.900470  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:02.449265   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185060/0
10-17 14:44:03.195386  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.196603  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.197045  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.215820  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.216232  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.222922  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.234139  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.235649  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.248897  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.249905  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.250366  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.255405  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.256762  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.257306  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.261885  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.262753  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.263400  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.267202  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.267857  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.268165  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.272625  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.273545  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.274031  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.278055  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.278260  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.280870  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.283421  1450 29539 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.283599  1450 29539 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.286724  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.287436  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.287763  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.291897  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.292115  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.294395  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.297001  1450  1511 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.297179  1450  1511 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.300485  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.301290  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.301633  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.305514  1450  1515 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.305727  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.308009  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.310363  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.310530  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.313933  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.314641  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.314975  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.318827  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.319037  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.321500  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.323827  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.323991  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:06.660241  1450  1450 D RILJ    : [9495]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:44:06.663298   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:44:06.663406   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9120, pRI=0x7f9784c210, p=0x7f978572d0, pUCI=0x0
10-17 14:44:06.663439   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f978572d0 dispatched to RIL_ATCI_PROXY
10-17 14:44:06.663570   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:44:06.663598   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:44:06.663635   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:44:06.663666   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:44:06.663706   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:44:06.663707   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:44:06.663738   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:44:06.663744   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:44:06.663770   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f978572d0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:44:06.663782   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:44:06.663799   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:44:06.663808   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:44:06.663828   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:44:06.663844   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:44:06.663852   721   753 D RIL     : radioState:10
10-17 14:44:06.663869   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:44:06.663890   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:44:06.663904   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:44:06.663924   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:44:06.663930   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:44:06.663950   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:44:06.663967   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:44:06.663972   721   753 I AT      : AT write start
10-17 14:44:06.663992   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:44:06.664027   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:44:06.664050   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:44:06.664143   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:44:06.664224   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:44:06.664279   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:44:06.664375   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:44:06.664459   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:44:06.664491   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:44:06.664534   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:44:06.664558   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:44:06.665359   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:44:06.665417   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:44:06.672545   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:44:06.672646   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:44:06.672723   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:44:06.672765   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:06.672937   721   770 I AT      : AT read end: 6
10-17 14:44:06.672978   721   770 D AT      : AT< OK
10-17 14:44:06.673008   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:44:06.673054   721   770 I AT      : AT read start
10-17 14:44:06.673112   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:44:06.673153   721   753 D RIL     : p_response->success = 1
10-17 14:44:06.673182   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:44:06.673209   721   753 D RIL     : strLength = 6
10-17 14:44:06.673242   721   753 D RIL     : line = <
10-17 14:44:06.673242   721   753 D RIL     : OK
10-17 14:44:06.673242   721   753 D RIL     : >
10-17 14:44:06.673275   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:44:06.673328   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:06.673408   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f978572d0 
10-17 14:44:06.673441   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9120
10-17 14:44:06.673466   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:44:06.673664  1450  1606 D RILJ    : [9495]< OEM_HOOK_RAW [B@9a2d43e [SUB0]
10-17 14:44:07.446341   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:07.787873   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:11.480394   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:12.607935   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:16.261062   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:21.726992   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:24.296362   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:24.734964   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:33.209262   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:41.682589   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:58.630752   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:07.104792   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:15.578683   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:32.526292   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:36.372316   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:36.785249   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.205077   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.395836   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.999639   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:45.951575   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:46.627620   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:49.473400   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:56.957396 25918 25952 D getTestMode: Test mode is 0
10-17 14:45:57.947286   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:02.234692   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:02.248160   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:05.120045  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:05.126681  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:07.454200   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185112/0
10-17 14:46:10.520698   721   760 I RILC    : NUMBER:1
10-17 14:46:10.520765   721   760 I RILC    : arg len:14
10-17 14:46:10.520800   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:10.520943   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:10.521002   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c3f0 p=0x7f97856690 dispatched to RIL_CMD_PROXY_1
10-17 14:46:10.521116   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:10.521143   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:10.521149   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:10.521187   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:10.521199   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:10.521222   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:10.521264   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:10.521269   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:10.521297   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:10.521339   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:10.521342   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:10.521366   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:10.521404   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:10.521444   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:10.521469   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:10.521505   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:10.521533   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:10.521566   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c3f0 p=0x7f97856690 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:10.521599   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:10.521628   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:10.521656   721   751 D RIL     : radioState:10
10-17 14:46:10.521695   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:10.521736   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:10.521764   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:10.521789   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:10.521812   721   751 I AT      : AT write start
10-17 14:46:10.521913   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:10.521939   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:10.521948   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:10.521997   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:10.522112   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:10.522170   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:10.522226   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:10.522326   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:10.522416   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:10.522422   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:10.522454   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:10.529905   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:10.530051   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:10.530132   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:10.530181   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:10.530235   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:10.530292   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:10.530343   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:10.530384   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:10.530499   721   768 I AT      : AT read end: 46
10-17 14:46:10.530546   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:10.530578   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:10.530615   721   768 D AT      : AT< OK
10-17 14:46:10.530640   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:10.530677   721   768 I AT      : AT read start
10-17 14:46:10.531282   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:10.531338   721   751 D RIL     : requestQueryThermal success
10-17 14:46:10.531369   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:10.531398   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:10.531436   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:10.531498   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c3f0 p=0x7f97856690 
10-17 14:46:10.531535   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:46:10.531567   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:12.454440   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185114/0
10-17 14:46:17.389891  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:17.394358  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:46:17.394570  1450  1450 D RILJ    : [9507]> SCREEN_STATE: false [SUB0]
10-17 14:46:17.397130  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:17.397434   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.397546   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf91e0, pRI=0x7f9784c8d0, p=0x7f978567e0, pUCI=0x0
10-17 14:46:17.397588   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c8d0 p=0x7f978567e0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.397714   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.397730  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:46:17.397755   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.397764   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.397814   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.397841   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.397852  1450  1450 D RILJ    : [9508]> SCREEN_STATE: false [SUB1]
10-17 14:46:17.397880   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.397904   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.397943   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.397971   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.398010   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.398033   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.398068   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.398097   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:17.398127   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c8d0 p=0x7f978567e0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:17.398155   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.398195   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.398226   721   749 D RIL     : radioState:10
10-17 14:46:17.398224   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.398259   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.398296   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.398300   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.398326   721   749 D AT      : AT> AT+CREG=1
10-17 14:46:17.398326   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.398353   721   749 I AT      : AT write start
10-17 14:46:17.398369   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.398393   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.398431   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.398447   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.398459   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.398501   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.398536   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.399184   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.399279   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.399331   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.399419   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.400708   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.400794   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cda760, pRI=0x7f9784c930, p=0x7f97856e70, pUCI=0x0
10-17 14:46:17.400830   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97856e70 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:17.400995   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.401005   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.401010   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.401050   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.401094   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.401110   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.401119   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.401149   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.401163   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.401179   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:17.401187   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.401210   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97856e70 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:17.401220   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.401240   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.401244   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.401270   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.401295   721   755 D RIL     : radioState:0
10-17 14:46:17.401317   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.401335   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401341   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.401359   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401380   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.401397   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401403   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.401429   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.401443   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.401476   721   755 D AT      : AT> AT+CREG=1
10-17 14:46:17.401500   721   755 I AT      : AT write start
10-17 14:46:17.401592   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.401618   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.401654   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.401692   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.401799   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.401856   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.401905   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.401987   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.406800   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.406878   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.406944   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.406985   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.407088   721   766 I AT      : AT read end: 6
10-17 14:46:17.407139   721   766 D AT      : AT< OK
10-17 14:46:17.407170   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.407215   721   766 I AT      : AT read start
10-17 14:46:17.407231   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.407253   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.407281   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.407305   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.407331   721   749 D AT      : AT> AT+CGREG=1
10-17 14:46:17.407341   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.407355   721   749 I AT      : AT write start
10-17 14:46:17.407381   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.407467   721   772 I AT      : AT read end: 6
10-17 14:46:17.407495   721   772 D AT      : AT< OK
10-17 14:46:17.407526   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.407567   721   772 I AT      : AT read start
10-17 14:46:17.407608   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.407636   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.407658   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.407680   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.407685   721   755 D AT      : AT> AT+CGREG=1
10-17 14:46:17.407712   721   755 I AT      : AT write start
10-17 14:46:17.407728   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.407810   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.407833   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.407874   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.407920   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.407988   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.408628   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.408691   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.408760   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.408803   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.408894   721   766 I AT      : AT read end: 6
10-17 14:46:17.408934   721   766 D AT      : AT< OK
10-17 14:46:17.408963   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.408998   721   766 I AT      : AT read start
10-17 14:46:17.409036   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.409100   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.409149   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:46:17.409175   721   749 I AT      : AT write start
10-17 14:46:17.409216   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.409267   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.409290   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.409324   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.409337   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.409364   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.409381   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.409467   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.409531   721   772 I AT      : AT read end: 6
10-17 14:46:17.409561   721   772 D AT      : AT< OK
10-17 14:46:17.409589   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.409627   721   772 I AT      : AT read start
10-17 14:46:17.409671   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.409714   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.409742   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:46:17.409764   721   755 I AT      : AT write start
10-17 14:46:17.409889   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.409936   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.409982   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.410056   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.410704   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.410763   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.410828   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.410871   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.411100   721   766 I AT      : AT read end: 6
10-17 14:46:17.411161   721   766 D AT      : AT< OK
10-17 14:46:17.411252   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.411254   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.411296   721   766 I AT      : AT read start
10-17 14:46:17.411313   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.411380   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.411423   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.411519   721   772 I AT      : AT read end: 6
10-17 14:46:17.411524   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.411561   721   772 D AT      : AT< OK
10-17 14:46:17.411580   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.411588   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.411608   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:46:17.411627   721   772 I AT      : AT read start
10-17 14:46:17.411632   721   749 I AT      : AT write start
10-17 14:46:17.411663   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.411703   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.411728   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:46:17.411750   721   755 I AT      : AT write start
10-17 14:46:17.411777   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.411828   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.411865   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.411877   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.411907   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.411972   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:17.412033   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.412104   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:17.412764   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.412825   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.412889   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.412930   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.413026   721   766 I AT      : AT read end: 6
10-17 14:46:17.413063   721   766 D AT      : AT< OK
10-17 14:46:17.413091   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.413127   721   766 I AT      : AT read start
10-17 14:46:17.413174   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.413290   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.413319   721   749 D AT      : AT> AT+CEREG=1
10-17 14:46:17.413343   721   749 I AT      : AT write start
10-17 14:46:17.413463   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.413467   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.413515   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.413520   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.413561   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.413578   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.413621   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.413637   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.413715   721   772 I AT      : AT read end: 6
10-17 14:46:17.413746   721   772 D AT      : AT< OK
10-17 14:46:17.413771   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.413811   721   772 I AT      : AT read start
10-17 14:46:17.413857   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.413900   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.413924   721   755 D AT      : AT> AT+CEREG=1
10-17 14:46:17.413946   721   755 I AT      : AT write start
10-17 14:46:17.414063   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.414111   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.414157   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.414234   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.414789   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.414848   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.414909   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.414947   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.415043   721   766 I AT      : AT read end: 6
10-17 14:46:17.415074   721   766 D AT      : AT< OK
10-17 14:46:17.415100   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.415142   721   766 I AT      : AT read start
10-17 14:46:17.415184   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.415220   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:17.415263   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.415333   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c8d0 p=0x7f978567e0 
10-17 14:46:17.415371   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf91e0
10-17 14:46:17.415397   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:17.415513  1450  1606 D RILJ    : [9507]< SCREEN_STATE  [SUB0]
10-17 14:46:17.416079   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.416153   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.416226   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.416270   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.416385   721   772 I AT      : AT read end: 6
10-17 14:46:17.416425   721   772 D AT      : AT< OK
10-17 14:46:17.416452   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.416499   721   772 I AT      : AT read start
10-17 14:46:17.416573   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.416615   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:17.416654   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:17.416730   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c930 p=0x7f97856e70 
10-17 14:46:17.416763   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:46:17.416791   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.416895  1450  1609 D RILJ    : [9508]< SCREEN_STATE  [SUB1]
10-17 14:46:17.454626   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185124/0
10-17 14:46:17.634776  1450  1450 D RILJ    : [9509]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:17.636509   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:17.636584   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9240, pRI=0x7f9784cae0, p=0x7f97857d50, pUCI=0x0
10-17 14:46:17.636618   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cae0 p=0x7f97857d50 dispatched to RIL_ATCI_PROXY
10-17 14:46:17.636707   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.636710   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.636714   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.636744   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.636756   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.636782   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.636800   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.636808   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:17.636814   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.636815   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.636847   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.636853   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cae0 p=0x7f97857d50 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:17.636879   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.636883   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.636906   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:17.636917   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:17.636940   721   753 D RIL     : radioState:10
10-17 14:46:17.636948   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.636970   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.636979   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:17.637010   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:17.637012   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.637038   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:17.637062   721   753 I AT      : AT write start
10-17 14:46:17.637063   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.637083   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.637131   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.637149   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.637223   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.637272   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.637322   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:17.637419   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:17.637469   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.637519   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.637568   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.637598   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.644820   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:17.644900   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:17.644968   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:17.645021   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.645119   721   770 I AT      : AT read end: 6
10-17 14:46:17.645159   721   770 D AT      : AT< OK
10-17 14:46:17.645187   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:17.645227   721   770 I AT      : AT read start
10-17 14:46:17.645267   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:17.645309   721   753 D RIL     : p_response->success = 1
10-17 14:46:17.645337   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:17.645359   721   753 D RIL     : strLength = 6
10-17 14:46:17.645382   721   753 D RIL     : line = <
10-17 14:46:17.645382   721   753 D RIL     : OK
10-17 14:46:17.645382   721   753 D RIL     : >
10-17 14:46:17.645408   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:17.645453   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.645523   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cae0 p=0x7f97857d50 
10-17 14:46:17.645554   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:46:17.645577   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.645726  1450  1606 D RILJ    : [9509]< OEM_HOOK_RAW [B@7708533 [SUB0]
10-17 14:46:17.796150  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.797315  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.797765  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.818583  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:17.819639  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:17.824550  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:17.829652  1450  1807 D DCT     : [0]phoneSubId = 1
10-17 14:46:17.831300  1450  1807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:17.938800  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.951296  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:17.952141  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:46:17.952299  1450  1450 D RILJ    : [9510]> SCREEN_STATE: true [SUB0]
10-17 14:46:17.954836  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:17.955639  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:46:17.955735   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.955808   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6a20, pRI=0x7f9784c360, p=0x7f97857dc0, pUCI=0x0
10-17 14:46:17.955821  1450  1450 D RILJ    : [9511]> SCREEN_STATE: true [SUB1]
10-17 14:46:17.955847   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97857dc0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.955980   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.956000   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.956035   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.956092   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.956136   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.956141   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.956174   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.956226   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.956268   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.956304   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.956349   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.956377   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.956421   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.956448   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.956492   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.956516   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.956562   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.956591   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.956632   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.956657   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.957047   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.957113   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:17.957154   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97857dc0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:17.957190   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.957225   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.957253   721   749 D RIL     : radioState:10
10-17 14:46:17.957331   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.957361   721   749 D AT      : AT> AT+CREG=3
10-17 14:46:17.957387   721   749 I AT      : AT write start
10-17 14:46:17.957645   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.957697   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.957731   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.957804   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.957861   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.957986   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.961839   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.961957   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9460, pRI=0x7f9784c4b0, p=0x7f97857e30, pUCI=0x0
10-17 14:46:17.961999   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c4b0 p=0x7f97857e30 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:17.962116   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.962116   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.962173   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.962207   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.962233   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.962244   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.962295   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.962299   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.962325   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.962365   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.962367   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.962403   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.962443   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.962468   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.962509   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.962554   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.962578   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.962621   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.962927   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.963032   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:17.963094   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c4b0 p=0x7f97857e30 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:17.963132   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.963125   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.963169   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.963172   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.963212   721   755 D RIL     : radioState:0
10-17 14:46:17.963257   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963284   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963312   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963367   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.963396   721   755 D AT      : AT> AT+CREG=3
10-17 14:46:17.963422   721   755 I AT      : AT write start
10-17 14:46:17.964142   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.964231   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.964286   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.964379   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.965635   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:46:17.965729   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:17.965834   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:46:17.965888   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.965945   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.965987   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.966043   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.966086   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.966209   721   765 I AT      : AT read end: 36
10-17 14:46:17.966268   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966304   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966349   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966392   721   765 D RIL     : NW state changed: normal case
10-17 14:46:17.966425   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:46:17.966458   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:17.966488   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:46:17.966547   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:46:17.966582   721   765 D RIL     : bCREGType3Support=1
10-17 14:46:17.966612   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:17.966618   721   766 I AT      : AT read end: 6
10-17 14:46:17.966638   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:46:17.966657   721   766 D AT      : AT< OK
10-17 14:46:17.966689   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.966723   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:17.966735   721   766 I AT      : AT read start
10-17 14:46:17.966901   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.966887   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.965318  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.966959   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.966970   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e434e0
10-17 14:46:17.966988   721   749 D AT      : AT> AT+CGREG=3
10-17 14:46:17.967004   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e434f0
10-17 14:46:17.967013   721   749 I AT      : AT write start
10-17 14:46:17.967120   721   765 I AT      : AT read start
10-17 14:46:17.967355  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.967385  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:46:17.967637   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.967720   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.967783   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.967900   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.968202  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:17.968366  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:46:17.968517  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:17.968859   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:46:17.968956   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:46:17.969048   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:46:17.969101   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.969157   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.969206   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.969338   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.969392   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.969920   721   771 I AT      : AT read end: 36
10-17 14:46:17.970028   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970063   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970110   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970150   721   771 D RIL     : NW state changed: normal case
10-17 14:46:17.970185   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:46:17.970217   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:46:17.970249   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:46:17.970309   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:46:17.970347   721   771 D RIL     : bCREGType3Support=1
10-17 14:46:17.970378   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:17.970409   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:46:17.970497   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:17.970531   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:17.970596   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e434e0, cancel
10-17 14:46:17.970631   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e435a0
10-17 14:46:17.970666   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e435b0
10-17 14:46:17.970739   721   771 I AT      : AT read start
10-17 14:46:17.970822   721   772 I AT      : AT read end: 6
10-17 14:46:17.970851   721   772 D AT      : AT< OK
10-17 14:46:17.971136   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.971228   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.971329   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.971386   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.971392  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:46:17.971481  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:46:17.971488  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:46:17.971550   721   766 I AT      : AT read end: 6
10-17 14:46:17.971587   721   766 D AT      : AT< OK
10-17 14:46:17.971605  1450  1450 D RILJ    : [9512]> OPERATOR [SUB0]
10-17 14:46:17.971616   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.971666   721   766 I AT      : AT read start
10-17 14:46:17.970887   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.971735   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.971752   721   772 I AT      : AT read start
10-17 14:46:17.971806   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.971836   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:46:17.971865   721   749 I AT      : AT write start
10-17 14:46:17.971997   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.972069   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.972099   721   755 D AT      : AT> AT+CGREG=3
10-17 14:46:17.972129   721   755 I AT      : AT write start
10-17 14:46:17.972348   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.972413   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.972468   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.972558   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.973078   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.973156   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.973211   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.973305   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.973698  1450  1450 D RILJ    : [9513]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:46:17.974292   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:46:17.974376   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9540, pRI=0x7f9784c6f0, p=0x7f97857f10, pUCI=0x0
10-17 14:46:17.974413   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.974523   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.974559   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.974604   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.974630   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.974721   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.974755   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.974855   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.974886   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.974928   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.974955   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.974996   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.975023   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.975086   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.975112   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.975158   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.975183   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.975184   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.975219   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.975357   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.975392   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.975666  1450  1450 D RILJ    : [9514]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:46:17.976124   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:17.976213   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9b80, pRI=0x7f9784cb10, p=0x7f97857f80, pUCI=0x0
10-17 14:46:17.976253   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.976284   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.976321   721   760 D RILC-MTK: Request pRI=0x7f9784cb10 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:46:17.977963  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.978076  1450  1450 D RILJ    : [9515]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:46:17.978453   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:17.978547   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9bc0, pRI=0x7f9784cba0, p=0x7f97857ff0, pUCI=0x0
10-17 14:46:17.978588   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.978619   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.978650   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.978683   721   760 D RILC-MTK: Request pRI=0x7f9784cba0 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:46:17.980733   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.980834   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.983041   721   772 I AT      : AT read end: 6
10-17 14:46:17.983131   721   772 D AT      : AT< OK
10-17 14:46:17.983165   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.983215   721   772 I AT      : AT read start
10-17 14:46:17.983286   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.983343   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.983373   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:46:17.983398   721   755 I AT      : AT write start
10-17 14:46:17.983518   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.983570   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.983595   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.983618   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.983657   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.983671   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.983698   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.983762   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.983775   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.983814   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.983941   721   766 I AT      : AT read end: 6
10-17 14:46:17.983992   721   766 D AT      : AT< OK
10-17 14:46:17.984023   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.984063   721   766 I AT      : AT read start
10-17 14:46:17.984119   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.984172   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.984201   721   749 D AT      : AT> AT+ECSQ
10-17 14:46:17.984239   721   749 I AT      : AT write start
10-17 14:46:17.985467   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.985566   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.985630   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.985727   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:46:17.986599  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.987042  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.988018  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:17.988177  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:17.988266  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:46:17.988353  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:17.988405  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:46:17.989349  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:17.989478  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:17.989552  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:46:17.989603  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:46:17.989688  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:17.989749  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:46:17.989808  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:46:17.989862  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:46:17.989904  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:46:17.989941  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:46:17.989973  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:17.990088  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:17.990191  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:46:17.990258  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:46:17.990308  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:46:17.990560  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:46:17.991128   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:17.991312   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9be0, pRI=0x7f9784cbd0, p=0x7f97858140, pUCI=0x0
10-17 14:46:17.991358   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991389   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991418   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cba0 p=0x7f97857ff0 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991448   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.991447   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.991485   721   760 D RILC-MTK: Request pRI=0x7f9784cbd0 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:46:17.991512   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.991589   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.991634   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.991738   721   772 I AT      : AT read end: 6
10-17 14:46:17.991808   721   772 D AT      : AT< OK
10-17 14:46:17.991838   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.991878   721   772 I AT      : AT read start
10-17 14:46:17.991931   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.991954   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:46:17.991975   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.992002   721   755 D AT      : AT> AT+ECSQ
10-17 14:46:17.992005   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.992029   721   755 I AT      : AT write start
10-17 14:46:17.992076   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:46:17.992117   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.992195   721   766 I AT      : AT read end: 37
10-17 14:46:17.992225   721   766 D AT      : AT< +ECSQ: 42,99,-273,1,1,1,1,3,32767
10-17 14:46:17.992252   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 42,99,-273,1,1,1,1,3,32767
10-17 14:46:17.992282   721   766 I AT      : AT read start
10-17 14:46:17.992277   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.992326   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.992375   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.992458   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:46:17.993089   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.993167   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.993242   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.993285   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.993420   721   766 I AT      : AT read end: 6
10-17 14:46:17.993463   721   766 D AT      : AT< OK
10-17 14:46:17.993490   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.993541   721   766 I AT      : AT read start
10-17 14:46:17.993599   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.993694   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:17.993737   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:17.993763   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.993835   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.993863   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:46:17.993887   721   749 I AT      : AT write start
10-17 14:46:17.994091   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:46:17.994171   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.994244   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:46:17.994286   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.994340   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.994383   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.994430   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.994468   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.994567   721   772 I AT      : AT read end: 42
10-17 14:46:17.994603   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:17.994631   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:17.994668   721   772 D AT      : AT< OK
10-17 14:46:17.994693   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.994731   721   772 I AT      : AT read start
10-17 14:46:17.994773   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.994822   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:46:17.994859   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:46:17.994888   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.994911   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:46:17.994933   721   755 I AT      : AT write start
10-17 14:46:17.995083   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.995144   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.995194   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.995270   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:17.995639   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.995709   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.995760   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.995840   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:17.997082   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.997177   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.997446   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.997496   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.997559   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.997602   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.997658   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.997699   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.997833   721   772 I AT      : AT read end: 6
10-17 14:46:17.997884   721   772 D AT      : AT< OK
10-17 14:46:17.997919   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.997962   721   772 I AT      : AT read start
10-17 14:46:17.998007   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.998023   721   766 I AT      : AT read end: 6
10-17 14:46:17.998050   721   766 D AT      : AT< OK
10-17 14:46:17.998074   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.998079   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.998109   721   755 D AT      : AT> AT+CEREG=3
10-17 14:46:17.998123   721   766 I AT      : AT read start
10-17 14:46:17.998150   721   755 I AT      : AT write start
10-17 14:46:17.998417   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.998483   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.998511   721   749 D AT      : AT> AT+CEREG=3
10-17 14:46:17.998536   721   749 I AT      : AT write start
10-17 14:46:17.998712   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.998712   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.998775   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.998774   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.998831   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.998925   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.998998   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.999086   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:18.000472   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.000544   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.000624   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.000671   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.000810   721   766 I AT      : AT read end: 6
10-17 14:46:18.001044   721   766 D AT      : AT< OK
10-17 14:46:18.001093   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.001146   721   766 I AT      : AT read start
10-17 14:46:18.000233  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.001249   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.001301   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.001341   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.001430   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97857dc0 
10-17 14:46:18.001464   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:46:18.001504   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.001537   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.001567   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.001596   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:18.001619   721   749 D RIL     : radioState:10
10-17 14:46:18.001656   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.001691   721   749 D AT      : AT> AT+COPS?
10-17 14:46:18.001715   721   749 I AT      : AT write start
10-17 14:46:18.001948   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.002035   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.002096   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.002191   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.002290   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:18.002342   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.002357  1450  1606 D RILJ    : [9510]< SCREEN_STATE  [SUB0]
10-17 14:46:18.002426   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:18.002473   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.002613   721   772 I AT      : AT read end: 6
10-17 14:46:18.002662   721   772 D AT      : AT< OK
10-17 14:46:18.002696   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:18.002689  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.002758   721   772 I AT      : AT read start
10-17 14:46:18.002790  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.002819   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.002848  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:46:18.002863   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.002909   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.002999   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f97857e30 
10-17 14:46:18.003036   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9460
10-17 14:46:18.003064   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.003300  1450  1609 D RILJ    : [9511]< SCREEN_STATE  [SUB1]
10-17 14:46:18.003284  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.003715  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.004434   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:18.004518   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.004598   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:18.004640   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.004690   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.004731   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.004776   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.004818   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.004978   721   766 I AT      : AT read end: 30
10-17 14:46:18.005022   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:18.005055   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:18.005093   721   766 D AT      : AT< OK
10-17 14:46:18.005119   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.005157   721   766 I AT      : AT read start
10-17 14:46:18.005218   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.005269   721   749 D RIL     : Get operator code 25020
10-17 14:46:18.005305   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:46:18.005348   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:46:18.005379   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.005443   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.005525   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f97857f10 
10-17 14:46:18.005568   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9540
10-17 14:46:18.005601   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.005637   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.005667   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.005697   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.005722   721   749 D RIL     : radioState:10
10-17 14:46:18.005776   721   749 D RIL     : request gprs reg state: normal case
10-17 14:46:18.005810   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.005838   721   749 D AT      : AT> AT+CGREG?
10-17 14:46:18.005861   721   749 I AT      : AT write start
10-17 14:46:18.007482   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.007579   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.007637   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.007731   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:18.008185  1450  1606 D RILJ    : [9512]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:46:18.010680  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:46:18.010871  1450  1450 D RILJ    : [9516]> OPERATOR [SUB1]
10-17 14:46:18.015035  1450  1450 D RILJ    : [9517]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:46:18.016083   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:46:18.016112   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:46:18.016176   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.016180   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9c00, pRI=0x7f9784cc00, p=0x7f978581b0, pUCI=0x0
10-17 14:46:18.016219   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cc00 p=0x7f978581b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.016274   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:46:18.016320   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.016342   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.016377   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.016385   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.016422   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784cc00 p=0x7f978581b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.016424   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.016456   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.016483   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.016487   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:18.016516   721   755 D RIL     : radioState:0
10-17 14:46:18.016527   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.016566   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016593   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016620   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016649   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016687   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.016717   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.016771   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.016782   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.016822   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.016853   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc00 p=0x7f978581b0 
10-17 14:46:18.016867   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.016886   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c00
10-17 14:46:18.016894   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.016970   721   766 I AT      : AT read end: 50
10-17 14:46:18.017006   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:18.017036   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:18.017071   721   766 D AT      : AT< OK
10-17 14:46:18.017097   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.017144   721   766 I AT      : AT read start
10-17 14:46:18.017331   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.017344  1450  1609 D RilRequest: [9516]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.017383   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.017436   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.017464   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.017495   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.017507   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.017535   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.017543   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.017573   721   749 E RIL     : The value in the field <lac> :0
10-17 14:46:18.017576   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.017610   721   749 D RIL     : cid: 3583
10-17 14:46:18.017627   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.017640   721   749 E RIL     : The value of act: 3
10-17 14:46:18.017668   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.017673   721   749 D RIL     : cause_type: 0
10-17 14:46:18.017694   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.017702   721   749 D RIL     : reject_cause: 0
10-17 14:46:18.017737   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.017744   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.017767   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.017773   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:46:18.017799   721   749 I AT      : AT write start
10-17 14:46:18.017961   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.017991   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.018053   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.018272   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.018340   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.018392   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.018480   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:46:18.019033  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.020175  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.020547  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.022159  1450  1450 D RILJ    : [9518]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:46:18.022845   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:18.022916   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9c80, pRI=0x7f9784cc30, p=0x7f978565b0, pUCI=0x0
10-17 14:46:18.022953   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f978565b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.023103   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.023134   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.023148   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.023196   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.023204   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.023224   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.023270   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.023273   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.023299   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.023312   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f978565b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.023342   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.023377   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.023404   721   755 D RIL     : radioState:0
10-17 14:46:18.023425   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.023448   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023454   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.023477   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023506   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023498   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.023534   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023543   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.023572   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.023587   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.023603   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.023620   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.023629   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.023648   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.023653   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.023710   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc30 p=0x7f978565b0 
10-17 14:46:18.023710   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.023741   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.023750   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c80
10-17 14:46:18.023781   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.023994   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.024342   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.024418   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.024660  1450  1450 D RILJ    : [9519]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:46:18.024869   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:18.024963  1450  1609 D RilRequest: [9517]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.024978   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9ca0, pRI=0x7f9784c510, p=0x7f97856bd0, pUCI=0x0
10-17 14:46:18.025022   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f97856bd0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.025128   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.025164   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.025242   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.025252   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.025280   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.025325   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.025332   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.025363   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.025381   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f97856bd0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.025414   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.025448   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.025479   721   755 D RIL     : radioState:0
10-17 14:46:18.025531   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025558   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025585   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025615   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025650   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.025678   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.025727   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.025789   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f97856bd0 
10-17 14:46:18.025829   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9ca0
10-17 14:46:18.025856   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.025949   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.025978   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.026047   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.026079   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.026175   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.026216   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.026262   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.026287   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.026362   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.026416  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.026398   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.026459   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:46:18.026506   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.026519   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.026534   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.026530  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:18.026580   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.026597   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:46:18.026604   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.026643   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.026683  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:18.026760   721   766 I AT      : AT read end: 19
10-17 14:46:18.026795   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:46:18.026813  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:18.026826   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:46:18.026862   721   766 I AT      : AT read start
10-17 14:46:18.026860  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.026948  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:18.027073  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:18.027117  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:18.027887   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:18.027962   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cda740, pRI=0x7f9784cab0, p=0x7f97856c40, pUCI=0x0
10-17 14:46:18.027999   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cab0 p=0x7f97856c40 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.028123   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.028148   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.028159   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.028199   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.028203   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.028211   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.028234   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.028275   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.028279   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.028314   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.028640  1450  1609 D RilRequest: [9518]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.028839   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.028879   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.028933   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.028959   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.029019   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.029099   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.029315   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.029350   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.029383   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cab0 p=0x7f97856c40 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.029415   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.029447   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:18.029473   721   755 D RIL     : radioState:0
10-17 14:46:18.029512   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.029541   721   755 D AT      : AT> AT+COPS?
10-17 14:46:18.029564   721   755 I AT      : AT write start
10-17 14:46:18.031774   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.031847   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.031901   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:18.031990   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:46:18.032111   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.032154   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.032224   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.032249   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.032351   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.032406   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.032490   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.032534   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.032701   721   766 I AT      : AT read end: 6
10-17 14:46:18.032742   721   766 D AT      : AT< OK
10-17 14:46:18.032774   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.032823   721   766 I AT      : AT read start
10-17 14:46:18.032894   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.032979   721   749 E RIL     : rid: 0
10-17 14:46:18.033011   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:18.033042   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:18.033068   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:18.033097   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:18.033127   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.033186   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.033290   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f97857f80 
10-17 14:46:18.033334   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:46:18.033366   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.033398   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cba0 p=0x7f97857ff0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.033428   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.033459   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.033484   721   749 D RIL     : radioState:10
10-17 14:46:18.033525   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.033554   721   749 D AT      : AT> AT+CREG?
10-17 14:46:18.033578   721   749 I AT      : AT write start
10-17 14:46:18.034042  1450  1606 D RILJ    : [9513]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:46:18.034770  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.034876  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:46:18.034948  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:46:18.034994  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:46:18.036732  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.036829  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:46:18.036902  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:46:18.036955  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:46:18.037037  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:46:18.037088  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:46:18.037126  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:46:18.037165  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:46:18.037284  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:46:18.037580   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.037665   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.037722   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.037820   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.041212   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:46:18.041285   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.041381   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:46:18.041429   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041486   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:18.041529   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.041588   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:18.041631   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041679   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:46:18.041747   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.041810   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:46:18.041854   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041901   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.041942   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.041987   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.042024   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.042293   721   766 I AT      : AT read end: 44
10-17 14:46:18.042337   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:18.042369   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:18.042415   721   766 D AT      : AT< OK
10-17 14:46:18.042441   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.042465   721   772 I AT      : AT read end: 18
10-17 14:46:18.042482   721   766 I AT      : AT read start
10-17 14:46:18.042498   721   772 D AT      : AT< +COPS: 0
10-17 14:46:18.042525   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:46:18.042533   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.042556   721   772 D AT      : AT< OK
10-17 14:46:18.042585   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.042583   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:18.042623   721   749 E RIL     : The value in the field <lac> :127
10-17 14:46:18.042635   721   772 I AT      : AT read start
10-17 14:46:18.042668   721   749 D RIL     : cid: 3583
10-17 14:46:18.042699   721   749 E RIL     : The value of act: 3
10-17 14:46:18.042724   721   749 D RIL     : cause_type: 0
10-17 14:46:18.042749   721   749 D RIL     : reject_cause: 0
10-17 14:46:18.042813   721   749 E RIL     : rid: 0
10-17 14:46:18.042846   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:18.042880   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:18.042907   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:18.042937   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:18.042967   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.043006   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.043088   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.043183   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f97857ff0 
10-17 14:46:18.043217   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9bc0
10-17 14:46:18.043257   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.043290   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cbd0 p=0x7f97858140 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.043322   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.043352   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:18.043376   721   749 D RIL     : radioState:10
10-17 14:46:18.043420   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.043447   721   749 D AT      : AT> AT+COPS?
10-17 14:46:18.043469   721   749 I AT      : AT write start
10-17 14:46:18.043488  1450  1606 D RILJ    : [9514]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:46:18.043711   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.043781   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.043834   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.043893   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.043936   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.043951   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.044005   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.044090   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cab0 p=0x7f97856c40 
10-17 14:46:18.044123   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda740
10-17 14:46:18.044153   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.044388  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:46:18.044481  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:46:18.044567  1450  1609 D RILJ    : [9519]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:46:18.045742   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:18.045812   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.045884   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:18.045928   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.046110   721   766 I AT      : AT read end: 24
10-17 14:46:18.046152   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:18.046184   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:18.046222   721   766 I AT      : AT read start
10-17 14:46:18.046297   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.046343   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.046403   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.046442   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.046522   721   766 I AT      : AT read end: 6
10-17 14:46:18.046551   721   766 D AT      : AT< OK
10-17 14:46:18.046582   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.046623   721   766 I AT      : AT read start
10-17 14:46:18.046673   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.046721   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.046772   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.046860   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97858140 
10-17 14:46:18.046893   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9be0
10-17 14:46:18.046920   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.047017  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:46:18.047086  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:46:18.047160  1450  1606 D RILJ    : [9515]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:46:18.053316  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.053495  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:18.055702  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:18.055804  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:46:18.055847  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.055913  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:46:18.055955  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.055985  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.056032  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:18.056068  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.056106  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.056163  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:46:18.056220  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:46:18.056262  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:46:18.056430  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:46:18.056491  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:18.056544  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:46:18.056579  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.056646  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:18.058263  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:46:18.058361  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:46:18.058453  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:46:18.058493  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:46:18.058661  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:46:18.058706  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:46:18.058745  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.058806  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:18.058846  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.058877  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.059714  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:18.059798  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:46:18.061747  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:46:18.061837  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:46:18.061893  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:18.062053  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:18.062201  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:46:18.062485  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:18.062568  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:18.062629  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:46:18.062685  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:46:18.062871  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:18.062937  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:18.063010  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:46:18.063102  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063157  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063202  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063247  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063294  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063339  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063390  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063434  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063495  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063546  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063588  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:46:18.063632  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:46:18.063678  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:46:18.063743  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:46:18.064749  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:46:18.065672  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.065839  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:46:18.066546  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:46:18.067460  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:46:18.067
10-17 14:46:18.067669  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:46:18.068471  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.068798  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.068943  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:46:18.069020  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:46:18.069092  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.069396  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:46:18.070181   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.070315   909  6090 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.070527   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=2
10-17 14:46:18.071006   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.071502   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.071960   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072398   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072813   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072904   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:46:18.072961   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073125   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.073250   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073407   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.073715   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073928   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074180   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.074386   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074498   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.074679   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074931   909  6090 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.075285  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.075462  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:18.075530  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:18.075565  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.075609  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:18.075636  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.086654  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.087641   909  6090 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.092721  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:46:18.092840  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.093082  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.093157  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:18.098944   909  7313 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.099263   909  7313 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.101247  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.101386  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:18.103171   909  6089 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.103576   909  6089 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.104891  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:46:18.106530  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.107349  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.107567  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:18.107843  1450  1450 D RILJ    : [9520]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:18.111618   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:18.111732   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cdaa00, pRI=0x7f9784cd80, p=0x7f97856cb0, pUCI=0x0
10-17 14:46:18.111773   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f97856cb0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:18.111899   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.111955   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.111960   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.111996   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.112036   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.112045   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.112065   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.112115   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.112150   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.112191   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:18.112211   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.112257   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.112284   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.112316   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.112329   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.112344   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.112372   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f97856cb0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.112403   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.112405   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.112433   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.112442   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:18.112469   721   749 D RIL     : radioState:10
10-17 14:46:18.112488   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.112514   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.112519   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:18.112553   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:46:18.112568   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.112583   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.112595   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.112611   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:46:18.112637   721   749 I AT      : AT write start
10-17 14:46:18.112652   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.112682   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.113843   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.113925   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.113985   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.114117   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:18.117162  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:18.119531  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.119671  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:18.119820  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.119899  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.120880   909  6089 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.121063   909  6089 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.122329   909  6089 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.123641  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.123848  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:18.124023  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.124161  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.124636   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.124813   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.125151   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.129379   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:46:18.132985  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.134091   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.134167   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.134267   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.134314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.134491   721   766 I AT      : AT read end: 6
10-17 14:46:18.134537   721   766 D AT      : AT< OK
10-17 14:46:18.134570   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.134627   721   766 I AT      : AT read start
10-17 14:46:18.134706   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.134742   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.134787   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.134863   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cd80 p=0x7f97856cb0 
10-17 14:46:18.134901   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaa00
10-17 14:46:18.134931   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.135055  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:18.135163  1450  1606 D RILJ    : [9520]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:18.144672  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.145267  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.148497  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.148742  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:18.154223  1450  4234 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:18.156278  1450  4234 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:18.181493  1450  1752 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:18.182769  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:46:18.182876  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:46:18.183826  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:46:18.183906  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:46:18.183956  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:18.183989  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:18.184150  1450  1752 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:18.228221  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.229944  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.246347  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.283632  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.283904  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.331074  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.334616  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.335212  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.379040  1450  4234 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.379277  1450  4234 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.382983  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.385200  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.418671  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.421536  1450 23534 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.421619  1450 23534 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.423449  1450  1683 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.423612  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:46:18.451658  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.455130  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.455621  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.475880  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.479508  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.479908  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.505221  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.507164  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.518410  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.521981  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:18.523566  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.523703  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:18.528983   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.529309   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.534786  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.534940  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:18.539213   909  1946 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.539541   909  1946 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.542105  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.542294  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:18.542528  1450  1450 D RILJ    : [9521]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:18.544980   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:18.545084   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cc36c0, pRI=0x7f9784cde0, p=0x7f97856540, pUCI=0x0
10-17 14:46:18.545124   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 dispatched to RIL_CMD_PROXY_3
10-17 14:46:18.545256   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.545286   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.545308   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.545342   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.545352   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.545368   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.545402   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.545411   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.545427   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.545460   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.545469   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.545486   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.545529   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.545554   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.545592   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.545644   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:18.545676   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.545711   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.545707   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.545739   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.545745   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.545779   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.545778   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:18.545807   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.545810   721   749 D RIL     : radioState:10
10-17 14:46:18.545845   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.545853   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:18.545885   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.545886   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:46:18.545919   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.545945   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:46:18.545966   721   749 I AT      : AT write start
10-17 14:46:18.546106   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.546571  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:18.546592   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.546649   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.546702   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.546799   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:18.548277  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.548354  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:18.548435  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.548463  1450  1634 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.548487  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.548588  1450  1634 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.548973   909   923 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.549055   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.549275   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.550028  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.550151  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:18.550798  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.551082  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.551800   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.551924   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.554439   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.554508   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.554582   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.554626   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.554752   721   766 I AT      : AT read end: 6
10-17 14:46:18.554804   721   766 D AT      : AT< OK
10-17 14:46:18.554835   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.554880   721   766 I AT      : AT read start
10-17 14:46:18.554948   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.554979   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.555020   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.555091   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cde0 p=0x7f97856540 
10-17 14:46:18.555153   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:46:18.555179   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.555227  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:18.555319  1450  1606 D RILJ    : [9521]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:18.556190   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.559390  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.559533  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:18.574275  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.577042  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.577560  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.605900  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.607036  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.614884  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.637039  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.637211  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.645719  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.647743  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.648101  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.658181  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.658899  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.663273  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.666461  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.666660  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.967571   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e435a0 
10-17 14:46:18.967647   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e434e0
10-17 14:46:18.967676   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e434f0
10-17 14:46:18.970853   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e435a0 reset to NULL
10-17 14:46:18.970970   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e435a0
10-17 14:46:18.971002   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e435b0
10-17 14:46:20.456228  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:20.459498  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:20.459938  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:20.493430  1450  1683 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:20.494291  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:20.502343  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:20.515652  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:46:20.515964  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:20.538150   721   760 I RILC    : NUMBER:1
10-17 14:46:20.538220   721   760 I RILC    : arg len:14
10-17 14:46:20.538255   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:20.538377   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:20.538450   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978567e0 dispatched to RIL_CMD_PROXY_1
10-17 14:46:20.538575   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:20.538584   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:20.538630   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:20.538626   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:20.538678   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:20.538664   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978567e0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:20.538704   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:20.538728   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:20.538746   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:20.538764   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:20.538771   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:20.538794   721   751 D RIL     : radioState:10
10-17 14:46:20.538811   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:20.538836   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:20.538840   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:20.538884   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:20.538894   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:20.538910   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:20.538926   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:20.538953   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:20.538950   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:20.538983   721   751 I AT      : AT write start
10-17 14:46:20.538983   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:20.539032   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:20.539058   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:20.539132   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:20.539167   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:20.539215   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:20.539240   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:20.539280   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:20.539306   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:20.539351   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:20.539383   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:20.539692   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:20.539774   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:20.539837   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:20.539980   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:20.544782   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:20.544889   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:20.545044   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:20.545085   721   768 I AT      : AT read end: 40
10-17 14:46:20.545115   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:20.545138   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:20.545174   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:20.545189   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:20.545223   721   768 I AT      : AT read start
10-17 14:46:20.545233   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:20.545310   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:20.545359   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:20.545481   721   768 I AT      : AT read end: 6
10-17 14:46:20.545529   721   768 D AT      : AT< OK
10-17 14:46:20.545559   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:20.545606   721   768 I AT      : AT read start
10-17 14:46:20.545685   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:20.545730   721   751 D RIL     : requestQueryThermal success
10-17 14:46:20.545768   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:20.545802   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:20.545848   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:20.545932   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f978567e0 
10-17 14:46:20.545985   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda8a0
10-17 14:46:20.546024   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:20.801562  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:20.804326  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:20.804666  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:20.931711  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:20.979721  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:20.988527  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:20.996058  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:21.029289  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:21.029466  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:21.734808  1450  1450 D RILJ    : [9522]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:21.737265   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:21.737356   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda960, pRI=0x7f9784c360, p=0x7f97856930, pUCI=0x0
10-17 14:46:21.737393   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856930 dispatched to RIL_ATCI_PROXY
10-17 14:46:21.737491   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:21.737502   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:21.737529   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:21.737529   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:21.737559   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:21.737589   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:21.737598   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:21.737634   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:21.737637   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:21.737663   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:21.737705   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:21.737715   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:21.737728   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:21.737772   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:21.737829   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:21.737853   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:21.737860   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:21.737891   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856930 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:21.737895   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:21.737925   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:21.737955   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:21.737949   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:21.737970   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:21.737982   721   753 D RIL     : radioState:10
10-17 14:46:21.737985   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:21.738023   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:21.738028   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:21.738030   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:21.738054   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:21.738078   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:21.738100   721   753 I AT      : AT write start
10-17 14:46:21.738134   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:21.738263   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:21.738320   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:21.738370   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:21.738456   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:21.745961   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:21.746041   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:21.746112   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:21.746155   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:21.746261   721   770 I AT      : AT read end: 6
10-17 14:46:21.746311   721   770 D AT      : AT< OK
10-17 14:46:21.746342   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:21.746391   721   770 I AT      : AT read start
10-17 14:46:21.746462   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:21.746496   721   753 D RIL     : p_response->success = 1
10-17 14:46:21.746522   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:21.746544   721   753 D RIL     : strLength = 6
10-17 14:46:21.746567   721   753 D RIL     : line = <
10-17 14:46:21.746567   721   753 D RIL     : OK
10-17 14:46:21.746567   721   753 D RIL     : >
10-17 14:46:21.746595   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:21.746641   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:21.746720   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97856930 
10-17 14:46:21.746755   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda960
10-17 14:46:21.746787   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:21.746965  1450  1606 D RILJ    : [9522]< OEM_HOOK_RAW [B@bf070f0 [SUB0]
10-17 14:46:22.454849   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185158/0
10-17 14:46:23.035167  1450  1450 D RILJ    : [9523]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:23.038209   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:23.038275   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9100, pRI=0x7f9784c6f0, p=0x7f978569a0, pUCI=0x0
10-17 14:46:23.038309   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978569a0 dispatched to RIL_ATCI_PROXY
10-17 14:46:23.038421   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:23.038469   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:23.038475   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:23.038502   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:23.038502   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978569a0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:23.038538   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:23.038545   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:23.038569   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:23.038573   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:23.038594   721   753 D RIL     : radioState:10
10-17 14:46:23.038636   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:23.038645   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:23.038632   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:23.038679   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:23.038706   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.038733   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:23.038756   721   753 I AT      : AT write start
10-17 14:46:23.038779   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:23.038779   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:23.038809   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:23.038858   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:23.038872   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:23.038882   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:23.038934   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:23.038731   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:23.038979   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:23.039028   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:23.039039   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:23.039053   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:23.039092   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:23.039152   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:23.039208   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:23.039261   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:23.039352   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:23.039428   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:23.039595   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:23.047053   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:23.047163   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:23.047251   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:23.047303   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.047501   721   770 I AT      : AT read end: 6
10-17 14:46:23.047560   721   770 D AT      : AT< OK
10-17 14:46:23.047590   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:23.047642   721   770 I AT      : AT read start
10-17 14:46:23.047737   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.047775   721   753 D RIL     : p_response->success = 1
10-17 14:46:23.047806   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:23.047831   721   753 D RIL     : strLength = 6
10-17 14:46:23.047858   721   753 D RIL     : line = <
10-17 14:46:23.047858   721   753 D RIL     : OK
10-17 14:46:23.047858   721   753 D RIL     : >
10-17 14:46:23.047899   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:23.047956   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.048045   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f978569a0 
10-17 14:46:23.048093   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9100
10-17 14:46:23.048121   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:23.048479  1450  1606 D RILJ    : [9523]< OEM_HOOK_RAW [B@1696669 [SUB0]
10-17 14:46:23.368795   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:46:23.368877   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:23.368950   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:46:23.368991   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.369099   721   765 I AT      : AT read end: 37
10-17 14:46:23.369145   721   765 D AT      : AT< +ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369175   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369213   721   765 D RIL     : Nw URC:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369274   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:23.369309   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:23.369343   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.369400   721   765 I AT      : AT read start
10-17 14:46:23.369654  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:23.369814  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:23.369896  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.370070  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370195  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.370253  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.370287  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370328  1450  1450 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.370358  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370455  1450  1450 D GsmSST  : [GsmSST0] notifySignalStrength: mSignalStrength.getLevel=4
10-17 14:46:23.370721  1450  1450 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1 sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad}
10-17 14:46:23.371318   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: subId=1 signalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.371410   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: logSSC.length=5 next=2
10-17 14:46:23.371809   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372225   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372601   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372938   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.373265   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.373337   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: ----------------
10-17 14:46:23.374388   909   920 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:23.374472   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: valid phoneId=0
10-17 14:46:23.374518   909   920 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:23.374658   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.374767   909   920 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:23.374916   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.375166   909   920 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:23.375408   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375551   909   920 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.375575  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375604   909   920 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.375634   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375665  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.375673   909   920 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.375703   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375707  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.375738  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375776  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.375801  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375901  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375946  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:23.376038  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376101  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.376140  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.376169  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376206  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:23.376231  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376311  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376372  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.376418  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.376446  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376482  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.376508  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376536  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376577  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.376921  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376990  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.377040  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.377068  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.377112  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.377140  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.377933  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:23.843563  1450  1450 D RILJ    : [9524]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:23.845473   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:23.845560   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaaa0, pRI=0x7f9784c870, p=0x7f97856ee0, pUCI=0x0
10-17 14:46:23.845597   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c870 p=0x7f97856ee0 dispatched to RIL_ATCI_PROXY
10-17 14:46:23.845699   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:23.845702   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:23.845704   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:23.845736   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:23.845743   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:23.845778   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:23.845785   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:23.845789   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:23.845802   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:23.845828   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:23.845859   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:23.845861   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:23.845890   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:23.845929   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:23.845983   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:23.846011   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:23.846053   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:23.846075   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:23.846104   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:23.846150   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:23.846154   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:23.846210   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:23.846245   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c870 p=0x7f97856ee0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:23.846264   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:23.846276   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:23.846309   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:23.846333   721   753 D RIL     : radioState:10
10-17 14:46:23.846374   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:23.846404   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.846433   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:23.846457   721   753 I AT      : AT write start
10-17 14:46:23.846569   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:23.846604   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:23.846655   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:23.846703   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:23.846784   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:23.854391   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:23.854472   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:23.854544   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:23.854586   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.854704   721   770 I AT      : AT read end: 6
10-17 14:46:23.854746   721   770 D AT      : AT< OK
10-17 14:46:23.854776   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:23.854816   721   770 I AT      : AT read start
10-17 14:46:23.854854   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.854889   721   753 D RIL     : p_response->success = 1
10-17 14:46:23.854917   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:23.854942   721   753 D RIL     : strLength = 6
10-17 14:46:23.854965   721   753 D RIL     : line = <
10-17 14:46:23.854965   721   753 D RIL     : OK
10-17 14:46:23.854965   721   753 D RIL     : >
10-17 14:46:23.854992   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:23.855038   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.855112   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c870 p=0x7f97856ee0 
10-17 14:46:23.855144   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:46:23.855177   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:23.855373  1450  1606 D RILJ    : [9524]< OEM_HOOK_RAW [B@54ac8ee [SUB0]
10-17 14:46:24.292306  1450  1450 D RILJ    : [9525]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:24.295293   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:24.295415   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9140, pRI=0x7f9784c210, p=0x7f97856fc0, pUCI=0x0
10-17 14:46:24.295451   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856fc0 dispatched to RIL_ATCI_PROXY
10-17 14:46:24.295566   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.295582   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:24.295583   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.295608   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.295640   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.295644   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.295650   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:24.295685   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.295690   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.295692   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.295723   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.295761   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.295775   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.295785   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.295824   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:24.295844   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.295860   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856fc0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:24.295864   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.295875   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.295896   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.295916   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.295917   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.295935   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:24.295947   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.295962   721   753 D RIL     : radioState:10
10-17 14:46:24.295981   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.296009   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:24.296046   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:24.296071   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:24.296093   721   753 I AT      : AT write start
10-17 14:46:24.296233   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.296284   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.296287   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.296348   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.296404   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:24.296492   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:24.304107   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:24.304197   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:24.304271   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:24.304314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.304445   721   770 I AT      : AT read end: 6
10-17 14:46:24.304487   721   770 D AT      : AT< OK
10-17 14:46:24.304515   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:24.304566   721   770 I AT      : AT read start
10-17 14:46:24.304795   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:24.304865   721   753 D RIL     : p_response->success = 1
10-17 14:46:24.304896   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:24.304921   721   753 D RIL     : strLength = 6
10-17 14:46:24.304948   721   753 D RIL     : line = <
10-17 14:46:24.304948   721   753 D RIL     : OK
10-17 14:46:24.304948   721   753 D RIL     : >
10-17 14:46:24.304977   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:24.305027   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:24.305125   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f97856fc0 
10-17 14:46:24.305162   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9140
10-17 14:46:24.305191   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.305472  1450  1606 D RILJ    : [9525]< OEM_HOOK_RAW [B@24418f [SUB0]
10-17 14:46:24.624216  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:24.626443  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:46:24.626621  1450  1450 D RILJ    : [9526]> SCREEN_STATE: false [SUB0]
10-17 14:46:24.629158  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:24.629966  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:46:24.630009   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:24.630083   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6a60, pRI=0x7f9784c240, p=0x7f978570a0, pUCI=0x0
10-17 14:46:24.630121   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c240 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:24.630152  1450  1450 D RILJ    : [9527]> SCREEN_STATE: false [SUB1]
10-17 14:46:24.630284   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.630309   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.630324   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.630366   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.630373   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.630375   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.630394   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.630425   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.630433   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.630437   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.630465   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.630511   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.630662   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:24.630705   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:24.630740   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c240 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:24.630776   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.630821   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:24.630852   721   749 D RIL     : radioState:10
10-17 14:46:24.630998   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.631054   721   749 D AT      : AT> AT+CREG=1
10-17 14:46:24.631084   721   749 I AT      : AT write start
10-17 14:46:24.631074   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.631407   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.631479   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.631591   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.631638   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.631703   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.631763   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.631899   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:24.632026   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.632083   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.632144   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.632179   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.632294   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.632378   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.634070   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:24.634153   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cc3ee0, pRI=0x7f9784c7b0, p=0x7f97857110, pUCI=0x0
10-17 14:46:24.634186   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c7b0 p=0x7f97857110 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:24.634307   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.634346   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.634383   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.634392   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.634411   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.634450   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.634454   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.634479   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.634515   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.634603   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.634633   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.634705   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.634739   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.634785   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:24.634832   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c7b0 p=0x7f97857110 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:24.634865   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.634896   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:24.634922   721   755 D RIL     : radioState:0
10-17 14:46:24.634970   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.634997   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.635022   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.635089   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.635118   721   755 D AT      : AT> AT+CREG=1
10-17 14:46:24.635141   721   755 I AT      : AT write start
10-17 14:46:24.635212   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.635255   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.635303   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.635338   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.635390   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.635402   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.635417   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.635459   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.635516   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.635602   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:24.635711   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.635746   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.639541   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.639642   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.639721   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.639768   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.640249   721   766 I AT      : AT read end: 6
10-17 14:46:24.640334   721   766 D AT      : AT< OK
10-17 14:46:24.640372   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.640419   721   766 I AT      : AT read start
10-17 14:46:24.640652   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.640721   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.640802   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.640849   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.641074   721   772 I AT      : AT read end: 6
10-17 14:46:24.641149   721   772 D AT      : AT< OK
10-17 14:46:24.641182   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.641231   721   772 I AT      : AT read start
10-17 14:46:24.640497   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.641332   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.641363   721   749 D AT      : AT> AT+CGREG=1
10-17 14:46:24.641386   721   749 I AT      : AT write start
10-17 14:46:24.641568   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.641649   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.641705   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.641805   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:24.642448   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.642553   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.642595   721   755 D AT      : AT> AT+CGREG=1
10-17 14:46:24.642621   721   755 I AT      : AT write start
10-17 14:46:24.642820   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.642883   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.642933   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.643015   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:24.643360   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.643432   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.643500   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.643542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.643645   721   766 I AT      : AT read end: 6
10-17 14:46:24.643697   721   766 D AT      : AT< OK
10-17 14:46:24.643725   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.643763   721   766 I AT      : AT read start
10-17 14:46:24.643804   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.643846   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.643871   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:46:24.643893   721   749 I AT      : AT write start
10-17 14:46:24.644030   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.644084   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.644131   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.644281   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:24.644361   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.644407   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.644468   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.644510   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.644604   721   772 I AT      : AT read end: 6
10-17 14:46:24.644644   721   772 D AT      : AT< OK
10-17 14:46:24.644673   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.644711   721   772 I AT      : AT read start
10-17 14:46:24.644748   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.644793   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.644827   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:46:24.644851   721   755 I AT      : AT write start
10-17 14:46:24.644983   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.645048   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.645097   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.645174   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:24.645441   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.645507   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.645571   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.645611   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.645721   721   766 I AT      : AT read end: 6
10-17 14:46:24.645761   721   766 D AT      : AT< OK
10-17 14:46:24.645790   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.645830   721   766 I AT      : AT read start
10-17 14:46:24.645870   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.645907   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.645947   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:46:24.645971   721   749 I AT      : AT write start
10-17 14:46:24.646090   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.646139   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.646185   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.646362   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:24.646438   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.646482   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.646542   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.646581   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.646679   721   772 I AT      : AT read end: 6
10-17 14:46:24.646718   721   772 D AT      : AT< OK
10-17 14:46:24.646748   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.646786   721   772 I AT      : AT read start
10-17 14:46:24.646836   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.646877   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.646904   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:46:24.646927   721   755 I AT      : AT write start
10-17 14:46:24.647085   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.647149   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.647198   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.647499   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.647551   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.647612   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.647650   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.647958   721   766 I AT      : AT read end: 6
10-17 14:46:24.648017   721   766 D AT      : AT< OK
10-17 14:46:24.648045   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.648080   721   766 I AT      : AT read start
10-17 14:46:24.648121   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.648169   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.648197   721   749 D AT      : AT> AT+CEREG=1
10-17 14:46:24.648220   721   749 I AT      : AT write start
10-17 14:46:24.648350   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.648407   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.651176   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:24.651268   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.651343   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:24.658387   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.658465   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.658533   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.658576   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.658693   721   772 I AT      : AT read end: 6
10-17 14:46:24.658736   721   772 D AT      : AT< OK
10-17 14:46:24.658791   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.658840   721   772 I AT      : AT read start
10-17 14:46:24.658874   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.658926   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.658954   721   755 D AT      : AT> AT+CEREG=1
10-17 14:46:24.658945   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.658983   721   755 I AT      : AT write start
10-17 14:46:24.659001   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.659058   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.659098   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.659112   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.659154   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.659179   721   766 I AT      : AT read end: 6
10-17 14:46:24.659197   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.659208   721   766 D AT      : AT< OK
10-17 14:46:24.659235   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.659270   721   766 I AT      : AT read start
10-17 14:46:24.659274   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:24.659309   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.659354   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:24.659395   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:24.659461   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f978570a0 
10-17 14:46:24.659492   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a60
10-17 14:46:24.659516   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:24.659629  1450  1606 D RILJ    : [9526]< SCREEN_STATE  [SUB0]
10-17 14:46:24.660341   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.660411   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.660483   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.660527   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.660643   721   772 I AT      : AT read end: 6
10-17 14:46:24.660694   721   772 D AT      : AT< OK
10-17 14:46:24.660725   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.660772   721   772 I AT      : AT read start
10-17 14:46:24.660810   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.660849   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:24.660889   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:24.661366   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97857110 
10-17 14:46:24.661407   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:46:24.661433   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.661517  1450  1609 D RILJ    : [9527]< SCREEN_STATE  [SUB1]
10-17 14:46:25.083759  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.086306  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.086662  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.124822  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.125307  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.128517  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.147066  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.151630  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.249932  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.254609  1450  4234 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.254959  1450  4234 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.272597  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:25.274609  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.274679  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:25.294463  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.295940  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.296576   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.296678  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.296866   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.297792  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.297897  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:25.299468   909  6090 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.299741   909  6090 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.300538  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:25.302054  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:46:25.302204  1450  1450 D RILJ    : [9528]> SCREEN_STATE: true [SUB0]
10-17 14:46:25.304649  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:25.304995   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:25.305087   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6160, pRI=0x7f9784cb10, p=0x7f978571f0, pUCI=0x0
10-17 14:46:25.305126   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb10 p=0x7f978571f0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.305257   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.305298   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.305326   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.305340   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.305358   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.305396   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.305408   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.305423   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.305467   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.305473   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.305494   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.305562   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.305606   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.305608   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.305646   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.305688   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.305714   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.305821   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.305861   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.305897   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb10 p=0x7f978571f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.305933   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.305931   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.305962   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.305969   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:25.305995   721   749 D RIL     : radioState:10
10-17 14:46:25.306004   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.306030   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.306056   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.306066   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.306084   721   749 D AT      : AT> AT+CREG=3
10-17 14:46:25.306110   721   749 I AT      : AT write start
10-17 14:46:25.306366  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:46:25.306489  1450  1450 D RILJ    : [9529]> SCREEN_STATE: true [SUB1]
10-17 14:46:25.306719   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.306786   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.306839   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.306931   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.309181  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.309371  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:25.309514  1450  1450 D RILJ    : [9530]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:25.311735   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:25.311831   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9240, pRI=0x7f9784c150, p=0x7f97857340, pUCI=0x0
10-17 14:46:25.311866   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857340 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.311982   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.312020   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.312064   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.312078   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.312090   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.312130   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.312151   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.312166   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.312209   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.312249   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.312253   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.312282   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.312284   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.312325   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857340 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.312358   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.312389   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:25.312415   721   755 D RIL     : radioState:0
10-17 14:46:25.312460   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312487   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312513   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312566   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.312594   721   755 D AT      : AT> AT+CREG=3
10-17 14:46:25.312620   721   755 I AT      : AT write start
10-17 14:46:25.312730   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.312762   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.312805   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.312830   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.312880   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.312905   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.313035   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.313102   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.313154   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.313247   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:25.313427   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.313469   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.313519   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.314582   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:46:25.314655   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:25.314761   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:46:25.314808   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.314860   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.314902   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.314954   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.314995   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.315144   721   765 I AT      : AT read end: 36
10-17 14:46:25.315194   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315224   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315270   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315311   721   765 D RIL     : NW state changed: normal case
10-17 14:46:25.315341   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:46:25.315372   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.315400   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:46:25.315455   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:46:25.315494   721   765 D RIL     : bCREGType3Support=1
10-17 14:46:25.315523   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:25.315548   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:46:25.315772   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:25.315850   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.315916   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e436c0
10-17 14:46:25.315955   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e436d0
10-17 14:46:25.316032   721   765 I AT      : AT read start
10-17 14:46:25.316158   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:46:25.316171  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:46:25.316222   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:46:25.316302   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:46:25.316347   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.316406   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.316448   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.316504   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.316541   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.316674   721   771 I AT      : AT read end: 36
10-17 14:46:25.316718   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316751   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316794   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316829   721   771 D RIL     : NW state changed: normal case
10-17 14:46:25.316858   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:46:25.316888   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:46:25.316916   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:46:25.316970   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:46:25.317005   721   771 D RIL     : bCREGType3Support=1
10-17 14:46:25.317036   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:25.317061   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:46:25.317139   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:25.317167   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.317224   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e436c0, cancel
10-17 14:46:25.317257   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43660
10-17 14:46:25.317292   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43670
10-17 14:46:25.317349   721   771 I AT      : AT read start
10-17 14:46:25.317420   721   772 I AT      : AT read end: 6
10-17 14:46:25.317446   721   772 D AT      : AT< OK
10-17 14:46:25.317473   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.317509   721   772 I AT      : AT read start
10-17 14:46:25.318867   721   766 I AT      : AT read end: 6
10-17 14:46:25.318936   721   766 D AT      : AT< OK
10-17 14:46:25.318966   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.319011   721   766 I AT      : AT read start
10-17 14:46:25.319062   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.319123   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.319150   721   749 D AT      : AT> AT+CGREG=3
10-17 14:46:25.319175   721   749 I AT      : AT write start
10-17 14:46:25.319358   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.319419   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.319470   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.319577   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.320460  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:46:25.321053   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.321155   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.321186   721   755 D AT      : AT> AT+CGREG=3
10-17 14:46:25.321212   721   755 I AT      : AT write start
10-17 14:46:25.321395   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.321458   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.321511   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.321613   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:25.321950  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:25.322072  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:46:25.322230  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:25.322855   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:25.322938   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cf9360, pRI=0x7f9784c540, p=0x7f978573b0, pUCI=0x0
10-17 14:46:25.322974   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.323078   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.323112   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.323146   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.323156   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.323174   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.323220   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.323217   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.323248   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.323454   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.323519   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.323544   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.323593   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.323619   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.323689   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.323715   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.323756   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.323769   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.323827   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.323854   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.324087   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.325979  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:46:25.326151  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:46:25.326304  1450  1450 D RILJ    : [9531]> OPERATOR [SUB0]
10-17 14:46:25.329184   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.329271   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.329352   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.329394   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.329444   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.329484   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.329539   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.329580   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.329720   721   766 I AT      : AT read end: 6
10-17 14:46:25.329720   721   772 I AT      : AT read end: 6
10-17 14:46:25.329782   721   766 D AT      : AT< OK
10-17 14:46:25.329783   721   772 D AT      : AT< OK
10-17 14:46:25.329816   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.329816   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.329872   721   772 I AT      : AT read start
10-17 14:46:25.329883   721   766 I AT      : AT read start
10-17 14:46:25.329971   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.329995   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.330009   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.330036   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:46:25.330036   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.330063   721   755 I AT      : AT write start
10-17 14:46:25.330066   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:46:25.330093   721   749 I AT      : AT write start
10-17 14:46:25.331096   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.331198   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.331258   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.331270   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.331316   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.331343   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:25.331593   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.331764   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.332213  1450  1450 D RILJ    : [9532]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:46:25.332634   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:46:25.332735   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9340, pRI=0x7f9784c660, p=0x7f97857490, pUCI=0x0
10-17 14:46:25.332778   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.332811   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.332851   721   760 D RILC-MTK: Request pRI=0x7f9784c660 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:46:25.335003  1450  1450 D RILJ    : [9533]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:46:25.335418   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:25.335492   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9b80, pRI=0x7f9784cb40, p=0x7f97857570, pUCI=0x0
10-17 14:46:25.335530   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.335560   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.335596   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.335629   721   760 D RILC-MTK: Request pRI=0x7f9784cb40 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:46:25.339199   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.339297   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.339491   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.339542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.339548   721   772 I AT      : AT read end: 6
10-17 14:46:25.339593   721   772 D AT      : AT< OK
10-17 14:46:25.339595   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.339630   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.339641   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.339679   721   772 I AT      : AT read start
10-17 14:46:25.339702   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.339735   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.339746   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.339784   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.339826   721   755 D AT      : AT> AT+ECSQ
10-17 14:46:25.339853   721   755 I AT      : AT write start
10-17 14:46:25.339986   721   766 I AT      : AT read end: 6
10-17 14:46:25.340016   721   766 D AT      : AT< OK
10-17 14:46:25.340015   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.340048   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.340064   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.340088   721   766 I AT      : AT read start
10-17 14:46:25.340110   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.340132   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.340179   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.340205   721   749 D AT      : AT> AT+ECSQ
10-17 14:46:25.340206   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:46:25.340233   721   749 I AT      : AT write start
10-17 14:46:25.340381   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.340436   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.340486   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.340581   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:46:25.340750   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:25.340818   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9c20, pRI=0x7f9784cb70, p=0x7f97857730, pUCI=0x0
10-17 14:46:25.340854   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.340884   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.341036   721   760 D RILC-MTK: 3:DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.341067   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.341099   721   760 D RILC-MTK: Request pRI=0x7f9784cb70 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:46:25.341540  1450  1450 D RILJ    : [9534]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:46:25.342403   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:46:25.342493   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.342567   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:46:25.342609   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.342656   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.342699   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.342744   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.342781   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.342892   721   772 I AT      : AT read end: 42
10-17 14:46:25.342939   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:25.342972   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:25.343006   721   772 D AT      : AT< OK
10-17 14:46:25.343031   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.343077   721   772 I AT      : AT read start
10-17 14:46:25.343138   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.343193   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:46:25.343228   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:46:25.343269   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.343296   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:46:25.343319   721   755 I AT      : AT write start
10-17 14:46:25.343485   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.343488   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:46:25.343550   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.343556   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.343604   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.343625   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:46:25.343667   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.343686   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:25.343717   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.343757   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.343802   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.343839   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.343954   721   766 I AT      : AT read end: 43
10-17 14:46:25.343995   721   766 D AT      : AT< +ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:25.344025   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:25.344061   721   766 D AT      : AT< OK
10-17 14:46:25.344094   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.344139   721   766 I AT      : AT read start
10-17 14:46:25.344544   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.344586  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.344702  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:25.344713   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:25.344782  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:46:25.344786   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:25.344833   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.344856  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:25.344911  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:46:25.344912   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.344946   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:46:25.344971   721   749 I AT      : AT write start
10-17 14:46:25.345163   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.345240   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.345241   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:25.345307   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9c40, pRI=0x7f9784cc60, p=0x7f978578f0, pUCI=0x0
10-17 14:46:25.345320   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.345343   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345362   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.345376   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345406   721   760 D RILC-MTK: 3:DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345434   721   760 D RILC-MTK: 4:VOICE_REGISTRATION_STATE pRI=0x7f9784cb70 p=0x7f97857730 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345464   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.345459   721   772 I AT      : AT read end: 6
10-17 14:46:25.345500   721   772 D AT      : AT< OK
10-17 14:46:25.345500   721   760 D RILC-MTK: Request pRI=0x7f9784cc60 to RIL_CMD_PROXY_3 is busy. total:5 requests pending
10-17 14:46:25.345533   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.345574   721   772 I AT      : AT read start
10-17 14:46:25.345639   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.345689   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.345739   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.345828   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:25.345912   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.345968   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.345995   721   755 D AT      : AT> AT+CEREG=3
10-17 14:46:25.346019   721   755 I AT      : AT write start
10-17 14:46:25.346334   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.346410   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.346465   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.346556   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:25.346653  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.346750  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.346866  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:46:25.346923  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:46:25.347050  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:25.347110  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:46:25.347185  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:46:25.347220  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:46:25.347253  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:46:25.347290  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:46:25.347323  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:25.347453  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:25.347477   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.347540   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.347579  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:46:25.347626   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.347648  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:46:25.347668   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.347696  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:46:25.347825   721   766 I AT      : AT read end: 6
10-17 14:46:25.347865   721   766 D AT      : AT< OK
10-17 14:46:25.347894   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.347940   721   766 I AT      : AT read start
10-17 14:46:25.347941   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.347995   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.348060   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.348101   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.348193   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.348257   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.348264  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:46:25.348285   721   749 D AT      : AT> AT+CEREG=3
10-17 14:46:25.348308   721   749 I AT      : AT write start
10-17 14:46:25.348459   721   772 I AT      : AT read end: 6
10-17 14:46:25.348498   721   772 D AT      : AT< OK
10-17 14:46:25.348493   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.348536   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.348549   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.348580   721   772 I AT      : AT read start
10-17 14:46:25.348608   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.348698   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.348781   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.348822   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.348866   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.348951   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f97857340 
10-17 14:46:25.348987   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:46:25.349019   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.349264  1450  1609 D RILJ    : [9529]< SCREEN_STATE  [SUB1]
10-17 14:46:25.350731   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.350794   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.350875   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.351140   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.351139   721   766 I AT      : AT read end: 6
10-17 14:46:25.351191   721   766 D AT      : AT< OK
10-17 14:46:25.351222   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.351274   721   766 I AT      : AT read start
10-17 14:46:25.351318   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.351360   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.351402   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.351479   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f978571f0 
10-17 14:46:25.351511   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6160
10-17 14:46:25.351547   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.351580   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.351612   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.351641   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:25.351665   721   749 D RIL     : radioState:10
10-17 14:46:25.351680  1450  1606 D RILJ    : [9528]< SCREEN_STATE  [SUB0]
10-17 14:46:25.351706   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:25.351743   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:46:25.351774   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.351800   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:46:25.351827   721   749 I AT      : AT write start
10-17 14:46:25.352053   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.352128   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.352181   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.352270   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.352637  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.352763  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.352824  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:46:25.353211   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.353288   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.353356   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.353398   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.353663   721   766 I AT      : AT read end: 6
10-17 14:46:25.353723   721   766 D AT      : AT< OK
10-17 14:46:25.353756   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.353807   721   766 I AT      : AT read start
10-17 14:46:25.353867   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.353908   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.353958   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.354002  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:46:25.354045   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c540 p=0x7f978573b0 
10-17 14:46:25.354083   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9360
10-17 14:46:25.354113   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.354145   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784c660 p=0x7f97857490 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.354161  1450  1450 D RILJ    : [9535]> OPERATOR [SUB1]
10-17 14:46:25.354174   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.354167  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:25.354208   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:25.354233   721   749 D RIL     : radioState:10
10-17 14:46:25.354243  1450  1606 D RILJ    : [9530]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:25.354270   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.354304   721   749 D AT      : AT> AT+COPS?
10-17 14:46:25.354331   721   749 I AT      : AT write start
10-17 14:46:25.355882   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.355944   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.355995   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.356088   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.356755   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:46:25.356832   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9c60, pRI=0x7f9784ce10, p=0x7f97857dc0, pUCI=0x0
10-17 14:46:25.356866   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784ce10 p=0x7f97857dc0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.356985   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.357021   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.357066   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.357072   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.357097   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.357143   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.357150   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.357171   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.357216   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.357206   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.357245   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.357281   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.357334   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.357359   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.357402   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.357428   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.357467   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.357484   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.357528   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.357559   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.357592   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784ce10 p=0x7f97857dc0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.357621   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.357652   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:25.357679   721   755 D RIL     : radioState:0
10-17 14:46:25.357719   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357748   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357773   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357799   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357834   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.357861   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.357905   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.357964   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce10 p=0x7f97857dc0 
10-17 14:46:25.357996   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c60
10-17 14:46:25.358023   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.358072   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.358126   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.358536  1450  1609 D RilRequest: [9535]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.361113  1450  1450 D RILJ    : [9536]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:46:25.363976   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:25.364063   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.364145   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:25.364191   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.364244   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.364297   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.364348   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.364387   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.364534   721   766 I AT      : AT read end: 30
10-17 14:46:25.364601   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:25.364636   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:25.364672   721   766 D AT      : AT< OK
10-17 14:46:25.364705   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.364749   721   766 I AT      : AT read start
10-17 14:46:25.365382   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.365480   721   749 D RIL     : Get operator code 25020
10-17 14:46:25.365517   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:46:25.365557   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:46:25.365587   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.365650   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.365733   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c660 p=0x7f97857490 
10-17 14:46:25.365781   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:46:25.365824   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.365860   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.365893   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.365925   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.365952   721   749 D RIL     : radioState:10
10-17 14:46:25.366003   721   749 D RIL     : request gprs reg state: normal case
10-17 14:46:25.366002  1450  1606 D RILJ    : [9531]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:46:25.366046   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.366075   721   749 D AT      : AT> AT+CGREG?
10-17 14:46:25.366099   721   749 I AT      : AT write start
10-17 14:46:25.366287   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.366358   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.366412   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.366502   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.374140   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:46:25.374235   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.374309   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:46:25.374356   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.374462   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.374488   721   766 I AT      : AT read end: 44
10-17 14:46:25.374514   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.374534   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:25.374565   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:25.374577   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.374604   721   766 I AT      : AT read start
10-17 14:46:25.374617   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.374691   721   766 I AT      : AT read end: 6
10-17 14:46:25.374719   721   766 D AT      : AT< OK
10-17 14:46:25.374746   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.374784   721   766 I AT      : AT read start
10-17 14:46:25.374848   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.374911   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.374941   721   749 E RIL     : The value in the field <lac> :0
10-17 14:46:25.374968   721   749 D RIL     : cid: 3583
10-17 14:46:25.374993   721   749 E RIL     : The value of act: 3
10-17 14:46:25.375017   721   749 D RIL     : cause_type: 0
10-17 14:46:25.375041   721   749 D RIL     : reject_cause: 0
10-17 14:46:25.375078   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.375104   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:46:25.375127   721   749 I AT      : AT write start
10-17 14:46:25.375273   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.375334   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.375387   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.375476   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:46:25.377114   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:46:25.377198   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.377270   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:46:25.377314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.377526   721   766 I AT      : AT read end: 19
10-17 14:46:25.377584   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:46:25.377618   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:46:25.377651   721   766 I AT      : AT read start
10-17 14:46:25.377767   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.377830   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.377901   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.377942   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.378103   721   766 I AT      : AT read end: 6
10-17 14:46:25.378148   721   766 D AT      : AT< OK
10-17 14:46:25.378177   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.378222   721   766 I AT      : AT read start
10-17 14:46:25.378378   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.378453   721   749 E RIL     : rid: 0
10-17 14:46:25.378484   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:25.378515   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:25.378543   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:25.378568   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:25.378598   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.378656   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.378732   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb40 p=0x7f97857570 
10-17 14:46:25.378771   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:46:25.378802   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.378833   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cb70 p=0x7f97857730 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.378861   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.378888   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.378915   721   749 D RIL     : radioState:10
10-17 14:46:25.378951   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.378979   721   749 D AT      : AT> AT+CREG?
10-17 14:46:25.378959  1450  1606 D RILJ    : [9532]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:46:25.379001   721   749 I AT      : AT write start
10-17 14:46:25.379186   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.379256   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.379310   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.379398   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.380112   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:46:25.380189   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.380271   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:46:25.380321   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.380431   721   766 I AT      : AT read end: 38
10-17 14:46:25.380475   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.380510   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.380544   721   766 I AT      : AT read start
10-17 14:46:25.380747   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.380809   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.380877   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.380990   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.381126   721   766 I AT      : AT read end: 6
10-17 14:46:25.381177   721   766 D AT      : AT< OK
10-17 14:46:25.381208   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.381248   721   766 I AT      : AT read start
10-17 14:46:25.381361   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.381422   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.381453   721   749 E RIL     : The value in the field <lac> :127
10-17 14:46:25.381480   721   749 D RIL     : cid: 3583
10-17 14:46:25.381506   721   749 E RIL     : The value of act: 3
10-17 14:46:25.381531   721   749 D RIL     : cause_type: 0
10-17 14:46:25.381556   721   749 D RIL     : reject_cause: 0
10-17 14:46:25.381610   721   749 E RIL     : rid: 0
10-17 14:46:25.381637   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:25.381670   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:25.381699   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:25.381725   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:25.381756   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.381790   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.381852   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.381938   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb70 p=0x7f97857730 
10-17 14:46:25.381971   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c20
10-17 14:46:25.382001   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.382032   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cc60 p=0x7f978578f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.382063   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.382092   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:25.382117   721   749 D RIL     : radioState:10
10-17 14:46:25.382154   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.382185   721   749 D AT      : AT> AT+COPS?
10-17 14:46:25.382181  1450  1606 D RILJ    : [9533]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:46:25.382214   721   749 I AT      : AT write start
10-17 14:46:25.382411   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.382484   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.382538   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.382633   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.384247   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:25.384333   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.384408   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:25.384452   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.384572   721   766 I AT      : AT read end: 24
10-17 14:46:25.384649   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:25.384747   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:25.384770   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.384790   721   766 I AT      : AT read start
10-17 14:46:25.384819   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.384883   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.384923   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.385011   721   766 I AT      : AT read end: 6
10-17 14:46:25.385041   721   766 D AT      : AT< OK
10-17 14:46:25.385068   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.385106   721   766 I AT      : AT read start
10-17 14:46:25.385156   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.385201   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.385247   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.385320   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc60 p=0x7f978578f0 
10-17 14:46:25.385360   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c40
10-17 14:46:25.385390   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.385478  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:46:25.385543  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:46:25.385622  1450  1606 D RILJ    : [9534]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:46:25.395330  1450  1450 D RILJ    : [9537]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:46:25.395532   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:25.395627   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9cc0, pRI=0x7f9784ce40, p=0x7f97856540, pUCI=0x0
10-17 14:46:25.395668   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856540 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.395772   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.395822   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.395862   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.395875   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.395875   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.395891   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.395931   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.395936   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.395962   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.395993   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.396028   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.396039   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.396074   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.396095   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.396110   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.396206   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.396236   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.396281   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.396330   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.396373   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.396425   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.396460   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.396500   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856540 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.396531   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.396563   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.396593   721   755 D RIL     : radioState:0
10-17 14:46:25.396642   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396669   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396696   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396722   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396756   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.396804   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.396854   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.396924   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce40 p=0x7f97856540 
10-17 14:46:25.396958   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9cc0
10-17 14:46:25.396985   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.397039   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.397071   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.397193  1450  1450 D RILJ    : [9538]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:46:25.397192  1450  1609 D RilRequest: [9536]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.397236  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.397639   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:25.397747   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9ce0, pRI=0x7f9784c240, p=0x7f97856cb0, pUCI=0x0
10-17 14:46:25.397788   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97856cb0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.397949   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.397950   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.397990   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.398040   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.398027   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.398030   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.398076   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.398117   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.398116   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.398148   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.398198   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.398212   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.398233   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.398248   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97856cb0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.398281   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.398288   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.398310   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.398327   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.398347   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.398354   721   755 D RIL     : radioState:0
10-17 14:46:25.398399   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398408   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.398439   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398447   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.398472   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398488   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.398500   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398547   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.398576   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.398623   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.398681   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97856cb0 
10-17 14:46:25.398718   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9ce0
10-17 14:46:25.398744   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.398795   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.398822   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.398861   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.398904   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.398930   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.399541  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.399895  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.402599  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.402796  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:25.403307  1450  1609 D RilRequest: [9537]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.404493   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:25.404596   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cc36c0, pRI=0x7f9784c4b0, p=0x7f97856e70, pUCI=0x0
10-17 14:46:25.404640   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c4b0 p=0x7f97856e70 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.404765   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.404822   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.404858   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.404868   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.404900   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.404957   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.404996   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.405023   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.405073   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.405100   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.405139   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.405168   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.405212   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.405219   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.405238   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.405282   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.405289   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.405311   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.405358   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.405363   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.405415   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.405441   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.405618   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.405690   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.405729   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c4b0 p=0x7f97856e70 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.405761   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.405795   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:25.405822   721   755 D RIL     : radioState:0
10-17 14:46:25.405863   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.405894   721   755 D AT      : AT> AT+COPS?
10-17 14:46:25.405918   721   755 I AT      : AT write start
10-17 14:46:25.406124   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.406205   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.406260   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.406356   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:46:25.406720  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:25.406876  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:25.406973  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:25.407015  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.407106  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:25.407155  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:46:25.407195  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.407251  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:25.407384  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:25.407434  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:25.408914  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.409013  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:46:25.409107  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:46:25.409153  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:46:25.413395  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.413501  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:46:25.413590  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:46:25.413640  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:46:25.413731  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:46:25.413786  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:46:25.414011   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:46:25.414096   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.414182   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:46:25.414247   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.414369   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.414400   721   772 I AT      : AT read end: 12
10-17 14:46:25.414431   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.414453   721   772 D AT      : AT< +COPS: 0
10-17 14:46:25.414490   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:46:25.414500   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.414534   721   772 I AT      : AT read start
10-17 14:46:25.414542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.414633   721   772 I AT      : AT read end: 6
10-17 14:46:25.414663   721   772 D AT      : AT< OK
10-17 14:46:25.414692   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.414735   721   772 I AT      : AT read start
10-17 14:46:25.414799   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.414859   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.414919   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.415007   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f97856e70 
10-17 14:46:25.415058   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:46:25.415092   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.415186  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:46:25.415281  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:46:25.415365  1450  1609 D RILJ    : [9538]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:46:25.415468  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:46:25.415555  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:46:25.415661  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:46:25.423046  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.423194  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:46:25.423257  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:46:25.423386  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:46:25.423469  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:46:25.423513  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:25.423575  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:46:25.423610  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.423685  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:25.423763  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:46:25.423831  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:46:25.423914  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:46:25.423945  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:46:25.424104  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:46:25.424147  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:46:25.424189  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.424265  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:25.424317  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:46:25.426489  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:46:25.426617  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:46:25.426664  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:25.426798  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:25.426939  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:46:25.427372  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:25.427470  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:25.427543  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:46:25.427597  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:46:25.427737  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:25.427782  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:25.427842  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:46:25.427909  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.427958  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428002  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428054  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428097  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428142  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428183  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428224  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428266  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428309  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428353  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:46:25.428390  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:46:25.428439  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:46:25.428498  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:46:25.429920  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:46:25.431433  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.431636  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:46:25.432533  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:46:25.433569  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:46:25.433
10-17 14:46:25.433791  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:46:25.434755  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.435054  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.435182  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:46:25.435261  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:46:25.435323  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.435648  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:46:25.436536   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.436674   909  1190 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.436858   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=3
10-17 14:46:25.437252   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.437720   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.438228   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.438679   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439102   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144625Europe/Samara(1,290,14400,0,1476701185) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439205   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:46:25.439269   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.439427   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439568   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.439760   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440049   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.440240   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440504   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.440718   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440855   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.441103   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.442599   909  1190 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.443555  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.443729  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:25.443794  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:25.443837  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.443886  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:25.443915  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.447233  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.447612   909  1190 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.456103  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:46:25.456179  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.456267  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:46:25.456343  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.456378  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.456438  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:25.456473  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.456505  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.456676  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.456740  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:25.456950  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.457036  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.457746   909  7315 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.457894   909  7315 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.458308   909  7315 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.459956  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.460118  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:25.460296  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.460401  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.460982   909  1631 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.461070   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.461381   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.464317  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:25.464417  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.464456  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.464596  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:46:25.467030  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.469357  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.469558  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:25.478555  1450  1752 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:25.482800  1450  1752 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:25.488197  1450  4234 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:25.489664  1450  4234 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:25.490297  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:46:25.490433  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:46:25.493028  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:46:25.493189  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:46:25.493262  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:25.493312  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:25.547979   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:46:25.547979  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.550257  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.550705  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.564832  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.566405  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.566885  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.640219  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.641731  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.675439  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.703051  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.703794  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.739862  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.745480  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.745988  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.765485  1450  1511 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.765610  1450  1511 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.788198  1450 29539 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.788716  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.806029  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.808977  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.810709  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.810809  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.811686  1450  1515 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.811870  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:46:25.816701  1450  1511 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.816837  1450  1511 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.823788  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.826644  1450  2351 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.826921  1450  2351 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.840453  1450 29539 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.841215  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.845907  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.850735  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.850993  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.859471  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.865748  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.866118  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.881812  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:25.883325  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.883455  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:25.885652   909  1512 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.886121   909  1512 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.889663  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.889854  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:25.891707  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.892641  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.893518   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.893788   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.897189  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.897365  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:25.897610  1450  1450 D RILJ    : [9539]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:25.901568  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.902233   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:25.902347   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cda900, pRI=0x7f9784c510, p=0x7f978570a0, pUCI=0x0
10-17 14:46:25.902389   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c510 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.902498   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.902528   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.902560   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.902609   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.902645   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.902678   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.902685   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c510 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.902704   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.902723   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.902748   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.902756   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:25.902773   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.902782   721   749 D RIL     : radioState:10
10-17 14:46:25.902815   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.902829   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:25.902842   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.902863   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:46:25.902883   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.902898   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.902909   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.902927   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:46:25.902951   721   749 I AT      : AT write start
10-17 14:46:25.902965   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.902989   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.903070   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.903100   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.903567   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.903668   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.903712   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.903993   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.904050   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.904103   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.904208   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.904430  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:25.906924   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.907004   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.907091   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.907121   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.907303  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.907392  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:25.907747  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.907884  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.908574   909  1632 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.908756   909  1632 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.909039   909  1632 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.910011  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.910202  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:25.910341  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.910408  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.911353   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.911484   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.911967   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.912751   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.912817   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.912918   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.912972   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.913100   721   766 I AT      : AT read end: 6
10-17 14:46:25.913156   721   766 D AT      : AT< OK
10-17 14:46:25.913187   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.913234   721   766 I AT      : AT read start
10-17 14:46:25.913365   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.913413   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.913454   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.913524   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f978570a0 
10-17 14:46:25.913558   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda900
10-17 14:46:25.913584   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.913693  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:25.913812  1450  1606 D RILJ    : [9539]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:25.914860  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.915021  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:25.917570  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.917775  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:26.316598   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43660 
10-17 14:46:26.316688   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e436c0
10-17 14:46:26.316721   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e436d0
10-17 14:46:26.317660   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43660 reset to NULL
10-17 14:46:26.317733   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43660
10-17 14:46:26.317765   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43670
10-17 14:46:26.599736  1450  1450 D RILJ    : [9540]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:26.608411   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:26.608543   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784cb10, p=0x7f978565b0, pUCI=0x0
10-17 14:46:26.608588   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cb10 p=0x7f978565b0 dispatched to RIL_ATCI_PROXY
10-17 14:46:26.608835   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:26.608885   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:26.608935   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:26.608964   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:26.609022   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:26.609051   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:26.609101   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:26.609128   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:26.609425   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:26.609485   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:26.609554   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:26.609584   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:26.609642   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:26.609670   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:26.609735   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:26.609765   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:26.609824   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:26.609853   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:26.612333   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:26.612438   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:26.612482   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cb10 p=0x7f978565b0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:26.612522   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:26.612589   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:26.612623   721   753 D RIL     : radioState:10
10-17 14:46:26.612679   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:26.612718   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:26.612753   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:26.612781   721   753 I AT      : AT write start
10-17 14:46:26.613179   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:26.613256   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:26.613317   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:26.613468   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:26.613653   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:26.613756   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:26.616008   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:26.616128   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:26.621395   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:26.624921   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:26.625005   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:26.625054   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:26.625931   721   770 I AT      : AT read end: 6
10-17 14:46:26.626009   721   770 D AT      : AT< OK
10-17 14:46:26.626041   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:26.626093   721   770 I AT      : AT read start
10-17 14:46:26.626167   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:26.626214   721   753 D RIL     : p_response->success = 1
10-17 14:46:26.626243   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:26.626267   721   753 D RIL     : strLength = 6
10-17 14:46:26.626293   721   753 D RIL     : line = <
10-17 14:46:26.626293   721   753 D RIL     : OK
10-17 14:46:26.626293   721   753 D RIL     : >
10-17 14:46:26.626322   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:26.626373   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:26.626467   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f978565b0 
10-17 14:46:26.626503   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:46:26.626537   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:26.627819  1450  1606 D RILJ    : [9540]< OEM_HOOK_RAW [B@f03ac1c [SUB0]
10-17 14:46:26.721664  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:26.722994  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:26.727214  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:26.877155  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:26.938973  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:26.939821  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:26.958287  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:26.964204  1450  1752 D DCT     : [0]phoneSubId = 1
10-17 14:46:26.965055  1450  1752 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:27.455067   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185203/0
10-17 14:46:28.555055  1450  1450 D RILJ    : [9541]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:28.557321   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:28.557404   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaac0, pRI=0x7f9784cba0, p=0x7f97856bd0, pUCI=0x0
10-17 14:46:28.557440   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cba0 p=0x7f97856bd0 dispatched to RIL_ATCI_PROXY
10-17 14:46:28.557538   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:28.557580   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:28.557616   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:28.557623   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:28.557646   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:28.557676   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:28.557691   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:28.557709   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:28.557738   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:28.557744   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:28.557752   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:28.557770   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:28.557803   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:28.557809   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:28.557812   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:28.557856   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:28.557895   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:28.557967   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:28.557994   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:28.558031   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:28.558070   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:28.558109   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:28.558186   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:28.558229   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:28.558262   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cba0 p=0x7f97856bd0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:28.558293   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:28.558322   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:28.558347   721   753 D RIL     : radioState:10
10-17 14:46:28.558384   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:28.558413   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:28.558437   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:28.558461   721   753 I AT      : AT write start
10-17 14:46:28.558615   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:28.558675   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:28.558724   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:28.558805   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:28.560607   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:28.560679   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:28.560763   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:28.560810   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:28.560984   721   770 I AT      : AT read end: 6
10-17 14:46:28.561049   721   770 D AT      : AT< OK
10-17 14:46:28.561082   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:28.561127   721   770 I AT      : AT read start
10-17 14:46:28.561172   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:28.561206   721   753 D RIL     : p_response->success = 1
10-17 14:46:28.561233   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:28.561257   721   753 D RIL     : strLength = 6
10-17 14:46:28.561281   721   753 D RIL     : line = <
10-17 14:46:28.561281   721   753 D RIL     : OK
10-17 14:46:28.561281   721   753 D RIL     : >
10-17 14:46:28.561310   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:28.561360   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:28.561430   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f97856bd0 
10-17 14:46:28.561470   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:46:28.561495   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:28.561638  1450  1606 D RILJ    : [9541]< OEM_HOOK_RAW [B@ca90025 [SUB0]
10-17 14:46:30.553603   721   760 I RILC    : NUMBER:1
10-17 14:46:30.553685   721   760 I RILC    : arg len:14
10-17 14:46:30.553725   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:30.553889   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:30.553996   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784cbd0 p=0x7f97856c40 dispatched to RIL_CMD_PROXY_1
10-17 14:46:30.554120   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:30.554173   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:30.554223   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:30.554251   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:30.554298   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:30.554325   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:30.554318   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:30.554357   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:30.554400   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:30.554413   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:30.554428   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:30.554474   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:30.554476   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:30.554505   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:30.554555   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:30.554561   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:30.554583   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:30.554602   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784cbd0 p=0x7f97856c40 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:30.554623   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:30.554650   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:30.554684   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:30.554712   721   751 D RIL     : radioState:10
10-17 14:46:30.554795   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:30.554928   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:30.554967   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:30.554994   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:30.555023   721   751 I AT      : AT write start
10-17 14:46:30.555212   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:30.555271   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:30.555319   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:30.555321   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:30.555346   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:30.555381   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:30.555389   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:30.555415   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:30.555435   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:30.555540   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:30.563327   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:30.563441   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:30.563539   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:30.563592   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:30.563658   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:30.563701   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:30.563781   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:30.563825   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:30.563970   721   768 I AT      : AT read end: 46
10-17 14:46:30.564039   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:30.564071   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:30.564110   721   768 D AT      : AT< OK
10-17 14:46:30.564137   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:30.564190   721   768 I AT      : AT read start
10-17 14:46:30.564245   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:30.564294   721   751 D RIL     : requestQueryThermal success
10-17 14:46:30.564325   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:30.564357   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:30.564399   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:30.564472   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97856c40 
10-17 14:46:30.564514   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:46:30.564539   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:30.626852  1450  1515 D use-Rlog/RLOG-GSM: [RadioCapSwitchUtil] getMainCapabilityPhoneId 0
10-17 14:46:30.627439 25918 25918 D ImsManager: MainCapabilityPhoneId is 0 on feature 2
10-17 14:46:30.640748 25918 25918 D ImsManager: wfc resource value is true, system property is 0, Carrier value is true
10-17 14:46:31.815043   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:46:31.815113   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:31.815182   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:46:31.815222   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:31.815499   721   765 I AT      : AT read end: 37
10-17 14:46:31.815545   721   765 D AT      : AT< +ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815574   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815619   721   765 D RIL     : Nw URC:+ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815688   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:31.815724   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:31.815750   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:31.815818   721   765 I AT      : AT read start
10-17 14:46:31.816216  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:31.816417  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:31.816499  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -280 1 1
10-17 14:46:31.816547  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:32.455351   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185207/0
10-17 14:46:34.643190  1450  1450 D RILJ    : [9542]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:34.645950   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:34.646021   721   760 I RILC-MTK: create request 59: pRequest=0x7f94ce6a60, pRI=0x7f9784cc00, p=0x7f97857110, pUCI=0x0
10-17 14:46:34.646055   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc00 p=0x7f97857110 dispatched to RIL_ATCI_PROXY
10-17 14:46:34.646168   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:34.646197   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:34.646220   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:34.646224   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:34.646221   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:34.646258   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:34.646289   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:34.646292   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:34.646339   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:34.646346   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:34.646363   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:34.646380   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc00 p=0x7f97857110 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:34.646400   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:34.646417   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:34.646424   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:34.646449   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:34.646463   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:34.646474   721   753 D RIL     : radioState:10
10-17 14:46:34.646507   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:34.646513   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:34.646530   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:34.646538   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:34.646546   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:34.646571   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:34.646595   721   753 I AT      : AT write start
10-17 14:46:34.646593   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:34.646745   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:34.646795   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:34.646843   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:34.646927   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:34.647138   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:34.647182   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:34.647224   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:34.647248   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:34.647285   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:34.647308   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:34.654380   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:4
10-17 14:46:34.654460   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 4 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:34.654528   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 4/4 bytes of frame to /dev/pts/6
10-17 14:46:34.654572   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:34.654673   721   770 I AT      : AT read end: 4
10-17 14:46:34.654709   721   770 I AT      : AT read start
10-17 14:46:34.657135   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:2
10-17 14:46:34.657193   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 2 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:34.657253   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 2/2 bytes of frame to /dev/pts/6
10-17 14:46:34.657291   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:34.657392   721   770 I AT      : AT read end: 2
10-17 14:46:34.657430   721   770 D AT      : AT< OK
10-17 14:46:34.657458   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:34.657498   721   770 I AT      : AT read start
10-17 14:46:34.657543   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:34.657577   721   753 D RIL     : p_response->success = 1
10-17 14:46:34.657603   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:34.657626   721   753 D RIL     : strLength = 6
10-17 14:46:34.657649   721   753 D RIL     : line = <
10-17 14:46:34.657649   721   753 D RIL     : OK
10-17 14:46:34.657649   721   753 D RIL     : >
10-17 14:46:34.657676   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:34.657732   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:34.657802   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc00 p=0x7f97857110 
10-17 14:46:34.657832   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a60
10-17 14:46:34.657872   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:34.658038  1450  1606 D RILJ    : [9542]< OEM_HOOK_RAW [B@39e85fa [SUB0]
10-17 14:46:35.117815  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:35.118982  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:35.359861  1450  1450 D RILJ    : [9543]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:35.369803   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:35.370031   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda740, pRI=0x7f9784cc30, p=0x7f97856930, pUCI=0x0
10-17 14:46:35.370115   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc30 p=0x7f97856930 dispatched to RIL_ATCI_PROXY
10-17 14:46:35.370315   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:35.370389   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:35.370402   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:35.370394   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:35.370453   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:35.370500   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:35.370507   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:35.370516   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:35.370580   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:35.370597   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:35.370605   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:35.370641   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:35.370716   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:35.370771   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:35.370844   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:35.370886   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:35.371101   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:35.371105   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:35.371203   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:35.371228   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:35.371418   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:35.371454   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:35.371483   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc30 p=0x7f97856930 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:35.371525   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:35.371575   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:35.371611   721   753 D RIL     : radioState:10
10-17 14:46:35.371688   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:35.371745   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:35.371781   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:35.371809   721   753 I AT      : AT write start
10-17 14:46:35.372113   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:35.372254   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:35.372344   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:35.372511   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:35.372929   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:35.373381   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:35.380078   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:35.380192   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:35.380293   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:35.380353   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:35.380552   721   770 I AT      : AT read end: 6
10-17 14:46:35.380631   721   770 D AT      : AT< OK
10-17 14:46:35.380671   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:35.380730   721   770 I AT      : AT read start
10-17 14:46:35.380794   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:35.380840   721   753 D RIL     : p_response->success = 1
10-17 14:46:35.380869   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:35.381091   721   753 D RIL     : strLength = 6
10-17 14:46:35.381190   721   753 D RIL     : line = <
10-17 14:46:35.381190   721   753 D RIL     : OK
10-17 14:46:35.381190   721   753 D RIL     : >
10-17 14:46:35.381229   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:35.381293   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:35.381415   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc30 p=0x7f97856930 
10-17 14:46:35.381454   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda740
10-17 14:46:35.381479   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:35.381753  1450  1606 D RILJ    : [9543]< OEM_HOOK_RAW [B@ad67ab [SUB0]
