----- timezone:GMT
10-17 14:43:59.875701  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:43:59.887524  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:43:59.887969  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:43:59.891554  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:43:59.894879  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:43:59.895071  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:00.320988   721   760 I RILC    : NUMBER:1
10-17 14:44:00.321047   721   760 I RILC    : arg len:14
10-17 14:44:00.321081   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:44:00.321169   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:44:00.321238   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c7b0 p=0x7f97856ee0 dispatched to RIL_CMD_PROXY_1
10-17 14:44:00.321356   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:44:00.321384   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:44:00.321422   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:44:00.321446   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:44:00.321482   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:44:00.321510   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:44:00.321540   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c7b0 p=0x7f97856ee0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:44:00.321573   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:44:00.321598   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:44:00.321606   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:44:00.321629   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:44:00.321634   721   751 D RIL     : radioState:10
10-17 14:44:00.321670   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:44:00.321677   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:44:00.321695   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:44:00.321719   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:44:00.321731   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:44:00.321747   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:44:00.321755   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:44:00.321771   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:44:00.321789   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:44:00.321793   721   751 I AT      : AT write start
10-17 14:44:00.321816   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:44:00.321852   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:44:00.321876   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:44:00.321877   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:44:00.321906   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:44:00.321944   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:44:00.321976   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:44:00.322015   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:44:00.322040   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:44:00.322054   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:44:00.322074   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:44:00.322098   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:44:00.322104   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:44:00.322153   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:44:00.322254   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:44:00.329777   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:44:00.329932   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:44:00.330005   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:44:00.330049   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:00.330097   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:44:00.330140   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:44:00.330185   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:44:00.330222   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:00.330344   721   768 I AT      : AT read end: 46
10-17 14:44:00.330392   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:44:00.330425   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:44:00.330457   721   768 D AT      : AT< OK
10-17 14:44:00.330481   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:44:00.330519   721   768 I AT      : AT read start
10-17 14:44:00.331104   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:44:00.331172   721   751 D RIL     : requestQueryThermal success
10-17 14:44:00.331204   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:44:00.331235   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:44:00.331281   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:44:00.331340   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97856ee0 
10-17 14:44:00.331379   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:44:00.331874   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:44:00.883701  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:00.884649  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:00.885153  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:00.892971  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:00.893460  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:00.896447  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:00.900301  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:44:00.900470  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:02.449265   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185060/0
10-17 14:44:03.195386  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.196603  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.197045  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.215820  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.216232  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.222922  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.234139  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.235649  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.248897  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.249905  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.250366  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.255405  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.256762  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.257306  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.261885  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.262753  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.263400  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.267202  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.267857  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.268165  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.272625  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.273545  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.274031  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.278055  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.278260  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.280870  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.283421  1450 29539 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.283599  1450 29539 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.286724  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.287436  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.287763  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.291897  1450  2351 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.292115  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.294395  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.297001  1450  1511 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.297179  1450  1511 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.300485  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.301290  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.301633  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.305514  1450  1515 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.305727  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.308009  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.310363  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.310530  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:03.313933  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:44:03.314641  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:44:03.314975  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:44:03.318827  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:44:03.319037  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:44:03.321500  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:44:03.323827  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:44:03.323991  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:44:06.660241  1450  1450 D RILJ    : [9495]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:44:06.663298   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:44:06.663406   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9120, pRI=0x7f9784c210, p=0x7f978572d0, pUCI=0x0
10-17 14:44:06.663439   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f978572d0 dispatched to RIL_ATCI_PROXY
10-17 14:44:06.663570   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:44:06.663598   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:44:06.663635   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:44:06.663666   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:44:06.663706   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:44:06.663707   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:44:06.663738   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:44:06.663744   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:44:06.663770   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f978572d0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:44:06.663782   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:44:06.663799   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:44:06.663808   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:44:06.663828   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:44:06.663844   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:44:06.663852   721   753 D RIL     : radioState:10
10-17 14:44:06.663869   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:44:06.663890   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:44:06.663904   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:44:06.663924   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:44:06.663930   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:44:06.663950   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:44:06.663967   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:44:06.663972   721   753 I AT      : AT write start
10-17 14:44:06.663992   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:44:06.664027   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:44:06.664050   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:44:06.664143   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:44:06.664224   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:44:06.664279   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:44:06.664375   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:44:06.664459   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:44:06.664491   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:44:06.664534   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:44:06.664558   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:44:06.665359   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:44:06.665417   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:44:06.672545   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:44:06.672646   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:44:06.672723   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:44:06.672765   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:44:06.672937   721   770 I AT      : AT read end: 6
10-17 14:44:06.672978   721   770 D AT      : AT< OK
10-17 14:44:06.673008   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:44:06.673054   721   770 I AT      : AT read start
10-17 14:44:06.673112   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:44:06.673153   721   753 D RIL     : p_response->success = 1
10-17 14:44:06.673182   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:44:06.673209   721   753 D RIL     : strLength = 6
10-17 14:44:06.673242   721   753 D RIL     : line = <
10-17 14:44:06.673242   721   753 D RIL     : OK
10-17 14:44:06.673242   721   753 D RIL     : >
10-17 14:44:06.673275   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:44:06.673328   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:06.673408   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f978572d0 
10-17 14:44:06.673441   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9120
10-17 14:44:06.673466   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:44:06.673664  1450  1606 D RILJ    : [9495]< OEM_HOOK_RAW [B@9a2d43e [SUB0]
10-17 14:44:07.446341   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:07.787873   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:11.480394   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:12.607935   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:16.261062   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:21.726992   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:24.296362   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:24.734964   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:33.209262   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:41.682589   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:44:58.630752   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:07.104792   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:15.578683   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:32.526292   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:36.372316   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:36.785249   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.205077   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.395836   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:40.999639   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:45.951575   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:46.627620   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:49.473400   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:45:56.957396 25918 25952 D getTestMode: Test mode is 0
10-17 14:45:57.947286   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:02.234692   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:02.248160   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:05.120045  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:05.126681  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:07.454200   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185112/0
10-17 14:46:10.520698   721   760 I RILC    : NUMBER:1
10-17 14:46:10.520765   721   760 I RILC    : arg len:14
10-17 14:46:10.520800   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:10.520943   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:10.521002   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c3f0 p=0x7f97856690 dispatched to RIL_CMD_PROXY_1
10-17 14:46:10.521116   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:10.521143   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:10.521149   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:10.521187   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:10.521199   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:10.521222   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:10.521264   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:10.521269   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:10.521297   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:10.521339   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:10.521342   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:10.521366   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:10.521404   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:10.521444   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:10.521469   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:10.521505   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:10.521533   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:10.521566   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c3f0 p=0x7f97856690 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:10.521599   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:10.521628   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:10.521656   721   751 D RIL     : radioState:10
10-17 14:46:10.521695   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:10.521736   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:10.521764   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:10.521789   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:10.521812   721   751 I AT      : AT write start
10-17 14:46:10.521913   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:10.521939   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:10.521948   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:10.521997   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:10.522112   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:10.522170   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:10.522226   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:10.522326   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:10.522416   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:10.522422   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:10.522454   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:10.529905   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:10.530051   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:10.530132   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:10.530181   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:10.530235   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:10.530292   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:10.530343   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:10.530384   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:10.530499   721   768 I AT      : AT read end: 46
10-17 14:46:10.530546   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:10.530578   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:10.530615   721   768 D AT      : AT< OK
10-17 14:46:10.530640   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:10.530677   721   768 I AT      : AT read start
10-17 14:46:10.531282   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:10.531338   721   751 D RIL     : requestQueryThermal success
10-17 14:46:10.531369   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:10.531398   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:10.531436   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:10.531498   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c3f0 p=0x7f97856690 
10-17 14:46:10.531535   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:46:10.531567   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:12.454440   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185114/0
10-17 14:46:17.389891  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:17.394358  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:46:17.394570  1450  1450 D RILJ    : [9507]> SCREEN_STATE: false [SUB0]
10-17 14:46:17.397130  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:17.397434   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.397546   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf91e0, pRI=0x7f9784c8d0, p=0x7f978567e0, pUCI=0x0
10-17 14:46:17.397588   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c8d0 p=0x7f978567e0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.397714   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.397730  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:46:17.397755   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.397764   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.397814   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.397841   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.397852  1450  1450 D RILJ    : [9508]> SCREEN_STATE: false [SUB1]
10-17 14:46:17.397880   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.397904   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.397943   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.397971   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.398010   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.398033   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.398068   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.398097   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:17.398127   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c8d0 p=0x7f978567e0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:17.398155   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.398195   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.398226   721   749 D RIL     : radioState:10
10-17 14:46:17.398224   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.398259   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.398296   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.398300   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.398326   721   749 D AT      : AT> AT+CREG=1
10-17 14:46:17.398326   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.398353   721   749 I AT      : AT write start
10-17 14:46:17.398369   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.398393   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.398431   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.398447   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.398459   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.398501   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.398536   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.399184   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.399279   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.399331   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.399419   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.400708   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.400794   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cda760, pRI=0x7f9784c930, p=0x7f97856e70, pUCI=0x0
10-17 14:46:17.400830   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97856e70 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:17.400995   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.401005   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.401010   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.401050   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.401094   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.401110   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.401119   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.401149   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.401163   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.401179   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:17.401187   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.401210   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c930 p=0x7f97856e70 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:17.401220   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.401240   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.401244   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.401270   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.401295   721   755 D RIL     : radioState:0
10-17 14:46:17.401317   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.401335   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401341   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.401359   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401380   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.401397   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.401403   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.401429   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.401443   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.401476   721   755 D AT      : AT> AT+CREG=1
10-17 14:46:17.401500   721   755 I AT      : AT write start
10-17 14:46:17.401592   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.401618   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.401654   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.401692   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.401799   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.401856   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.401905   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.401987   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.406800   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.406878   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.406944   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.406985   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.407088   721   766 I AT      : AT read end: 6
10-17 14:46:17.407139   721   766 D AT      : AT< OK
10-17 14:46:17.407170   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.407215   721   766 I AT      : AT read start
10-17 14:46:17.407231   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.407253   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.407281   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.407305   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.407331   721   749 D AT      : AT> AT+CGREG=1
10-17 14:46:17.407341   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.407355   721   749 I AT      : AT write start
10-17 14:46:17.407381   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.407467   721   772 I AT      : AT read end: 6
10-17 14:46:17.407495   721   772 D AT      : AT< OK
10-17 14:46:17.407526   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.407567   721   772 I AT      : AT read start
10-17 14:46:17.407608   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.407636   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.407658   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.407680   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.407685   721   755 D AT      : AT> AT+CGREG=1
10-17 14:46:17.407712   721   755 I AT      : AT write start
10-17 14:46:17.407728   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.407810   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.407833   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.407874   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.407920   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.407988   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.408628   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.408691   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.408760   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.408803   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.408894   721   766 I AT      : AT read end: 6
10-17 14:46:17.408934   721   766 D AT      : AT< OK
10-17 14:46:17.408963   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.408998   721   766 I AT      : AT read start
10-17 14:46:17.409036   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.409100   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.409149   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:46:17.409175   721   749 I AT      : AT write start
10-17 14:46:17.409216   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.409267   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.409290   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.409324   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.409337   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.409364   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.409381   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.409467   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.409531   721   772 I AT      : AT read end: 6
10-17 14:46:17.409561   721   772 D AT      : AT< OK
10-17 14:46:17.409589   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.409627   721   772 I AT      : AT read start
10-17 14:46:17.409671   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.409714   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.409742   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:46:17.409764   721   755 I AT      : AT write start
10-17 14:46:17.409889   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.409936   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.409982   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.410056   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.410704   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.410763   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.410828   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.410871   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.411100   721   766 I AT      : AT read end: 6
10-17 14:46:17.411161   721   766 D AT      : AT< OK
10-17 14:46:17.411252   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.411254   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.411296   721   766 I AT      : AT read start
10-17 14:46:17.411313   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.411380   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.411423   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.411519   721   772 I AT      : AT read end: 6
10-17 14:46:17.411524   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.411561   721   772 D AT      : AT< OK
10-17 14:46:17.411580   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.411588   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.411608   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:46:17.411627   721   772 I AT      : AT read start
10-17 14:46:17.411632   721   749 I AT      : AT write start
10-17 14:46:17.411663   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.411703   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.411728   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:46:17.411750   721   755 I AT      : AT write start
10-17 14:46:17.411777   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.411828   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.411865   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.411877   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.411907   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.411972   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:17.412033   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.412104   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:17.412764   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.412825   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.412889   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.412930   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.413026   721   766 I AT      : AT read end: 6
10-17 14:46:17.413063   721   766 D AT      : AT< OK
10-17 14:46:17.413091   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.413127   721   766 I AT      : AT read start
10-17 14:46:17.413174   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.413290   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.413319   721   749 D AT      : AT> AT+CEREG=1
10-17 14:46:17.413343   721   749 I AT      : AT write start
10-17 14:46:17.413463   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.413467   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.413515   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.413520   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.413561   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.413578   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.413621   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.413637   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.413715   721   772 I AT      : AT read end: 6
10-17 14:46:17.413746   721   772 D AT      : AT< OK
10-17 14:46:17.413771   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.413811   721   772 I AT      : AT read start
10-17 14:46:17.413857   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.413900   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.413924   721   755 D AT      : AT> AT+CEREG=1
10-17 14:46:17.413946   721   755 I AT      : AT write start
10-17 14:46:17.414063   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.414111   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.414157   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.414234   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.414789   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.414848   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.414909   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.414947   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.415043   721   766 I AT      : AT read end: 6
10-17 14:46:17.415074   721   766 D AT      : AT< OK
10-17 14:46:17.415100   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.415142   721   766 I AT      : AT read start
10-17 14:46:17.415184   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.415220   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:17.415263   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.415333   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c8d0 p=0x7f978567e0 
10-17 14:46:17.415371   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf91e0
10-17 14:46:17.415397   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:17.415513  1450  1606 D RILJ    : [9507]< SCREEN_STATE  [SUB0]
10-17 14:46:17.416079   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.416153   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.416226   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.416270   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.416385   721   772 I AT      : AT read end: 6
10-17 14:46:17.416425   721   772 D AT      : AT< OK
10-17 14:46:17.416452   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.416499   721   772 I AT      : AT read start
10-17 14:46:17.416573   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.416615   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:17.416654   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:17.416730   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c930 p=0x7f97856e70 
10-17 14:46:17.416763   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:46:17.416791   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.416895  1450  1609 D RILJ    : [9508]< SCREEN_STATE  [SUB1]
10-17 14:46:17.454626   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185124/0
10-17 14:46:17.634776  1450  1450 D RILJ    : [9509]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:17.636509   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:17.636584   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9240, pRI=0x7f9784cae0, p=0x7f97857d50, pUCI=0x0
10-17 14:46:17.636618   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cae0 p=0x7f97857d50 dispatched to RIL_ATCI_PROXY
10-17 14:46:17.636707   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.636710   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.636714   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.636744   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.636756   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.636782   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.636800   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.636808   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:17.636814   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.636815   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.636847   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.636853   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cae0 p=0x7f97857d50 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:17.636879   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.636883   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.636906   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:17.636917   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:17.636940   721   753 D RIL     : radioState:10
10-17 14:46:17.636948   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.636970   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.636979   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:17.637010   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:17.637012   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.637038   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:17.637062   721   753 I AT      : AT write start
10-17 14:46:17.637063   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.637083   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.637131   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.637149   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.637223   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.637272   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.637322   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:17.637419   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:17.637469   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.637519   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.637568   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.637598   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.644820   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:17.644900   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:17.644968   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:17.645021   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.645119   721   770 I AT      : AT read end: 6
10-17 14:46:17.645159   721   770 D AT      : AT< OK
10-17 14:46:17.645187   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:17.645227   721   770 I AT      : AT read start
10-17 14:46:17.645267   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:17.645309   721   753 D RIL     : p_response->success = 1
10-17 14:46:17.645337   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:17.645359   721   753 D RIL     : strLength = 6
10-17 14:46:17.645382   721   753 D RIL     : line = <
10-17 14:46:17.645382   721   753 D RIL     : OK
10-17 14:46:17.645382   721   753 D RIL     : >
10-17 14:46:17.645408   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:17.645453   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.645523   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cae0 p=0x7f97857d50 
10-17 14:46:17.645554   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:46:17.645577   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.645726  1450  1606 D RILJ    : [9509]< OEM_HOOK_RAW [B@7708533 [SUB0]
10-17 14:46:17.796150  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.797315  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.797765  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.818583  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:17.819639  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:17.824550  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:17.829652  1450  1807 D DCT     : [0]phoneSubId = 1
10-17 14:46:17.831300  1450  1807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:17.938800  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.951296  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:17.952141  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:46:17.952299  1450  1450 D RILJ    : [9510]> SCREEN_STATE: true [SUB0]
10-17 14:46:17.954836  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:17.955639  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:46:17.955735   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.955808   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6a20, pRI=0x7f9784c360, p=0x7f97857dc0, pUCI=0x0
10-17 14:46:17.955821  1450  1450 D RILJ    : [9511]> SCREEN_STATE: true [SUB1]
10-17 14:46:17.955847   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97857dc0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.955980   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.956000   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.956035   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.956092   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.956136   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.956141   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.956174   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.956226   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.956268   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.956304   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.956349   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.956377   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.956421   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.956448   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.956492   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.956516   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.956562   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.956591   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.956632   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.956657   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.957047   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:17.957113   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:17.957154   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c360 p=0x7f97857dc0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:17.957190   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.957225   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.957253   721   749 D RIL     : radioState:10
10-17 14:46:17.957331   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.957361   721   749 D AT      : AT> AT+CREG=3
10-17 14:46:17.957387   721   749 I AT      : AT write start
10-17 14:46:17.957645   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.957697   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:17.957731   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.957804   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.957861   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.957986   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.961839   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:17.961957   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9460, pRI=0x7f9784c4b0, p=0x7f97857e30, pUCI=0x0
10-17 14:46:17.961999   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c4b0 p=0x7f97857e30 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:17.962116   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.962116   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.962173   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.962207   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.962233   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.962244   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.962295   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.962299   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.962325   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.962365   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.962367   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.962403   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.962443   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.962468   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.962509   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.962554   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.962578   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.962621   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.962927   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:17.963032   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:17.963094   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c4b0 p=0x7f97857e30 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:17.963132   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:17.963125   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.963169   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.963172   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:17.963212   721   755 D RIL     : radioState:0
10-17 14:46:17.963257   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963284   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963312   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:17.963367   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.963396   721   755 D AT      : AT> AT+CREG=3
10-17 14:46:17.963422   721   755 I AT      : AT write start
10-17 14:46:17.964142   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.964231   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.964286   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.964379   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.965635   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:46:17.965729   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:17.965834   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:46:17.965888   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.965945   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.965987   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.966043   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.966086   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.966209   721   765 I AT      : AT read end: 36
10-17 14:46:17.966268   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966304   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966349   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:17.966392   721   765 D RIL     : NW state changed: normal case
10-17 14:46:17.966425   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:46:17.966458   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:17.966488   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:46:17.966547   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:46:17.966582   721   765 D RIL     : bCREGType3Support=1
10-17 14:46:17.966612   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:17.966618   721   766 I AT      : AT read end: 6
10-17 14:46:17.966638   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:46:17.966657   721   766 D AT      : AT< OK
10-17 14:46:17.966689   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.966723   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:17.966735   721   766 I AT      : AT read start
10-17 14:46:17.966901   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.966887   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.965318  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.966959   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.966970   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e434e0
10-17 14:46:17.966988   721   749 D AT      : AT> AT+CGREG=3
10-17 14:46:17.967004   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e434f0
10-17 14:46:17.967013   721   749 I AT      : AT write start
10-17 14:46:17.967120   721   765 I AT      : AT read start
10-17 14:46:17.967355  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.967385  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:46:17.967637   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.967720   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.967783   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.967900   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.968202  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:17.968366  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:46:17.968517  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:17.968859   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:46:17.968956   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:46:17.969048   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:46:17.969101   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.969157   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.969206   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.969338   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.969392   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.969920   721   771 I AT      : AT read end: 36
10-17 14:46:17.970028   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970063   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970110   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:17.970150   721   771 D RIL     : NW state changed: normal case
10-17 14:46:17.970185   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:46:17.970217   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:46:17.970249   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:46:17.970309   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:46:17.970347   721   771 D RIL     : bCREGType3Support=1
10-17 14:46:17.970378   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:17.970409   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:46:17.970497   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:17.970531   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:17.970596   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e434e0, cancel
10-17 14:46:17.970631   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e435a0
10-17 14:46:17.970666   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e435b0
10-17 14:46:17.970739   721   771 I AT      : AT read start
10-17 14:46:17.970822   721   772 I AT      : AT read end: 6
10-17 14:46:17.970851   721   772 D AT      : AT< OK
10-17 14:46:17.971136   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.971228   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.971329   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.971386   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.971392  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:46:17.971481  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:46:17.971488  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:46:17.971550   721   766 I AT      : AT read end: 6
10-17 14:46:17.971587   721   766 D AT      : AT< OK
10-17 14:46:17.971605  1450  1450 D RILJ    : [9512]> OPERATOR [SUB0]
10-17 14:46:17.971616   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.971666   721   766 I AT      : AT read start
10-17 14:46:17.970887   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.971735   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.971752   721   772 I AT      : AT read start
10-17 14:46:17.971806   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.971836   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:46:17.971865   721   749 I AT      : AT write start
10-17 14:46:17.971997   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.972069   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.972099   721   755 D AT      : AT> AT+CGREG=3
10-17 14:46:17.972129   721   755 I AT      : AT write start
10-17 14:46:17.972348   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.972413   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.972468   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.972558   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:17.973078   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.973156   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.973211   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.973305   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:17.973698  1450  1450 D RILJ    : [9513]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:46:17.974292   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:46:17.974376   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9540, pRI=0x7f9784c6f0, p=0x7f97857f10, pUCI=0x0
10-17 14:46:17.974413   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 dispatched to RIL_CMD_PROXY_3
10-17 14:46:17.974523   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:17.974559   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:17.974604   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:17.974630   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:17.974721   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:17.974755   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:17.974855   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:17.974886   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:17.974928   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:17.974955   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:17.974996   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:17.975023   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:17.975086   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:17.975112   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:17.975158   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:17.975183   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:17.975184   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:17.975219   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:17.975357   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:17.975392   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:17.975666  1450  1450 D RILJ    : [9514]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:46:17.976124   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:17.976213   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9b80, pRI=0x7f9784cb10, p=0x7f97857f80, pUCI=0x0
10-17 14:46:17.976253   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.976284   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.976321   721   760 D RILC-MTK: Request pRI=0x7f9784cb10 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:46:17.977963  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:17.978076  1450  1450 D RILJ    : [9515]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:46:17.978453   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:17.978547   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9bc0, pRI=0x7f9784cba0, p=0x7f97857ff0, pUCI=0x0
10-17 14:46:17.978588   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.978619   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.978650   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.978683   721   760 D RILC-MTK: Request pRI=0x7f9784cba0 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:46:17.980733   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.980834   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.983041   721   772 I AT      : AT read end: 6
10-17 14:46:17.983131   721   772 D AT      : AT< OK
10-17 14:46:17.983165   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.983215   721   772 I AT      : AT read start
10-17 14:46:17.983286   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.983343   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.983373   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:46:17.983398   721   755 I AT      : AT write start
10-17 14:46:17.983518   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.983570   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.983595   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.983618   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.983657   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.983671   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.983698   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.983762   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:17.983775   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.983814   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.983941   721   766 I AT      : AT read end: 6
10-17 14:46:17.983992   721   766 D AT      : AT< OK
10-17 14:46:17.984023   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.984063   721   766 I AT      : AT read start
10-17 14:46:17.984119   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.984172   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.984201   721   749 D AT      : AT> AT+ECSQ
10-17 14:46:17.984239   721   749 I AT      : AT write start
10-17 14:46:17.985467   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.985566   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.985630   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.985727   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:46:17.986599  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:17.987042  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:17.988018  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:17.988177  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:17.988266  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:46:17.988353  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:17.988405  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:46:17.989349  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:17.989478  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:17.989552  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:46:17.989603  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:46:17.989688  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:17.989749  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:46:17.989808  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:46:17.989862  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:46:17.989904  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:46:17.989941  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:46:17.989973  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:17.990088  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:17.990191  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:46:17.990258  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:46:17.990308  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:46:17.990560  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:46:17.991128   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:17.991312   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9be0, pRI=0x7f9784cbd0, p=0x7f97858140, pUCI=0x0
10-17 14:46:17.991358   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991389   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991418   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cba0 p=0x7f97857ff0 is queued in RIL_CMD_PROXY_3
10-17 14:46:17.991448   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:17.991447   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.991485   721   760 D RILC-MTK: Request pRI=0x7f9784cbd0 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:46:17.991512   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.991589   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.991634   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.991738   721   772 I AT      : AT read end: 6
10-17 14:46:17.991808   721   772 D AT      : AT< OK
10-17 14:46:17.991838   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.991878   721   772 I AT      : AT read start
10-17 14:46:17.991931   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.991954   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:46:17.991975   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.992002   721   755 D AT      : AT> AT+ECSQ
10-17 14:46:17.992005   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.992029   721   755 I AT      : AT write start
10-17 14:46:17.992076   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:46:17.992117   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.992195   721   766 I AT      : AT read end: 37
10-17 14:46:17.992225   721   766 D AT      : AT< +ECSQ: 42,99,-273,1,1,1,1,3,32767
10-17 14:46:17.992252   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 42,99,-273,1,1,1,1,3,32767
10-17 14:46:17.992282   721   766 I AT      : AT read start
10-17 14:46:17.992277   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.992326   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.992375   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.992458   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:46:17.993089   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.993167   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.993242   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.993285   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.993420   721   766 I AT      : AT read end: 6
10-17 14:46:17.993463   721   766 D AT      : AT< OK
10-17 14:46:17.993490   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.993541   721   766 I AT      : AT read start
10-17 14:46:17.993599   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.993694   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:17.993737   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:17.993763   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:17.993835   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.993863   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:46:17.993887   721   749 I AT      : AT write start
10-17 14:46:17.994091   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:46:17.994171   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.994244   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:46:17.994286   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.994340   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.994383   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.994430   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.994468   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.994567   721   772 I AT      : AT read end: 42
10-17 14:46:17.994603   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:17.994631   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:17.994668   721   772 D AT      : AT< OK
10-17 14:46:17.994693   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.994731   721   772 I AT      : AT read start
10-17 14:46:17.994773   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.994822   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:46:17.994859   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:46:17.994888   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.994911   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:46:17.994933   721   755 I AT      : AT write start
10-17 14:46:17.995083   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.995144   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.995194   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.995270   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:17.995639   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.995709   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.995760   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.995840   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:17.997082   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:17.997177   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:17.997446   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:17.997496   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.997559   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:17.997602   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:17.997658   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:17.997699   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:17.997833   721   772 I AT      : AT read end: 6
10-17 14:46:17.997884   721   772 D AT      : AT< OK
10-17 14:46:17.997919   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:17.997962   721   772 I AT      : AT read start
10-17 14:46:17.998007   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.998023   721   766 I AT      : AT read end: 6
10-17 14:46:17.998050   721   766 D AT      : AT< OK
10-17 14:46:17.998074   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:17.998079   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:17.998109   721   755 D AT      : AT> AT+CEREG=3
10-17 14:46:17.998123   721   766 I AT      : AT read start
10-17 14:46:17.998150   721   755 I AT      : AT write start
10-17 14:46:17.998417   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.998483   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:17.998511   721   749 D AT      : AT> AT+CEREG=3
10-17 14:46:17.998536   721   749 I AT      : AT write start
10-17 14:46:17.998712   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.998712   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:17.998775   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.998774   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:17.998831   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:17.998925   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:17.998998   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:17.999086   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:18.000472   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.000544   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.000624   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.000671   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.000810   721   766 I AT      : AT read end: 6
10-17 14:46:18.001044   721   766 D AT      : AT< OK
10-17 14:46:18.001093   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.001146   721   766 I AT      : AT read start
10-17 14:46:18.000233  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.001249   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.001301   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.001341   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.001430   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97857dc0 
10-17 14:46:18.001464   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:46:18.001504   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.001537   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784c6f0 p=0x7f97857f10 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.001567   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.001596   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:18.001619   721   749 D RIL     : radioState:10
10-17 14:46:18.001656   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.001691   721   749 D AT      : AT> AT+COPS?
10-17 14:46:18.001715   721   749 I AT      : AT write start
10-17 14:46:18.001948   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.002035   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.002096   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.002191   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.002290   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:18.002342   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.002357  1450  1606 D RILJ    : [9510]< SCREEN_STATE  [SUB0]
10-17 14:46:18.002426   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:18.002473   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.002613   721   772 I AT      : AT read end: 6
10-17 14:46:18.002662   721   772 D AT      : AT< OK
10-17 14:46:18.002696   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:18.002689  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.002758   721   772 I AT      : AT read start
10-17 14:46:18.002790  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.002819   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.002848  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:46:18.002863   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.002909   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.002999   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f97857e30 
10-17 14:46:18.003036   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9460
10-17 14:46:18.003064   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.003300  1450  1609 D RILJ    : [9511]< SCREEN_STATE  [SUB1]
10-17 14:46:18.003284  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.003715  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.004434   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:18.004518   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.004598   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:18.004640   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.004690   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.004731   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.004776   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.004818   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.004978   721   766 I AT      : AT read end: 30
10-17 14:46:18.005022   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:18.005055   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:18.005093   721   766 D AT      : AT< OK
10-17 14:46:18.005119   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.005157   721   766 I AT      : AT read start
10-17 14:46:18.005218   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.005269   721   749 D RIL     : Get operator code 25020
10-17 14:46:18.005305   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:46:18.005348   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:46:18.005379   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.005443   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.005525   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f97857f10 
10-17 14:46:18.005568   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9540
10-17 14:46:18.005601   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.005637   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cb10 p=0x7f97857f80 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.005667   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.005697   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.005722   721   749 D RIL     : radioState:10
10-17 14:46:18.005776   721   749 D RIL     : request gprs reg state: normal case
10-17 14:46:18.005810   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.005838   721   749 D AT      : AT> AT+CGREG?
10-17 14:46:18.005861   721   749 I AT      : AT write start
10-17 14:46:18.007482   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.007579   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.007637   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.007731   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:18.008185  1450  1606 D RILJ    : [9512]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:46:18.010680  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:46:18.010871  1450  1450 D RILJ    : [9516]> OPERATOR [SUB1]
10-17 14:46:18.015035  1450  1450 D RILJ    : [9517]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:46:18.016083   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:46:18.016112   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:46:18.016176   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.016180   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9c00, pRI=0x7f9784cc00, p=0x7f978581b0, pUCI=0x0
10-17 14:46:18.016219   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cc00 p=0x7f978581b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.016274   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:46:18.016320   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.016342   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.016377   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.016385   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.016422   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784cc00 p=0x7f978581b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.016424   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.016456   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.016483   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.016487   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:18.016516   721   755 D RIL     : radioState:0
10-17 14:46:18.016527   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.016566   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016593   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016620   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016649   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.016687   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.016717   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.016771   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.016782   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.016822   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.016853   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc00 p=0x7f978581b0 
10-17 14:46:18.016867   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.016886   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c00
10-17 14:46:18.016894   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.016970   721   766 I AT      : AT read end: 50
10-17 14:46:18.017006   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:18.017036   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:18.017071   721   766 D AT      : AT< OK
10-17 14:46:18.017097   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.017144   721   766 I AT      : AT read start
10-17 14:46:18.017331   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.017344  1450  1609 D RilRequest: [9516]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.017383   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.017436   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.017464   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.017495   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.017507   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.017535   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.017543   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.017573   721   749 E RIL     : The value in the field <lac> :0
10-17 14:46:18.017576   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.017610   721   749 D RIL     : cid: 3583
10-17 14:46:18.017627   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.017640   721   749 E RIL     : The value of act: 3
10-17 14:46:18.017668   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.017673   721   749 D RIL     : cause_type: 0
10-17 14:46:18.017694   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.017702   721   749 D RIL     : reject_cause: 0
10-17 14:46:18.017737   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.017744   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.017767   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.017773   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:46:18.017799   721   749 I AT      : AT write start
10-17 14:46:18.017961   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.017991   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.018053   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.018272   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.018340   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.018392   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.018480   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:46:18.019033  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.020175  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.020547  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.022159  1450  1450 D RILJ    : [9518]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:46:18.022845   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:18.022916   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9c80, pRI=0x7f9784cc30, p=0x7f978565b0, pUCI=0x0
10-17 14:46:18.022953   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f978565b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.023103   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.023134   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.023148   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.023196   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.023204   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.023224   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.023270   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.023273   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.023299   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.023312   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f978565b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.023342   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.023377   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.023404   721   755 D RIL     : radioState:0
10-17 14:46:18.023425   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.023448   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023454   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.023477   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023506   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023498   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.023534   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.023543   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.023572   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.023587   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.023603   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.023620   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.023629   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.023648   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.023653   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.023710   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc30 p=0x7f978565b0 
10-17 14:46:18.023710   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.023741   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.023750   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c80
10-17 14:46:18.023781   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.023994   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.024342   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.024418   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.024660  1450  1450 D RILJ    : [9519]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:46:18.024869   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:18.024963  1450  1609 D RilRequest: [9517]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.024978   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9ca0, pRI=0x7f9784c510, p=0x7f97856bd0, pUCI=0x0
10-17 14:46:18.025022   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f97856bd0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.025128   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.025164   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.025242   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.025252   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.025280   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.025325   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.025332   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.025363   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.025381   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c510 p=0x7f97856bd0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.025414   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.025448   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.025479   721   755 D RIL     : radioState:0
10-17 14:46:18.025531   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025558   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025585   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025615   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:18.025650   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:18.025678   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.025727   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.025789   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f97856bd0 
10-17 14:46:18.025829   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9ca0
10-17 14:46:18.025856   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.025949   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.025978   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.026047   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.026079   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.026175   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.026216   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.026262   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.026287   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.026362   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.026416  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.026398   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.026459   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:46:18.026506   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.026519   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.026534   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.026530  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:18.026580   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.026597   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:46:18.026604   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.026643   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.026683  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:18.026760   721   766 I AT      : AT read end: 19
10-17 14:46:18.026795   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:46:18.026813  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:18.026826   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:46:18.026862   721   766 I AT      : AT read start
10-17 14:46:18.026860  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.026948  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:18.027073  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:18.027117  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:18.027887   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:18.027962   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cda740, pRI=0x7f9784cab0, p=0x7f97856c40, pUCI=0x0
10-17 14:46:18.027999   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cab0 p=0x7f97856c40 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:18.028123   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.028148   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.028159   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.028199   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.028203   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.028211   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.028234   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.028275   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.028279   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.028314   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.028640  1450  1609 D RilRequest: [9518]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:18.028839   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.028879   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.028933   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.028959   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.029019   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.029099   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.029315   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.029350   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:18.029383   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cab0 p=0x7f97856c40 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:18.029415   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.029447   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:18.029473   721   755 D RIL     : radioState:0
10-17 14:46:18.029512   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.029541   721   755 D AT      : AT> AT+COPS?
10-17 14:46:18.029564   721   755 I AT      : AT write start
10-17 14:46:18.031774   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.031847   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.031901   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:18.031990   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:46:18.032111   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.032154   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.032224   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.032249   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.032351   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.032406   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.032490   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.032534   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.032701   721   766 I AT      : AT read end: 6
10-17 14:46:18.032742   721   766 D AT      : AT< OK
10-17 14:46:18.032774   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.032823   721   766 I AT      : AT read start
10-17 14:46:18.032894   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.032979   721   749 E RIL     : rid: 0
10-17 14:46:18.033011   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:18.033042   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:18.033068   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:18.033097   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:18.033127   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.033186   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.033290   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f97857f80 
10-17 14:46:18.033334   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:46:18.033366   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.033398   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cba0 p=0x7f97857ff0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.033428   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.033459   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:18.033484   721   749 D RIL     : radioState:10
10-17 14:46:18.033525   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.033554   721   749 D AT      : AT> AT+CREG?
10-17 14:46:18.033578   721   749 I AT      : AT write start
10-17 14:46:18.034042  1450  1606 D RILJ    : [9513]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:46:18.034770  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.034876  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:46:18.034948  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:46:18.034994  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:46:18.036732  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.036829  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:46:18.036902  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:46:18.036955  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:46:18.037037  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:46:18.037088  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:46:18.037126  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:46:18.037165  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:46:18.037284  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:46:18.037580   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.037665   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.037722   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.037820   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.041212   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:46:18.041285   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.041381   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:46:18.041429   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041486   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:18.041529   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:18.041588   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:18.041631   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041679   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:46:18.041747   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.041810   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:46:18.041854   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.041901   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.041942   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.041987   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.042024   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.042293   721   766 I AT      : AT read end: 44
10-17 14:46:18.042337   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:18.042369   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:18.042415   721   766 D AT      : AT< OK
10-17 14:46:18.042441   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.042465   721   772 I AT      : AT read end: 18
10-17 14:46:18.042482   721   766 I AT      : AT read start
10-17 14:46:18.042498   721   772 D AT      : AT< +COPS: 0
10-17 14:46:18.042525   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:46:18.042533   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.042556   721   772 D AT      : AT< OK
10-17 14:46:18.042585   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.042583   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:18.042623   721   749 E RIL     : The value in the field <lac> :127
10-17 14:46:18.042635   721   772 I AT      : AT read start
10-17 14:46:18.042668   721   749 D RIL     : cid: 3583
10-17 14:46:18.042699   721   749 E RIL     : The value of act: 3
10-17 14:46:18.042724   721   749 D RIL     : cause_type: 0
10-17 14:46:18.042749   721   749 D RIL     : reject_cause: 0
10-17 14:46:18.042813   721   749 E RIL     : rid: 0
10-17 14:46:18.042846   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:18.042880   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:18.042907   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:18.042937   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:18.042967   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:46:18.043006   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.043088   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.043183   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f97857ff0 
10-17 14:46:18.043217   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9bc0
10-17 14:46:18.043257   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.043290   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cbd0 p=0x7f97858140 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.043322   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.043352   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:18.043376   721   749 D RIL     : radioState:10
10-17 14:46:18.043420   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.043447   721   749 D AT      : AT> AT+COPS?
10-17 14:46:18.043469   721   749 I AT      : AT write start
10-17 14:46:18.043488  1450  1606 D RILJ    : [9514]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:46:18.043711   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.043781   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.043834   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.043893   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:18.043936   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:18.043951   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:18.044005   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:18.044090   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cab0 p=0x7f97856c40 
10-17 14:46:18.044123   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda740
10-17 14:46:18.044153   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.044388  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:46:18.044481  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:46:18.044567  1450  1609 D RILJ    : [9519]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:46:18.045742   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:18.045812   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.045884   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:18.045928   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.046110   721   766 I AT      : AT read end: 24
10-17 14:46:18.046152   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:18.046184   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:18.046222   721   766 I AT      : AT read start
10-17 14:46:18.046297   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.046343   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.046403   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.046442   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.046522   721   766 I AT      : AT read end: 6
10-17 14:46:18.046551   721   766 D AT      : AT< OK
10-17 14:46:18.046582   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.046623   721   766 I AT      : AT read start
10-17 14:46:18.046673   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.046721   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.046772   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.046860   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97858140 
10-17 14:46:18.046893   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9be0
10-17 14:46:18.046920   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.047017  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:46:18.047086  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:46:18.047160  1450  1606 D RILJ    : [9515]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:46:18.053316  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.053495  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:18.055702  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:18.055804  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:46:18.055847  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.055913  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:46:18.055955  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.055985  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.056032  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:18.056068  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.056106  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.056163  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:46:18.056220  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:46:18.056262  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:46:18.056430  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:46:18.056491  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:18.056544  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:46:18.056579  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.056646  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:18.058263  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:46:18.058361  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:46:18.058453  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:46:18.058493  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:46:18.058661  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:46:18.058706  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:46:18.058745  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.058806  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:18.058846  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:18.058877  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:18.059714  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:18.059798  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:46:18.061747  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:46:18.061837  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:46:18.061893  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:18.062053  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:18.062201  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:46:18.062485  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:18.062568  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:18.062629  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:46:18.062685  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:46:18.062871  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:18.062937  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:18.063010  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:46:18.063102  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063157  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063202  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063247  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063294  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063339  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063390  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063434  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063495  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063546  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:18.063588  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:46:18.063632  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:46:18.063678  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:46:18.063743  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:46:18.064749  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:46:18.065672  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.065839  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:46:18.066546  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:46:18.067460  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:46:18.067
10-17 14:46:18.067669  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:46:18.068471  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.068798  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.068943  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:46:18.069020  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:46:18.069092  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.069396  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:46:18.070181   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.070315   909  6090 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.070527   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=2
10-17 14:46:18.071006   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.071502   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.071960   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072398   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072813   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.072904   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:46:18.072961   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073125   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.073250   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073407   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.073715   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.073928   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074180   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.074386   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074498   909  6090 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:18.074679   909  6090 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:18.074931   909  6090 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.075285  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.075462  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:18.075530  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:18.075565  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.075609  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:18.075636  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:18.086654  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.087641   909  6090 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.092721  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:46:18.092840  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:18.093082  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.093157  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:18.098944   909  7313 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.099263   909  7313 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.101247  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.101386  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:18.103171   909  6089 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.103576   909  6089 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.104891  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:46:18.106530  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.107349  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.107567  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:18.107843  1450  1450 D RILJ    : [9520]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:18.111618   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:18.111732   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cdaa00, pRI=0x7f9784cd80, p=0x7f97856cb0, pUCI=0x0
10-17 14:46:18.111773   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f97856cb0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:18.111899   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.111955   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.111960   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.111996   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.112036   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.112045   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.112065   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.112115   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.112150   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.112191   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:18.112211   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.112257   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.112284   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.112316   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.112329   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.112344   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.112372   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f97856cb0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.112403   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.112405   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.112433   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.112442   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:18.112469   721   749 D RIL     : radioState:10
10-17 14:46:18.112488   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.112514   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.112519   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:18.112553   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:46:18.112568   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.112583   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.112595   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.112611   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:46:18.112637   721   749 I AT      : AT write start
10-17 14:46:18.112652   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.112682   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.113843   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.113925   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.113985   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.114117   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:18.117162  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:18.119531  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.119671  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:18.119820  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.119899  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.120880   909  6089 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.121063   909  6089 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.122329   909  6089 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.123641  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.123848  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:18.124023  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.124161  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.124636   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.124813   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.125151   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.129379   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:46:18.132985  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.134091   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.134167   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.134267   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.134314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.134491   721   766 I AT      : AT read end: 6
10-17 14:46:18.134537   721   766 D AT      : AT< OK
10-17 14:46:18.134570   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.134627   721   766 I AT      : AT read start
10-17 14:46:18.134706   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.134742   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.134787   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.134863   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cd80 p=0x7f97856cb0 
10-17 14:46:18.134901   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaa00
10-17 14:46:18.134931   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.135055  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:18.135163  1450  1606 D RILJ    : [9520]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:18.144672  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.145267  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.148497  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:18.148742  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:18.154223  1450  4234 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:18.156278  1450  4234 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:18.181493  1450  1752 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:18.182769  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:46:18.182876  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:46:18.183826  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:46:18.183906  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:46:18.183956  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:18.183989  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:18.184150  1450  1752 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:18.228221  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.229944  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.246347  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.283632  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.283904  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.331074  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.334616  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.335212  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.379040  1450  4234 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.379277  1450  4234 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.382983  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.385200  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.418671  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.421536  1450 23534 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.421619  1450 23534 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.423449  1450  1683 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.423612  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:46:18.451658  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.455130  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.455621  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.475880  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.479508  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.479908  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.505221  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.507164  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.518410  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.521981  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:18.523566  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.523703  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:18.528983   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.529309   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.534786  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.534940  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:18.539213   909  1946 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.539541   909  1946 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.542105  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.542294  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:18.542528  1450  1450 D RILJ    : [9521]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:18.544980   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:18.545084   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cc36c0, pRI=0x7f9784cde0, p=0x7f97856540, pUCI=0x0
10-17 14:46:18.545124   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 dispatched to RIL_CMD_PROXY_3
10-17 14:46:18.545256   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:18.545286   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:18.545308   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:18.545342   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:18.545352   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:18.545368   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:18.545402   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:18.545411   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:18.545427   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:18.545460   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:18.545469   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:18.545486   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:18.545529   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:18.545554   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:18.545592   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:18.545644   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:18.545676   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:18.545711   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:18.545707   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:18.545739   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:18.545745   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:18.545779   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:18.545778   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:18.545807   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:18.545810   721   749 D RIL     : radioState:10
10-17 14:46:18.545845   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:18.545853   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:18.545885   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:18.545886   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:46:18.545919   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.545945   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:46:18.545966   721   749 I AT      : AT write start
10-17 14:46:18.546106   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:18.546571  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:18.546592   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:18.546649   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:18.546702   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:18.546799   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:18.548277  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.548354  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:18.548435  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.548463  1450  1634 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.548487  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.548588  1450  1634 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.548973   909   923 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.549055   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.549275   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.550028  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:18.550151  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:18.550798  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:18.551082  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:18.551800   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:18.551924   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:18.554439   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:18.554508   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:18.554582   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:18.554626   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:18.554752   721   766 I AT      : AT read end: 6
10-17 14:46:18.554804   721   766 D AT      : AT< OK
10-17 14:46:18.554835   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:18.554880   721   766 I AT      : AT read start
10-17 14:46:18.554948   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:18.554979   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:18.555020   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:18.555091   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cde0 p=0x7f97856540 
10-17 14:46:18.555153   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:46:18.555179   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:18.555227  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:18.555319  1450  1606 D RILJ    : [9521]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:18.556190   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:18.559390  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:18.559533  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:18.574275  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.577042  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.577560  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.605900  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.607036  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.614884  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.637039  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.637211  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.645719  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:18.647743  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:18.648101  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:18.658181  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:18.658899  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:18.663273  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:18.666461  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:18.666660  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:18.967571   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e435a0 
10-17 14:46:18.967647   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e434e0
10-17 14:46:18.967676   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e434f0
10-17 14:46:18.970853   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e435a0 reset to NULL
10-17 14:46:18.970970   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e435a0
10-17 14:46:18.971002   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e435b0
10-17 14:46:20.456228  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:20.459498  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:20.459938  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:20.493430  1450  1683 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:20.494291  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:20.502343  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:20.515652  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:46:20.515964  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:20.538150   721   760 I RILC    : NUMBER:1
10-17 14:46:20.538220   721   760 I RILC    : arg len:14
10-17 14:46:20.538255   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:20.538377   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:20.538450   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978567e0 dispatched to RIL_CMD_PROXY_1
10-17 14:46:20.538575   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:20.538584   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:20.538630   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:20.538626   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:20.538678   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:20.538664   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978567e0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:20.538704   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:20.538728   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:20.538746   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:20.538764   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:20.538771   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:20.538794   721   751 D RIL     : radioState:10
10-17 14:46:20.538811   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:20.538836   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:20.538840   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:20.538884   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:20.538894   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:20.538910   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:20.538926   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:20.538953   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:20.538950   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:20.538983   721   751 I AT      : AT write start
10-17 14:46:20.538983   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:20.539032   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:20.539058   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:20.539132   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:20.539167   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:20.539215   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:20.539240   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:20.539280   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:20.539306   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:20.539351   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:20.539383   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:20.539692   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:20.539774   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:20.539837   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:20.539980   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:20.544782   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:20.544889   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:20.545044   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:20.545085   721   768 I AT      : AT read end: 40
10-17 14:46:20.545115   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:20.545138   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:20.545174   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:20.545189   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:20.545223   721   768 I AT      : AT read start
10-17 14:46:20.545233   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:20.545310   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:20.545359   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:20.545481   721   768 I AT      : AT read end: 6
10-17 14:46:20.545529   721   768 D AT      : AT< OK
10-17 14:46:20.545559   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:20.545606   721   768 I AT      : AT read start
10-17 14:46:20.545685   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:20.545730   721   751 D RIL     : requestQueryThermal success
10-17 14:46:20.545768   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:20.545802   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:20.545848   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:20.545932   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f978567e0 
10-17 14:46:20.545985   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda8a0
10-17 14:46:20.546024   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:20.801562  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:20.804326  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:20.804666  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:20.931711  1450 20008 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:20.979721  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:20.988527  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:20.996058  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:21.029289  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:21.029466  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:21.734808  1450  1450 D RILJ    : [9522]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:21.737265   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:21.737356   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda960, pRI=0x7f9784c360, p=0x7f97856930, pUCI=0x0
10-17 14:46:21.737393   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856930 dispatched to RIL_ATCI_PROXY
10-17 14:46:21.737491   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:21.737502   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:21.737529   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:21.737529   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:21.737559   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:21.737589   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:21.737598   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:21.737634   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:21.737637   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:21.737663   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:21.737705   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:21.737715   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:21.737728   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:21.737772   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:21.737829   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:21.737853   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:21.737860   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:21.737891   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856930 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:21.737895   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:21.737925   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:21.737955   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:21.737949   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:21.737970   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:21.737982   721   753 D RIL     : radioState:10
10-17 14:46:21.737985   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:21.738023   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:21.738028   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:21.738030   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:21.738054   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:21.738078   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:21.738100   721   753 I AT      : AT write start
10-17 14:46:21.738134   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:21.738263   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:21.738320   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:21.738370   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:21.738456   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:21.745961   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:21.746041   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:21.746112   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:21.746155   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:21.746261   721   770 I AT      : AT read end: 6
10-17 14:46:21.746311   721   770 D AT      : AT< OK
10-17 14:46:21.746342   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:21.746391   721   770 I AT      : AT read start
10-17 14:46:21.746462   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:21.746496   721   753 D RIL     : p_response->success = 1
10-17 14:46:21.746522   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:21.746544   721   753 D RIL     : strLength = 6
10-17 14:46:21.746567   721   753 D RIL     : line = <
10-17 14:46:21.746567   721   753 D RIL     : OK
10-17 14:46:21.746567   721   753 D RIL     : >
10-17 14:46:21.746595   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:21.746641   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:21.746720   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97856930 
10-17 14:46:21.746755   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda960
10-17 14:46:21.746787   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:21.746965  1450  1606 D RILJ    : [9522]< OEM_HOOK_RAW [B@bf070f0 [SUB0]
10-17 14:46:22.454849   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185158/0
10-17 14:46:23.035167  1450  1450 D RILJ    : [9523]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:23.038209   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:23.038275   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9100, pRI=0x7f9784c6f0, p=0x7f978569a0, pUCI=0x0
10-17 14:46:23.038309   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978569a0 dispatched to RIL_ATCI_PROXY
10-17 14:46:23.038421   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:23.038469   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:23.038475   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:23.038502   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:23.038502   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978569a0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:23.038538   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:23.038545   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:23.038569   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:23.038573   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:23.038594   721   753 D RIL     : radioState:10
10-17 14:46:23.038636   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:23.038645   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:23.038632   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:23.038679   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:23.038706   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.038733   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:23.038756   721   753 I AT      : AT write start
10-17 14:46:23.038779   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:23.038779   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:23.038809   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:23.038858   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:23.038872   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:23.038882   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:23.038934   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:23.038731   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:23.038979   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:23.039028   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:23.039039   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:23.039053   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:23.039092   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:23.039152   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:23.039208   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:23.039261   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:23.039352   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:23.039428   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:23.039595   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:23.047053   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:23.047163   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:23.047251   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:23.047303   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.047501   721   770 I AT      : AT read end: 6
10-17 14:46:23.047560   721   770 D AT      : AT< OK
10-17 14:46:23.047590   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:23.047642   721   770 I AT      : AT read start
10-17 14:46:23.047737   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.047775   721   753 D RIL     : p_response->success = 1
10-17 14:46:23.047806   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:23.047831   721   753 D RIL     : strLength = 6
10-17 14:46:23.047858   721   753 D RIL     : line = <
10-17 14:46:23.047858   721   753 D RIL     : OK
10-17 14:46:23.047858   721   753 D RIL     : >
10-17 14:46:23.047899   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:23.047956   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.048045   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f978569a0 
10-17 14:46:23.048093   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9100
10-17 14:46:23.048121   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:23.048479  1450  1606 D RILJ    : [9523]< OEM_HOOK_RAW [B@1696669 [SUB0]
10-17 14:46:23.368795   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:46:23.368877   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:23.368950   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:46:23.368991   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.369099   721   765 I AT      : AT read end: 37
10-17 14:46:23.369145   721   765 D AT      : AT< +ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369175   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369213   721   765 D RIL     : Nw URC:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:23.369274   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:23.369309   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:23.369343   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.369400   721   765 I AT      : AT read start
10-17 14:46:23.369654  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:23.369814  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:46:23.369896  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.370070  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370195  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.370253  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.370287  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370328  1450  1450 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.370358  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.370455  1450  1450 D GsmSST  : [GsmSST0] notifySignalStrength: mSignalStrength.getLevel=4
10-17 14:46:23.370721  1450  1450 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1 sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad}
10-17 14:46:23.371318   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: subId=1 signalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.371410   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: logSSC.length=5 next=2
10-17 14:46:23.371809   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144005Europe/Samara(1,290,14400,0,1476700805) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372225   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372601   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.372938   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.373265   909   920 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:23.373337   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: ----------------
10-17 14:46:23.374388   909   920 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:23.374472   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: valid phoneId=0
10-17 14:46:23.374518   909   920 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:23.374658   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.374767   909   920 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:23.374916   909   920 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:23.375166   909   920 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:23.375408   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375551   909   920 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.375575  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375604   909   920 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.375634   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375665  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.375673   909   920 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.375703   909   920 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375707  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.375738  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375776  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.375801  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375901  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.375946  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:23.376038  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376101  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.376140  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.376169  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376206  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:46:23.376231  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376311  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376372  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.376418  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.376446  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376482  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.376508  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376536  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376577  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.376921  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.376990  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:23.377040  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:23.377068  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.377112  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:23.377140  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:23.377933  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:23.843563  1450  1450 D RILJ    : [9524]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:23.845473   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:23.845560   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaaa0, pRI=0x7f9784c870, p=0x7f97856ee0, pUCI=0x0
10-17 14:46:23.845597   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c870 p=0x7f97856ee0 dispatched to RIL_ATCI_PROXY
10-17 14:46:23.845699   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:23.845702   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:23.845704   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:23.845736   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:23.845743   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:23.845778   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:23.845785   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:23.845789   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:23.845802   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:23.845828   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:23.845859   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:23.845861   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:23.845890   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:23.845929   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:23.845983   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:23.846011   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:23.846053   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:23.846075   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:23.846104   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:23.846150   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:23.846154   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:23.846210   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:23.846245   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c870 p=0x7f97856ee0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:23.846264   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:23.846276   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:23.846309   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:23.846333   721   753 D RIL     : radioState:10
10-17 14:46:23.846374   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:23.846404   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.846433   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:23.846457   721   753 I AT      : AT write start
10-17 14:46:23.846569   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:23.846604   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:23.846655   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:23.846703   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:23.846784   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:23.854391   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:23.854472   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:23.854544   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:23.854586   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:23.854704   721   770 I AT      : AT read end: 6
10-17 14:46:23.854746   721   770 D AT      : AT< OK
10-17 14:46:23.854776   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:23.854816   721   770 I AT      : AT read start
10-17 14:46:23.854854   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:23.854889   721   753 D RIL     : p_response->success = 1
10-17 14:46:23.854917   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:23.854942   721   753 D RIL     : strLength = 6
10-17 14:46:23.854965   721   753 D RIL     : line = <
10-17 14:46:23.854965   721   753 D RIL     : OK
10-17 14:46:23.854965   721   753 D RIL     : >
10-17 14:46:23.854992   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:23.855038   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:23.855112   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c870 p=0x7f97856ee0 
10-17 14:46:23.855144   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:46:23.855177   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:23.855373  1450  1606 D RILJ    : [9524]< OEM_HOOK_RAW [B@54ac8ee [SUB0]
10-17 14:46:24.292306  1450  1450 D RILJ    : [9525]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:24.295293   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:24.295415   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9140, pRI=0x7f9784c210, p=0x7f97856fc0, pUCI=0x0
10-17 14:46:24.295451   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856fc0 dispatched to RIL_ATCI_PROXY
10-17 14:46:24.295566   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.295582   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:24.295583   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.295608   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.295640   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.295644   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.295650   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:24.295685   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.295690   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.295692   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.295723   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.295761   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.295775   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.295785   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.295824   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:24.295844   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.295860   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856fc0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:24.295864   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.295875   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.295896   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.295916   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.295917   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.295935   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:24.295947   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.295962   721   753 D RIL     : radioState:10
10-17 14:46:24.295981   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.296009   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:24.296046   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:24.296071   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:24.296093   721   753 I AT      : AT write start
10-17 14:46:24.296233   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.296284   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.296287   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.296348   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.296404   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:24.296492   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:24.304107   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:24.304197   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:24.304271   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:24.304314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.304445   721   770 I AT      : AT read end: 6
10-17 14:46:24.304487   721   770 D AT      : AT< OK
10-17 14:46:24.304515   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:24.304566   721   770 I AT      : AT read start
10-17 14:46:24.304795   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:24.304865   721   753 D RIL     : p_response->success = 1
10-17 14:46:24.304896   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:24.304921   721   753 D RIL     : strLength = 6
10-17 14:46:24.304948   721   753 D RIL     : line = <
10-17 14:46:24.304948   721   753 D RIL     : OK
10-17 14:46:24.304948   721   753 D RIL     : >
10-17 14:46:24.304977   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:24.305027   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:24.305125   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f97856fc0 
10-17 14:46:24.305162   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9140
10-17 14:46:24.305191   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.305472  1450  1606 D RILJ    : [9525]< OEM_HOOK_RAW [B@24418f [SUB0]
10-17 14:46:24.624216  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:24.626443  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:46:24.626621  1450  1450 D RILJ    : [9526]> SCREEN_STATE: false [SUB0]
10-17 14:46:24.629158  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:24.629966  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:46:24.630009   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:24.630083   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6a60, pRI=0x7f9784c240, p=0x7f978570a0, pUCI=0x0
10-17 14:46:24.630121   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c240 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:24.630152  1450  1450 D RILJ    : [9527]> SCREEN_STATE: false [SUB1]
10-17 14:46:24.630284   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.630309   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.630324   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.630366   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.630373   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.630375   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.630394   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.630425   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.630433   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.630437   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.630465   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.630511   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.630662   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:24.630705   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:24.630740   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c240 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:24.630776   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.630821   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:24.630852   721   749 D RIL     : radioState:10
10-17 14:46:24.630998   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.631054   721   749 D AT      : AT> AT+CREG=1
10-17 14:46:24.631084   721   749 I AT      : AT write start
10-17 14:46:24.631074   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.631407   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.631479   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.631591   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.631638   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.631703   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.631763   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.631899   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:24.632026   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.632083   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.632144   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.632179   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.632294   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.632378   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.634070   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:24.634153   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cc3ee0, pRI=0x7f9784c7b0, p=0x7f97857110, pUCI=0x0
10-17 14:46:24.634186   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c7b0 p=0x7f97857110 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:24.634307   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:24.634346   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:24.634383   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:24.634392   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:24.634411   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:24.634450   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:24.634454   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:24.634479   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:24.634515   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:24.634603   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:24.634633   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:24.634705   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:24.634739   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:24.634785   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:24.634832   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c7b0 p=0x7f97857110 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:24.634865   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:24.634896   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:24.634922   721   755 D RIL     : radioState:0
10-17 14:46:24.634970   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.634997   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.635022   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:24.635089   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.635118   721   755 D AT      : AT> AT+CREG=1
10-17 14:46:24.635141   721   755 I AT      : AT write start
10-17 14:46:24.635212   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:24.635255   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:24.635303   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:24.635338   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:24.635390   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:24.635402   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.635417   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:24.635459   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.635516   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.635602   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:24.635711   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:24.635746   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:24.639541   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.639642   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.639721   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.639768   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.640249   721   766 I AT      : AT read end: 6
10-17 14:46:24.640334   721   766 D AT      : AT< OK
10-17 14:46:24.640372   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.640419   721   766 I AT      : AT read start
10-17 14:46:24.640652   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.640721   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.640802   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.640849   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.641074   721   772 I AT      : AT read end: 6
10-17 14:46:24.641149   721   772 D AT      : AT< OK
10-17 14:46:24.641182   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.641231   721   772 I AT      : AT read start
10-17 14:46:24.640497   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.641332   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.641363   721   749 D AT      : AT> AT+CGREG=1
10-17 14:46:24.641386   721   749 I AT      : AT write start
10-17 14:46:24.641568   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.641649   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.641705   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.641805   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:24.642448   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.642553   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.642595   721   755 D AT      : AT> AT+CGREG=1
10-17 14:46:24.642621   721   755 I AT      : AT write start
10-17 14:46:24.642820   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.642883   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.642933   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.643015   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:24.643360   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.643432   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.643500   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.643542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.643645   721   766 I AT      : AT read end: 6
10-17 14:46:24.643697   721   766 D AT      : AT< OK
10-17 14:46:24.643725   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.643763   721   766 I AT      : AT read start
10-17 14:46:24.643804   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.643846   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.643871   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:46:24.643893   721   749 I AT      : AT write start
10-17 14:46:24.644030   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.644084   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.644131   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.644281   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:24.644361   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.644407   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.644468   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.644510   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.644604   721   772 I AT      : AT read end: 6
10-17 14:46:24.644644   721   772 D AT      : AT< OK
10-17 14:46:24.644673   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.644711   721   772 I AT      : AT read start
10-17 14:46:24.644748   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.644793   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.644827   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:46:24.644851   721   755 I AT      : AT write start
10-17 14:46:24.644983   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.645048   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.645097   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.645174   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:24.645441   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.645507   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.645571   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.645611   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.645721   721   766 I AT      : AT read end: 6
10-17 14:46:24.645761   721   766 D AT      : AT< OK
10-17 14:46:24.645790   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.645830   721   766 I AT      : AT read start
10-17 14:46:24.645870   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.645907   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.645947   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:46:24.645971   721   749 I AT      : AT write start
10-17 14:46:24.646090   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.646139   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.646185   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.646362   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:24.646438   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.646482   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.646542   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.646581   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.646679   721   772 I AT      : AT read end: 6
10-17 14:46:24.646718   721   772 D AT      : AT< OK
10-17 14:46:24.646748   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.646786   721   772 I AT      : AT read start
10-17 14:46:24.646836   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.646877   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.646904   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:46:24.646927   721   755 I AT      : AT write start
10-17 14:46:24.647085   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.647149   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.647198   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.647499   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.647551   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.647612   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.647650   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.647958   721   766 I AT      : AT read end: 6
10-17 14:46:24.648017   721   766 D AT      : AT< OK
10-17 14:46:24.648045   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.648080   721   766 I AT      : AT read start
10-17 14:46:24.648121   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.648169   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.648197   721   749 D AT      : AT> AT+CEREG=1
10-17 14:46:24.648220   721   749 I AT      : AT write start
10-17 14:46:24.648350   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.648407   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.651176   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:24.651268   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:24.651343   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:24.658387   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.658465   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.658533   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.658576   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.658693   721   772 I AT      : AT read end: 6
10-17 14:46:24.658736   721   772 D AT      : AT< OK
10-17 14:46:24.658791   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.658840   721   772 I AT      : AT read start
10-17 14:46:24.658874   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.658926   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.658954   721   755 D AT      : AT> AT+CEREG=1
10-17 14:46:24.658945   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:24.658983   721   755 I AT      : AT write start
10-17 14:46:24.659001   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:24.659058   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:24.659098   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.659112   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:24.659154   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:24.659179   721   766 I AT      : AT read end: 6
10-17 14:46:24.659197   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:24.659208   721   766 D AT      : AT< OK
10-17 14:46:24.659235   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:24.659270   721   766 I AT      : AT read start
10-17 14:46:24.659274   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:24.659309   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:24.659354   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:24.659395   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:24.659461   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f978570a0 
10-17 14:46:24.659492   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a60
10-17 14:46:24.659516   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:24.659629  1450  1606 D RILJ    : [9526]< SCREEN_STATE  [SUB0]
10-17 14:46:24.660341   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:24.660411   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:24.660483   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:24.660527   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:24.660643   721   772 I AT      : AT read end: 6
10-17 14:46:24.660694   721   772 D AT      : AT< OK
10-17 14:46:24.660725   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:24.660772   721   772 I AT      : AT read start
10-17 14:46:24.660810   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:24.660849   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:24.660889   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:24.661366   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97857110 
10-17 14:46:24.661407   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:46:24.661433   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:24.661517  1450  1609 D RILJ    : [9527]< SCREEN_STATE  [SUB1]
10-17 14:46:25.083759  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.086306  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.086662  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.124822  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.125307  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.128517  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.147066  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.151630  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.249932  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.254609  1450  4234 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.254959  1450  4234 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.272597  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:25.274609  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.274679  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:25.294463  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.295940  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.296576   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.296678  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.296866   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.297792  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.297897  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:25.299468   909  6090 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.299741   909  6090 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.300538  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:46:25.302054  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:46:25.302204  1450  1450 D RILJ    : [9528]> SCREEN_STATE: true [SUB0]
10-17 14:46:25.304649  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:46:25.304995   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:46:25.305087   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6160, pRI=0x7f9784cb10, p=0x7f978571f0, pUCI=0x0
10-17 14:46:25.305126   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb10 p=0x7f978571f0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.305257   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.305298   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.305326   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.305340   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.305358   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.305396   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.305408   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.305423   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.305467   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.305473   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.305494   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.305562   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.305606   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.305608   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.305646   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.305688   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.305714   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.305821   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.305861   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.305897   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cb10 p=0x7f978571f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.305933   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.305931   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.305962   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.305969   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:25.305995   721   749 D RIL     : radioState:10
10-17 14:46:25.306004   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.306030   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.306056   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.306066   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.306084   721   749 D AT      : AT> AT+CREG=3
10-17 14:46:25.306110   721   749 I AT      : AT write start
10-17 14:46:25.306366  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:46:25.306489  1450  1450 D RILJ    : [9529]> SCREEN_STATE: true [SUB1]
10-17 14:46:25.306719   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.306786   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.306839   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.306931   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.309181  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.309371  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:25.309514  1450  1450 D RILJ    : [9530]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:25.311735   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:46:25.311831   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9240, pRI=0x7f9784c150, p=0x7f97857340, pUCI=0x0
10-17 14:46:25.311866   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857340 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.311982   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.312020   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.312064   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.312078   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.312090   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.312130   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.312151   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.312166   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.312209   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.312249   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.312253   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.312282   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.312284   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.312325   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857340 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.312358   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.312389   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:46:25.312415   721   755 D RIL     : radioState:0
10-17 14:46:25.312460   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312487   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312513   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.312566   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.312594   721   755 D AT      : AT> AT+CREG=3
10-17 14:46:25.312620   721   755 I AT      : AT write start
10-17 14:46:25.312730   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.312762   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.312805   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.312830   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.312880   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.312905   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.313035   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.313102   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.313154   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.313247   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:25.313427   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.313469   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.313519   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.314582   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:46:25.314655   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:25.314761   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:46:25.314808   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.314860   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.314902   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.314954   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.314995   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.315144   721   765 I AT      : AT read end: 36
10-17 14:46:25.315194   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315224   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315270   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.315311   721   765 D RIL     : NW state changed: normal case
10-17 14:46:25.315341   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:46:25.315372   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.315400   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:46:25.315455   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:46:25.315494   721   765 D RIL     : bCREGType3Support=1
10-17 14:46:25.315523   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:25.315548   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:46:25.315772   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:25.315850   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.315916   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e436c0
10-17 14:46:25.315955   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e436d0
10-17 14:46:25.316032   721   765 I AT      : AT read start
10-17 14:46:25.316158   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:46:25.316171  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:46:25.316222   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:46:25.316302   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:46:25.316347   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.316406   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.316448   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.316504   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.316541   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.316674   721   771 I AT      : AT read end: 36
10-17 14:46:25.316718   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316751   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316794   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:46:25.316829   721   771 D RIL     : NW state changed: normal case
10-17 14:46:25.316858   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:46:25.316888   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:46:25.316916   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:46:25.316970   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:46:25.317005   721   771 D RIL     : bCREGType3Support=1
10-17 14:46:25.317036   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:46:25.317061   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:46:25.317139   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:46:25.317167   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.317224   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e436c0, cancel
10-17 14:46:25.317257   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43660
10-17 14:46:25.317292   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43670
10-17 14:46:25.317349   721   771 I AT      : AT read start
10-17 14:46:25.317420   721   772 I AT      : AT read end: 6
10-17 14:46:25.317446   721   772 D AT      : AT< OK
10-17 14:46:25.317473   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.317509   721   772 I AT      : AT read start
10-17 14:46:25.318867   721   766 I AT      : AT read end: 6
10-17 14:46:25.318936   721   766 D AT      : AT< OK
10-17 14:46:25.318966   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.319011   721   766 I AT      : AT read start
10-17 14:46:25.319062   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.319123   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.319150   721   749 D AT      : AT> AT+CGREG=3
10-17 14:46:25.319175   721   749 I AT      : AT write start
10-17 14:46:25.319358   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.319419   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.319470   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.319577   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.320460  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:46:25.321053   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.321155   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.321186   721   755 D AT      : AT> AT+CGREG=3
10-17 14:46:25.321212   721   755 I AT      : AT write start
10-17 14:46:25.321395   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.321458   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.321511   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.321613   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:25.321950  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:25.322072  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:46:25.322230  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:25.322855   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:25.322938   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cf9360, pRI=0x7f9784c540, p=0x7f978573b0, pUCI=0x0
10-17 14:46:25.322974   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.323078   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.323112   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.323146   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.323156   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.323174   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.323220   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.323217   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.323248   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.323454   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.323519   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.323544   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.323593   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.323619   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.323689   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.323715   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.323756   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.323769   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.323827   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.323854   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.324087   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.325979  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:46:25.326151  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:46:25.326304  1450  1450 D RILJ    : [9531]> OPERATOR [SUB0]
10-17 14:46:25.329184   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.329271   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.329352   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.329394   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.329444   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.329484   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.329539   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.329580   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.329720   721   766 I AT      : AT read end: 6
10-17 14:46:25.329720   721   772 I AT      : AT read end: 6
10-17 14:46:25.329782   721   766 D AT      : AT< OK
10-17 14:46:25.329783   721   772 D AT      : AT< OK
10-17 14:46:25.329816   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.329816   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.329872   721   772 I AT      : AT read start
10-17 14:46:25.329883   721   766 I AT      : AT read start
10-17 14:46:25.329971   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.329995   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.330009   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.330036   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:46:25.330036   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.330063   721   755 I AT      : AT write start
10-17 14:46:25.330066   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:46:25.330093   721   749 I AT      : AT write start
10-17 14:46:25.331096   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.331198   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.331258   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.331270   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.331316   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.331343   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:46:25.331593   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.331764   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.332213  1450  1450 D RILJ    : [9532]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:46:25.332634   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:46:25.332735   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9340, pRI=0x7f9784c660, p=0x7f97857490, pUCI=0x0
10-17 14:46:25.332778   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.332811   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.332851   721   760 D RILC-MTK: Request pRI=0x7f9784c660 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:46:25.335003  1450  1450 D RILJ    : [9533]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:46:25.335418   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:25.335492   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9b80, pRI=0x7f9784cb40, p=0x7f97857570, pUCI=0x0
10-17 14:46:25.335530   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.335560   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.335596   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.335629   721   760 D RILC-MTK: Request pRI=0x7f9784cb40 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:46:25.339199   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.339297   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.339491   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.339542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.339548   721   772 I AT      : AT read end: 6
10-17 14:46:25.339593   721   772 D AT      : AT< OK
10-17 14:46:25.339595   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.339630   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.339641   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.339679   721   772 I AT      : AT read start
10-17 14:46:25.339702   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.339735   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.339746   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.339784   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.339826   721   755 D AT      : AT> AT+ECSQ
10-17 14:46:25.339853   721   755 I AT      : AT write start
10-17 14:46:25.339986   721   766 I AT      : AT read end: 6
10-17 14:46:25.340016   721   766 D AT      : AT< OK
10-17 14:46:25.340015   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.340048   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.340064   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.340088   721   766 I AT      : AT read start
10-17 14:46:25.340110   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.340132   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.340179   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.340205   721   749 D AT      : AT> AT+ECSQ
10-17 14:46:25.340206   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:46:25.340233   721   749 I AT      : AT write start
10-17 14:46:25.340381   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.340436   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.340486   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.340581   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:46:25.340750   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:25.340818   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9c20, pRI=0x7f9784cb70, p=0x7f97857730, pUCI=0x0
10-17 14:46:25.340854   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.340884   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.341036   721   760 D RILC-MTK: 3:DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.341067   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.341099   721   760 D RILC-MTK: Request pRI=0x7f9784cb70 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:46:25.341540  1450  1450 D RILJ    : [9534]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:46:25.342403   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:46:25.342493   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.342567   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:46:25.342609   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.342656   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.342699   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.342744   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.342781   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.342892   721   772 I AT      : AT read end: 42
10-17 14:46:25.342939   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:25.342972   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:46:25.343006   721   772 D AT      : AT< OK
10-17 14:46:25.343031   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.343077   721   772 I AT      : AT read start
10-17 14:46:25.343138   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.343193   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:46:25.343228   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:46:25.343269   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.343296   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:46:25.343319   721   755 I AT      : AT write start
10-17 14:46:25.343485   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.343488   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:46:25.343550   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.343556   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.343604   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.343625   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:46:25.343667   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.343686   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:46:25.343717   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.343757   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.343802   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.343839   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.343954   721   766 I AT      : AT read end: 43
10-17 14:46:25.343995   721   766 D AT      : AT< +ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:25.344025   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 40,99,-282,1,1,1,1,3,32767
10-17 14:46:25.344061   721   766 D AT      : AT< OK
10-17 14:46:25.344094   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.344139   721   766 I AT      : AT read start
10-17 14:46:25.344544   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.344586  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.344702  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:46:25.344713   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:25.344782  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:46:25.344786   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:25.344833   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.344856  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:46:25.344911  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:46:25.344912   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.344946   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:46:25.344971   721   749 I AT      : AT write start
10-17 14:46:25.345163   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.345240   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.345241   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:25.345307   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9c40, pRI=0x7f9784cc60, p=0x7f978578f0, pUCI=0x0
10-17 14:46:25.345320   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.345343   721   760 D RILC-MTK: 1:RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345362   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.345376   721   760 D RILC-MTK: 2:OPERATOR pRI=0x7f9784c660 p=0x7f97857490 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345406   721   760 D RILC-MTK: 3:DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345434   721   760 D RILC-MTK: 4:VOICE_REGISTRATION_STATE pRI=0x7f9784cb70 p=0x7f97857730 is queued in RIL_CMD_PROXY_3
10-17 14:46:25.345464   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:46:25.345459   721   772 I AT      : AT read end: 6
10-17 14:46:25.345500   721   772 D AT      : AT< OK
10-17 14:46:25.345500   721   760 D RILC-MTK: Request pRI=0x7f9784cc60 to RIL_CMD_PROXY_3 is busy. total:5 requests pending
10-17 14:46:25.345533   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.345574   721   772 I AT      : AT read start
10-17 14:46:25.345639   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.345689   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.345739   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.345828   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:46:25.345912   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.345968   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.345995   721   755 D AT      : AT> AT+CEREG=3
10-17 14:46:25.346019   721   755 I AT      : AT write start
10-17 14:46:25.346334   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.346410   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.346465   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.346556   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:46:25.346653  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.346750  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.346866  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:46:25.346923  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:46:25.347050  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:25.347110  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:46:25.347185  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:46:25.347220  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:46:25.347253  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:46:25.347290  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:46:25.347323  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:46:25.347453  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:25.347477   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.347540   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.347579  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:46:25.347626   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.347648  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:46:25.347668   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.347696  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:46:25.347825   721   766 I AT      : AT read end: 6
10-17 14:46:25.347865   721   766 D AT      : AT< OK
10-17 14:46:25.347894   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.347940   721   766 I AT      : AT read start
10-17 14:46:25.347941   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.347995   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.348060   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.348101   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.348193   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.348257   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.348264  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:46:25.348285   721   749 D AT      : AT> AT+CEREG=3
10-17 14:46:25.348308   721   749 I AT      : AT write start
10-17 14:46:25.348459   721   772 I AT      : AT read end: 6
10-17 14:46:25.348498   721   772 D AT      : AT< OK
10-17 14:46:25.348493   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.348536   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.348549   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.348580   721   772 I AT      : AT read start
10-17 14:46:25.348608   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.348698   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.348781   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.348822   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.348866   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.348951   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f97857340 
10-17 14:46:25.348987   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:46:25.349019   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.349264  1450  1609 D RILJ    : [9529]< SCREEN_STATE  [SUB1]
10-17 14:46:25.350731   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.350794   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.350875   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.351140   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.351139   721   766 I AT      : AT read end: 6
10-17 14:46:25.351191   721   766 D AT      : AT< OK
10-17 14:46:25.351222   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.351274   721   766 I AT      : AT read start
10-17 14:46:25.351318   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.351360   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.351402   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.351479   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f978571f0 
10-17 14:46:25.351511   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6160
10-17 14:46:25.351547   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.351580   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c540 p=0x7f978573b0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.351612   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.351641   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:25.351665   721   749 D RIL     : radioState:10
10-17 14:46:25.351680  1450  1606 D RILJ    : [9528]< SCREEN_STATE  [SUB0]
10-17 14:46:25.351706   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:25.351743   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:46:25.351774   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.351800   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:46:25.351827   721   749 I AT      : AT write start
10-17 14:46:25.352053   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.352128   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.352181   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.352270   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.352637  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.352763  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.352824  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:46:25.353211   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.353288   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.353356   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.353398   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.353663   721   766 I AT      : AT read end: 6
10-17 14:46:25.353723   721   766 D AT      : AT< OK
10-17 14:46:25.353756   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.353807   721   766 I AT      : AT read start
10-17 14:46:25.353867   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.353908   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.353958   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.354002  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:46:25.354045   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c540 p=0x7f978573b0 
10-17 14:46:25.354083   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9360
10-17 14:46:25.354113   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.354145   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784c660 p=0x7f97857490 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.354161  1450  1450 D RILJ    : [9535]> OPERATOR [SUB1]
10-17 14:46:25.354174   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.354167  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:25.354208   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:25.354233   721   749 D RIL     : radioState:10
10-17 14:46:25.354243  1450  1606 D RILJ    : [9530]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:25.354270   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.354304   721   749 D AT      : AT> AT+COPS?
10-17 14:46:25.354331   721   749 I AT      : AT write start
10-17 14:46:25.355882   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.355944   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.355995   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.356088   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.356755   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:46:25.356832   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9c60, pRI=0x7f9784ce10, p=0x7f97857dc0, pUCI=0x0
10-17 14:46:25.356866   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784ce10 p=0x7f97857dc0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.356985   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.357021   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.357066   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.357072   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.357097   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.357143   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.357150   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.357171   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.357216   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.357206   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.357245   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.357281   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.357334   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.357359   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.357402   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.357428   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.357467   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.357484   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.357528   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.357559   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.357592   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784ce10 p=0x7f97857dc0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.357621   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.357652   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:46:25.357679   721   755 D RIL     : radioState:0
10-17 14:46:25.357719   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357748   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357773   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357799   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.357834   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.357861   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.357905   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.357964   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce10 p=0x7f97857dc0 
10-17 14:46:25.357996   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c60
10-17 14:46:25.358023   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.358072   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.358126   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.358536  1450  1609 D RilRequest: [9535]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.361113  1450  1450 D RILJ    : [9536]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:46:25.363976   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:25.364063   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.364145   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:25.364191   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.364244   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.364297   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.364348   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.364387   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.364534   721   766 I AT      : AT read end: 30
10-17 14:46:25.364601   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:25.364636   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:25.364672   721   766 D AT      : AT< OK
10-17 14:46:25.364705   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.364749   721   766 I AT      : AT read start
10-17 14:46:25.365382   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.365480   721   749 D RIL     : Get operator code 25020
10-17 14:46:25.365517   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:46:25.365557   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:46:25.365587   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.365650   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.365733   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c660 p=0x7f97857490 
10-17 14:46:25.365781   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:46:25.365824   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.365860   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cb40 p=0x7f97857570 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.365893   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.365925   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.365952   721   749 D RIL     : radioState:10
10-17 14:46:25.366003   721   749 D RIL     : request gprs reg state: normal case
10-17 14:46:25.366002  1450  1606 D RILJ    : [9531]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:46:25.366046   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.366075   721   749 D AT      : AT> AT+CGREG?
10-17 14:46:25.366099   721   749 I AT      : AT write start
10-17 14:46:25.366287   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.366358   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.366412   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.366502   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:46:25.374140   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:46:25.374235   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.374309   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:46:25.374356   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.374462   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.374488   721   766 I AT      : AT read end: 44
10-17 14:46:25.374514   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.374534   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:25.374565   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:46:25.374577   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.374604   721   766 I AT      : AT read start
10-17 14:46:25.374617   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.374691   721   766 I AT      : AT read end: 6
10-17 14:46:25.374719   721   766 D AT      : AT< OK
10-17 14:46:25.374746   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.374784   721   766 I AT      : AT read start
10-17 14:46:25.374848   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.374911   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.374941   721   749 E RIL     : The value in the field <lac> :0
10-17 14:46:25.374968   721   749 D RIL     : cid: 3583
10-17 14:46:25.374993   721   749 E RIL     : The value of act: 3
10-17 14:46:25.375017   721   749 D RIL     : cause_type: 0
10-17 14:46:25.375041   721   749 D RIL     : reject_cause: 0
10-17 14:46:25.375078   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.375104   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:46:25.375127   721   749 I AT      : AT write start
10-17 14:46:25.375273   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.375334   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.375387   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.375476   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:46:25.377114   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:46:25.377198   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.377270   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:46:25.377314   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.377526   721   766 I AT      : AT read end: 19
10-17 14:46:25.377584   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:46:25.377618   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:46:25.377651   721   766 I AT      : AT read start
10-17 14:46:25.377767   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.377830   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.377901   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.377942   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.378103   721   766 I AT      : AT read end: 6
10-17 14:46:25.378148   721   766 D AT      : AT< OK
10-17 14:46:25.378177   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.378222   721   766 I AT      : AT read start
10-17 14:46:25.378378   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.378453   721   749 E RIL     : rid: 0
10-17 14:46:25.378484   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:25.378515   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:25.378543   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:25.378568   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:25.378598   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.378656   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.378732   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb40 p=0x7f97857570 
10-17 14:46:25.378771   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:46:25.378802   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.378833   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cb70 p=0x7f97857730 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.378861   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.378888   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.378915   721   749 D RIL     : radioState:10
10-17 14:46:25.378951   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.378979   721   749 D AT      : AT> AT+CREG?
10-17 14:46:25.378959  1450  1606 D RILJ    : [9532]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:46:25.379001   721   749 I AT      : AT write start
10-17 14:46:25.379186   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.379256   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.379310   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.379398   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.380112   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:46:25.380189   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.380271   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:46:25.380321   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.380431   721   766 I AT      : AT read end: 38
10-17 14:46:25.380475   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.380510   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:46:25.380544   721   766 I AT      : AT read start
10-17 14:46:25.380747   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.380809   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.380877   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.380990   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.381126   721   766 I AT      : AT read end: 6
10-17 14:46:25.381177   721   766 D AT      : AT< OK
10-17 14:46:25.381208   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.381248   721   766 I AT      : AT read start
10-17 14:46:25.381361   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.381422   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.381453   721   749 E RIL     : The value in the field <lac> :127
10-17 14:46:25.381480   721   749 D RIL     : cid: 3583
10-17 14:46:25.381506   721   749 E RIL     : The value of act: 3
10-17 14:46:25.381531   721   749 D RIL     : cause_type: 0
10-17 14:46:25.381556   721   749 D RIL     : reject_cause: 0
10-17 14:46:25.381610   721   749 E RIL     : rid: 0
10-17 14:46:25.381637   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:46:25.381670   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:46:25.381699   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:46:25.381725   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:46:25.381756   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:46:25.381790   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.381852   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.381938   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb70 p=0x7f97857730 
10-17 14:46:25.381971   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c20
10-17 14:46:25.382001   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.382032   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cc60 p=0x7f978578f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.382063   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.382092   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:25.382117   721   749 D RIL     : radioState:10
10-17 14:46:25.382154   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.382185   721   749 D AT      : AT> AT+COPS?
10-17 14:46:25.382181  1450  1606 D RILJ    : [9533]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:46:25.382214   721   749 I AT      : AT write start
10-17 14:46:25.382411   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.382484   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.382538   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.382633   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:46:25.384247   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:46:25.384333   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.384408   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:46:25.384452   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.384572   721   766 I AT      : AT read end: 24
10-17 14:46:25.384649   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:46:25.384747   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:46:25.384770   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.384790   721   766 I AT      : AT read start
10-17 14:46:25.384819   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.384883   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.384923   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.385011   721   766 I AT      : AT read end: 6
10-17 14:46:25.385041   721   766 D AT      : AT< OK
10-17 14:46:25.385068   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.385106   721   766 I AT      : AT read start
10-17 14:46:25.385156   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.385201   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.385247   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.385320   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc60 p=0x7f978578f0 
10-17 14:46:25.385360   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c40
10-17 14:46:25.385390   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.385478  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:46:25.385543  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:46:25.385622  1450  1606 D RILJ    : [9534]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:46:25.395330  1450  1450 D RILJ    : [9537]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:46:25.395532   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:46:25.395627   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9cc0, pRI=0x7f9784ce40, p=0x7f97856540, pUCI=0x0
10-17 14:46:25.395668   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856540 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.395772   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.395822   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.395862   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.395875   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.395875   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.395891   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.395931   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.395936   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.395962   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.395993   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.396028   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.396039   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.396074   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.396095   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.396110   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.396206   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.396236   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.396281   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.396330   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.396373   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.396425   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.396460   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.396500   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856540 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.396531   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.396563   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.396593   721   755 D RIL     : radioState:0
10-17 14:46:25.396642   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396669   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396696   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396722   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.396756   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.396804   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.396854   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.396924   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce40 p=0x7f97856540 
10-17 14:46:25.396958   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9cc0
10-17 14:46:25.396985   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.397039   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.397071   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.397193  1450  1450 D RILJ    : [9538]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:46:25.397192  1450  1609 D RilRequest: [9536]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.397236  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.397639   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:46:25.397747   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9ce0, pRI=0x7f9784c240, p=0x7f97856cb0, pUCI=0x0
10-17 14:46:25.397788   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97856cb0 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.397949   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.397950   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.397990   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.398040   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.398027   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.398030   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.398076   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.398117   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.398116   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.398148   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.398198   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.398212   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.398233   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.398248   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c240 p=0x7f97856cb0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.398281   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.398288   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.398310   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.398327   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:46:25.398347   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.398354   721   755 D RIL     : radioState:0
10-17 14:46:25.398399   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398408   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.398439   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398447   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.398472   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398488   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.398500   721   755 I RIL     : isWfcSupport: 0
10-17 14:46:25.398547   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:46:25.398576   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.398623   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.398681   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97856cb0 
10-17 14:46:25.398718   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9ce0
10-17 14:46:25.398744   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.398795   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.398822   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.398861   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.398904   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.398930   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.399541  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.399895  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.402599  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.402796  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:46:25.403307  1450  1609 D RilRequest: [9537]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:46:25.404493   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:46:25.404596   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cc36c0, pRI=0x7f9784c4b0, p=0x7f97856e70, pUCI=0x0
10-17 14:46:25.404640   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c4b0 p=0x7f97856e70 dispatched to RIL_CMD2_PROXY_3
10-17 14:46:25.404765   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.404822   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.404858   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.404868   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.404900   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.404957   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.404996   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.405023   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.405073   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.405100   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.405139   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.405168   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.405212   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.405219   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.405238   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.405282   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.405289   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.405311   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.405358   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.405363   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.405415   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.405441   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.405618   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.405690   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:46:25.405729   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c4b0 p=0x7f97856e70 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:46:25.405761   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.405795   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:46:25.405822   721   755 D RIL     : radioState:0
10-17 14:46:25.405863   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.405894   721   755 D AT      : AT> AT+COPS?
10-17 14:46:25.405918   721   755 I AT      : AT write start
10-17 14:46:25.406124   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.406205   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.406260   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:46:25.406356   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:46:25.406720  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:25.406876  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:25.406973  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:25.407015  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.407106  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:25.407155  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:46:25.407195  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.407251  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:46:25.407384  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:25.407434  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:46:25.408914  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.409013  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:46:25.409107  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:46:25.409153  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:46:25.413395  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.413501  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:46:25.413590  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:46:25.413640  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:46:25.413731  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:46:25.413786  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:46:25.414011   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:46:25.414096   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.414182   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:46:25.414247   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.414369   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:46:25.414400   721   772 I AT      : AT read end: 12
10-17 14:46:25.414431   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:46:25.414453   721   772 D AT      : AT< +COPS: 0
10-17 14:46:25.414490   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:46:25.414500   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:46:25.414534   721   772 I AT      : AT read start
10-17 14:46:25.414542   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.414633   721   772 I AT      : AT read end: 6
10-17 14:46:25.414663   721   772 D AT      : AT< OK
10-17 14:46:25.414692   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:46:25.414735   721   772 I AT      : AT read start
10-17 14:46:25.414799   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:46:25.414859   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:46:25.414919   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:46:25.415007   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f97856e70 
10-17 14:46:25.415058   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:46:25.415092   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.415186  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:46:25.415281  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:46:25.415365  1450  1609 D RILJ    : [9538]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:46:25.415468  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:46:25.415555  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:46:25.415661  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:46:25.423046  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.423194  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:46:25.423257  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:46:25.423386  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:46:25.423469  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:46:25.423513  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:25.423575  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:46:25.423610  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.423685  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:25.423763  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:46:25.423831  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:46:25.423914  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:46:25.423945  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:46:25.424104  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:46:25.424147  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:46:25.424189  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.424265  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:25.424317  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:46:25.426489  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:46:25.426617  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:46:25.426664  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:46:25.426798  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:46:25.426939  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:46:25.427372  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:25.427470  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:25.427543  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:46:25.427597  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:46:25.427737  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:46:25.427782  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:46:25.427842  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:46:25.427909  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.427958  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428002  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428054  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428097  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428142  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428183  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428224  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428266  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428309  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:46:25.428353  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:46:25.428390  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:46:25.428439  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:46:25.428498  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:46:25.429920  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:46:25.431433  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.431636  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:46:25.432533  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:46:25.433569  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:46:25.433
10-17 14:46:25.433791  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:46:25.434755  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.435054  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.435182  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:46:25.435261  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:46:25.435323  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.435648  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:46:25.436536   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.436674   909  1190 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.436858   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=3
10-17 14:46:25.437252   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144053Europe/Samara(1,290,14400,0,1476700853) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.437720   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.438228   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.438679   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439102   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144625Europe/Samara(1,290,14400,0,1476701185) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439205   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:46:25.439269   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.439427   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.439568   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.439760   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440049   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.440240   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440504   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.440718   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.440855   909  1190 D TelephonyRegistry: idMatch: rlt=true
10-17 14:46:25.441103   909  1190 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:46:25.442599   909  1190 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.443555  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.443729  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:46:25.443794  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:46:25.443837  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.443886  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:46:25.443915  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:46:25.447233  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.447612   909  1190 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.456103  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:46:25.456179  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:25.456267  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:46:25.456343  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.456378  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.456438  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:46:25.456473  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.456505  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.456676  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.456740  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:25.456950  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.457036  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.457746   909  7315 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.457894   909  7315 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.458308   909  7315 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.459956  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.460118  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:25.460296  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.460401  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.460982   909  1631 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.461070   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.461381   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.464317  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:46:25.464417  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:46:25.464456  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:46:25.464596  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:46:25.467030  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.469357  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:46:25.469558  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:46:25.478555  1450  1752 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:25.482800  1450  1752 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:25.488197  1450  4234 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:46:25.489664  1450  4234 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:46:25.490297  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:46:25.490433  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:46:25.493028  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:46:25.493189  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:46:25.493262  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:25.493312  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:46:25.547979   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:46:25.547979  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.550257  1450 20008 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.550705  1450 20008 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.564832  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.566405  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.566885  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.640219  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.641731  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.675439  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.703051  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.703794  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.739862  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.745480  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.745988  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.765485  1450  1511 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.765610  1450  1511 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.788198  1450 29539 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.788716  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.806029  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.808977  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.810709  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.810809  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.811686  1450  1515 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.811870  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:46:25.816701  1450  1511 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.816837  1450  1511 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.823788  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.826644  1450  2351 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.826921  1450  2351 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.840453  1450 29539 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.841215  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.845907  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.850735  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.850993  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:25.859471  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:25.865748  1450 21807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:25.866118  1450 21807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:25.881812  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:25.883325  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.883455  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:46:25.885652   909  1512 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.886121   909  1512 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.889663  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.889854  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:46:25.891707  1450  4234 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:25.892641  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:25.893518   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.893788   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.897189  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.897365  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:25.897610  1450  1450 D RILJ    : [9539]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:46:25.901568  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:25.902233   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:46:25.902347   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cda900, pRI=0x7f9784c510, p=0x7f978570a0, pUCI=0x0
10-17 14:46:25.902389   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c510 p=0x7f978570a0 dispatched to RIL_CMD_PROXY_3
10-17 14:46:25.902498   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:25.902528   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:25.902560   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:25.902609   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:25.902645   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:46:25.902678   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:25.902685   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c510 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:46:25.902704   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:25.902723   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:46:25.902748   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:25.902756   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:46:25.902773   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:25.902782   721   749 D RIL     : radioState:10
10-17 14:46:25.902815   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:25.902829   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:46:25.902842   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:25.902863   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:46:25.902883   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:25.902898   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.902909   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:25.902927   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:46:25.902951   721   749 I AT      : AT write start
10-17 14:46:25.902965   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:25.902989   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:25.903070   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:25.903100   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:25.903567   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:25.903668   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:25.903712   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:25.903993   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:25.904050   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:25.904103   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:46:25.904208   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:46:25.904430  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:46:25.906924   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:25.907004   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:25.907091   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:25.907121   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:25.907303  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.907392  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:46:25.907747  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.907884  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.908574   909  1632 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.908756   909  1632 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.909039   909  1632 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.910011  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:46:25.910202  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:46:25.910341  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:46:25.910408  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:46:25.911353   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:46:25.911484   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:46:25.911967   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:46:25.912751   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:46:25.912817   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:46:25.912918   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:46:25.912972   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:25.913100   721   766 I AT      : AT read end: 6
10-17 14:46:25.913156   721   766 D AT      : AT< OK
10-17 14:46:25.913187   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:46:25.913234   721   766 I AT      : AT read start
10-17 14:46:25.913365   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:46:25.913413   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:25.913454   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:25.913524   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f978570a0 
10-17 14:46:25.913558   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda900
10-17 14:46:25.913584   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:25.913693  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:46:25.913812  1450  1606 D RILJ    : [9539]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:46:25.914860  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:46:25.915021  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:46:25.917570  1450 20008 D DCT     : [0]phoneSubId = 1
10-17 14:46:25.917775  1450 20008 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:26.316598   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43660 
10-17 14:46:26.316688   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e436c0
10-17 14:46:26.316721   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e436d0
10-17 14:46:26.317660   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43660 reset to NULL
10-17 14:46:26.317733   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43660
10-17 14:46:26.317765   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43670
10-17 14:46:26.599736  1450  1450 D RILJ    : [9540]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:26.608411   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:26.608543   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784cb10, p=0x7f978565b0, pUCI=0x0
10-17 14:46:26.608588   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cb10 p=0x7f978565b0 dispatched to RIL_ATCI_PROXY
10-17 14:46:26.608835   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:26.608885   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:26.608935   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:26.608964   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:26.609022   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:26.609051   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:26.609101   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:26.609128   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:26.609425   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:26.609485   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:26.609554   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:26.609584   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:26.609642   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:26.609670   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:26.609735   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:26.609765   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:26.609824   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:26.609853   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:26.612333   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:26.612438   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:26.612482   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cb10 p=0x7f978565b0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:26.612522   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:26.612589   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:26.612623   721   753 D RIL     : radioState:10
10-17 14:46:26.612679   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:26.612718   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:26.612753   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:26.612781   721   753 I AT      : AT write start
10-17 14:46:26.613179   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:26.613256   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:26.613317   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:26.613468   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:26.613653   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:26.613756   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:26.616008   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:26.616128   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:26.621395   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:26.624921   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:26.625005   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:26.625054   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:26.625931   721   770 I AT      : AT read end: 6
10-17 14:46:26.626009   721   770 D AT      : AT< OK
10-17 14:46:26.626041   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:26.626093   721   770 I AT      : AT read start
10-17 14:46:26.626167   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:26.626214   721   753 D RIL     : p_response->success = 1
10-17 14:46:26.626243   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:26.626267   721   753 D RIL     : strLength = 6
10-17 14:46:26.626293   721   753 D RIL     : line = <
10-17 14:46:26.626293   721   753 D RIL     : OK
10-17 14:46:26.626293   721   753 D RIL     : >
10-17 14:46:26.626322   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:26.626373   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:26.626467   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f978565b0 
10-17 14:46:26.626503   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:46:26.626537   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:26.627819  1450  1606 D RILJ    : [9540]< OEM_HOOK_RAW [B@f03ac1c [SUB0]
10-17 14:46:26.721664  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:26.722994  1450  1515 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:46:26.727214  1450  1515 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:46:26.877155  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:46:26.938973  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:46:26.939821  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:46:26.958287  1450 29539 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:46:26.964204  1450  1752 D DCT     : [0]phoneSubId = 1
10-17 14:46:26.965055  1450  1752 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:46:27.455067   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185203/0
10-17 14:46:28.555055  1450  1450 D RILJ    : [9541]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:28.557321   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:28.557404   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaac0, pRI=0x7f9784cba0, p=0x7f97856bd0, pUCI=0x0
10-17 14:46:28.557440   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cba0 p=0x7f97856bd0 dispatched to RIL_ATCI_PROXY
10-17 14:46:28.557538   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:28.557580   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:28.557616   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:28.557623   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:28.557646   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:28.557676   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:28.557691   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:28.557709   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:28.557738   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:28.557744   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:28.557752   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:28.557770   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:28.557803   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:28.557809   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:28.557812   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:28.557856   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:28.557895   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:28.557967   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:28.557994   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:28.558031   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:28.558070   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:28.558109   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:28.558186   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:28.558229   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:28.558262   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cba0 p=0x7f97856bd0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:28.558293   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:28.558322   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:28.558347   721   753 D RIL     : radioState:10
10-17 14:46:28.558384   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:28.558413   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:28.558437   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:28.558461   721   753 I AT      : AT write start
10-17 14:46:28.558615   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:28.558675   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:28.558724   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:28.558805   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:28.560607   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:28.560679   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:28.560763   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:28.560810   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:28.560984   721   770 I AT      : AT read end: 6
10-17 14:46:28.561049   721   770 D AT      : AT< OK
10-17 14:46:28.561082   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:28.561127   721   770 I AT      : AT read start
10-17 14:46:28.561172   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:28.561206   721   753 D RIL     : p_response->success = 1
10-17 14:46:28.561233   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:28.561257   721   753 D RIL     : strLength = 6
10-17 14:46:28.561281   721   753 D RIL     : line = <
10-17 14:46:28.561281   721   753 D RIL     : OK
10-17 14:46:28.561281   721   753 D RIL     : >
10-17 14:46:28.561310   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:28.561360   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:28.561430   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f97856bd0 
10-17 14:46:28.561470   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:46:28.561495   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:28.561638  1450  1606 D RILJ    : [9541]< OEM_HOOK_RAW [B@ca90025 [SUB0]
10-17 14:46:30.553603   721   760 I RILC    : NUMBER:1
10-17 14:46:30.553685   721   760 I RILC    : arg len:14
10-17 14:46:30.553725   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:46:30.553889   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:46:30.553996   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784cbd0 p=0x7f97856c40 dispatched to RIL_CMD_PROXY_1
10-17 14:46:30.554120   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:30.554173   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:30.554223   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:30.554251   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:30.554298   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:30.554325   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:30.554318   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:30.554357   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:30.554400   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:30.554413   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:30.554428   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:30.554474   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:30.554476   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:30.554505   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:30.554555   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:30.554561   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:46:30.554583   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:30.554602   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784cbd0 p=0x7f97856c40 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:46:30.554623   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:30.554650   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:46:30.554684   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:46:30.554712   721   751 D RIL     : radioState:10
10-17 14:46:30.554795   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:46:30.554928   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:46:30.554967   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:30.554994   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:46:30.555023   721   751 I AT      : AT write start
10-17 14:46:30.555212   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:30.555271   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:30.555319   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:30.555321   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:30.555346   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:30.555381   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:30.555389   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:30.555415   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:30.555435   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:46:30.555540   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:46:30.563327   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:46:30.563441   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:30.563539   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:46:30.563592   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:30.563658   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:46:30.563701   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:46:30.563781   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:46:30.563825   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:30.563970   721   768 I AT      : AT read end: 46
10-17 14:46:30.564039   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:30.564071   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:46:30.564110   721   768 D AT      : AT< OK
10-17 14:46:30.564137   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:46:30.564190   721   768 I AT      : AT read start
10-17 14:46:30.564245   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:46:30.564294   721   751 D RIL     : requestQueryThermal success
10-17 14:46:30.564325   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:30.564357   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:46:30.564399   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:46:30.564472   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97856c40 
10-17 14:46:30.564514   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:46:30.564539   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:30.626852  1450  1515 D use-Rlog/RLOG-GSM: [RadioCapSwitchUtil] getMainCapabilityPhoneId 0
10-17 14:46:30.627439 25918 25918 D ImsManager: MainCapabilityPhoneId is 0 on feature 2
10-17 14:46:30.640748 25918 25918 D ImsManager: wfc resource value is true, system property is 0, Carrier value is true
10-17 14:46:31.815043   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:46:31.815113   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:46:31.815182   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:46:31.815222   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:31.815499   721   765 I AT      : AT read end: 37
10-17 14:46:31.815545   721   765 D AT      : AT< +ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815574   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815619   721   765 D RIL     : Nw URC:+ECSQ: 41,99,-280,1,1,1,1,3,32767
10-17 14:46:31.815688   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:46:31.815724   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:46:31.815750   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:31.815818   721   765 I AT      : AT read start
10-17 14:46:31.816216  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:46:31.816417  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -282 1 1
10-17 14:46:31.816499  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -280 1 1
10-17 14:46:31.816547  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:46:32.455351   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185207/0
10-17 14:46:34.643190  1450  1450 D RILJ    : [9542]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:46:34.645950   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:46:34.646021   721   760 I RILC-MTK: create request 59: pRequest=0x7f94ce6a60, pRI=0x7f9784cc00, p=0x7f97857110, pUCI=0x0
10-17 14:46:34.646055   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc00 p=0x7f97857110 dispatched to RIL_ATCI_PROXY
10-17 14:46:34.646168   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:34.646197   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:34.646220   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:34.646224   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:34.646221   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:34.646258   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:34.646289   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:34.646292   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:34.646339   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:34.646346   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:34.646363   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:34.646380   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc00 p=0x7f97857110 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:34.646400   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:34.646417   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:34.646424   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:34.646449   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:46:34.646463   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:34.646474   721   753 D RIL     : radioState:10
10-17 14:46:34.646507   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:34.646513   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:46:34.646530   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:34.646538   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:34.646546   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:34.646571   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:46:34.646595   721   753 I AT      : AT write start
10-17 14:46:34.646593   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:34.646745   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:34.646795   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:34.646843   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:34.646927   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:46:34.647138   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:34.647182   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:34.647224   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:34.647248   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:34.647285   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:34.647308   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:34.654380   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:4
10-17 14:46:34.654460   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 4 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:34.654528   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 4/4 bytes of frame to /dev/pts/6
10-17 14:46:34.654572   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:34.654673   721   770 I AT      : AT read end: 4
10-17 14:46:34.654709   721   770 I AT      : AT read start
10-17 14:46:34.657135   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:2
10-17 14:46:34.657193   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 2 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:34.657253   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 2/2 bytes of frame to /dev/pts/6
10-17 14:46:34.657291   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:34.657392   721   770 I AT      : AT read end: 2
10-17 14:46:34.657430   721   770 D AT      : AT< OK
10-17 14:46:34.657458   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:34.657498   721   770 I AT      : AT read start
10-17 14:46:34.657543   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:34.657577   721   753 D RIL     : p_response->success = 1
10-17 14:46:34.657603   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:34.657626   721   753 D RIL     : strLength = 6
10-17 14:46:34.657649   721   753 D RIL     : line = <
10-17 14:46:34.657649   721   753 D RIL     : OK
10-17 14:46:34.657649   721   753 D RIL     : >
10-17 14:46:34.657676   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:34.657732   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:34.657802   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc00 p=0x7f97857110 
10-17 14:46:34.657832   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a60
10-17 14:46:34.657872   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:34.658038  1450  1606 D RILJ    : [9542]< OEM_HOOK_RAW [B@39e85fa [SUB0]
10-17 14:46:35.117815  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:35.118982  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:46:35.359861  1450  1450 D RILJ    : [9543]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:46:35.369803   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:46:35.370031   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda740, pRI=0x7f9784cc30, p=0x7f97856930, pUCI=0x0
10-17 14:46:35.370115   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc30 p=0x7f97856930 dispatched to RIL_ATCI_PROXY
10-17 14:46:35.370315   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:46:35.370389   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:46:35.370402   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:46:35.370394   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:46:35.370453   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:46:35.370500   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:46:35.370507   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:46:35.370516   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:46:35.370580   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:46:35.370597   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:46:35.370605   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:46:35.370641   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:46:35.370716   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:46:35.370771   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:46:35.370844   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:46:35.370886   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:46:35.371101   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:46:35.371105   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:46:35.371203   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:46:35.371228   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:46:35.371418   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:46:35.371454   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:46:35.371483   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784cc30 p=0x7f97856930 execute on RIL_ATCI_PROXY using channel 5
10-17 14:46:35.371525   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:46:35.371575   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:46:35.371611   721   753 D RIL     : radioState:10
10-17 14:46:35.371688   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:46:35.371745   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:46:35.371781   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:46:35.371809   721   753 I AT      : AT write start
10-17 14:46:35.372113   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:46:35.372254   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:46:35.372344   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:46:35.372511   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:46:35.372929   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:46:35.373381   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:46:35.380078   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:46:35.380192   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:46:35.380293   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:46:35.380353   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:46:35.380552   721   770 I AT      : AT read end: 6
10-17 14:46:35.380631   721   770 D AT      : AT< OK
10-17 14:46:35.380671   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:46:35.380730   721   770 I AT      : AT read start
10-17 14:46:35.380794   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:46:35.380840   721   753 D RIL     : p_response->success = 1
10-17 14:46:35.380869   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:46:35.381091   721   753 D RIL     : strLength = 6
10-17 14:46:35.381190   721   753 D RIL     : line = <
10-17 14:46:35.381190   721   753 D RIL     : OK
10-17 14:46:35.381190   721   753 D RIL     : >
10-17 14:46:35.381229   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:46:35.381293   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:35.381415   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc30 p=0x7f97856930 
10-17 14:46:35.381454   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda740
10-17 14:46:35.381479   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:46:35.381753  1450  1606 D RILJ    : [9543]< OEM_HOOK_RAW [B@ad67ab [SUB0]
10-17 14:46:40.316721   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:42.199635   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:48.178504   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:48.790757   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:49.260462   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:51.444346   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:53.541326   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:56.706712   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:57.264666   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:46:59.888297   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:01.128526   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:02.448299   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:05.738157   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:10.718345   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:11.465560   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:14.212582   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:18.685604   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:20.494317   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:22.495094   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:22.686200   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:27.096387   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:27.465371   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:28.230834   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:28.297164   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:28.682551   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:32.648533   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:32.760489   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:39.634125   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:46.172568   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:46.925866   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:48.107817   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:51.448083   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:52.745078   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:53.470777   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:55.993528   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:57.010224   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:47:57.138907 26268 26302 D getTestMode: Test mode is 0
10-17 14:47:59.332986   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:00.893543   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:03.164163   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:03.877599  1450  1450 D RILJ    : [9575]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:03.882635   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:03.882770   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaac0, pRI=0x7f9784c360, p=0x7f978567e0, pUCI=0x0
10-17 14:48:03.882805   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f978567e0 dispatched to RIL_ATCI_PROXY
10-17 14:48:03.882934   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:03.882939   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:03.882984   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:03.882984   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:03.883018   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:03.883062   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:03.883063   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:03.883096   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:03.883139   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:03.883143   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:03.883167   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:03.883210   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:03.883213   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:03.883242   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:03.883286   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:03.883295   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:03.883331   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:03.883346   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:03.883361   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:03.883371   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:03.883396   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f978567e0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:03.883403   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:03.883427   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:03.883451   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:03.883465   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:03.883477   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:03.883492   721   753 D RIL     : radioState:10
10-17 14:48:03.883533   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:03.883565   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:03.883591   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:03.883616   721   753 I AT      : AT write start
10-17 14:48:03.883857   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:03.883924   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:03.884027   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:03.884084   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:03.884202   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:03.891895   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:03.891978   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:03.892040   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:03.892082   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:03.892327   721   770 I AT      : AT read end: 6
10-17 14:48:03.892400   721   770 D AT      : AT< OK
10-17 14:48:03.892440   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:03.892503   721   770 I AT      : AT read start
10-17 14:48:03.892562   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:03.892628   721   753 D RIL     : p_response->success = 1
10-17 14:48:03.892657   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:03.892684   721   753 D RIL     : strLength = 6
10-17 14:48:03.892711   721   753 D RIL     : line = <
10-17 14:48:03.892711   721   753 D RIL     : OK
10-17 14:48:03.892711   721   753 D RIL     : >
10-17 14:48:03.892743   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:03.892807   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:03.892903   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f978567e0 
10-17 14:48:03.892940   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:48:03.892999   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:03.894022  1450  1606 D RILJ    : [9575]< OEM_HOOK_RAW [B@160178b [SUB0]
10-17 14:48:05.054968   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:48:05.055060   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:48:05.055136   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:48:05.055181   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:05.055307   721   765 I AT      : AT read end: 37
10-17 14:48:05.055347   721   765 D AT      : AT< +ECSQ: 43,99,-271,1,1,1,1,3,32767
10-17 14:48:05.055377   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 43,99,-271,1,1,1,1,3,32767
10-17 14:48:05.055417   721   765 D RIL     : Nw URC:+ECSQ: 43,99,-271,1,1,1,1,3,32767
10-17 14:48:05.055478   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:48:05.055516   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:48:05.055543   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:05.055616   721   765 I AT      : AT read start
10-17 14:48:05.055934  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:48:05.056112  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:48:05.056215  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -271 1 1
10-17 14:48:05.056268  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:05.124908  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:05.127619  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:05.975913  1450  1450 D RILJ    : [9576]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:05.978327   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:05.978400   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784c3f0, p=0x7f978571f0, pUCI=0x0
10-17 14:48:05.978433   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f978571f0 dispatched to RIL_ATCI_PROXY
10-17 14:48:05.978537   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:05.978555   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:05.978554   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:05.978579   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:05.978579   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:05.978610   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:05.978648   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:05.978653   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:05.978664   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:05.978675   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:05.978706   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:05.978720   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:05.978773   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:05.978794   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:05.978801   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:05.978835   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:05.978872   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:05.980275   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:05.980375   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:05.980403   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:05.980415   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:05.980442   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f978571f0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:05.980477   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:05.980488   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:05.980513   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:05.980516   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:05.980547   721   753 D RIL     : radioState:10
10-17 14:48:05.980588   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:05.980618   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:05.980647   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:05.980669   721   753 I AT      : AT write start
10-17 14:48:05.981054   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:05.981148   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:05.981205   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:05.981257   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:05.981358   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:05.988842   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:05.988920   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:05.988989   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:05.989036   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:05.989168   721   770 I AT      : AT read end: 6
10-17 14:48:05.989219   721   770 D AT      : AT< OK
10-17 14:48:05.989250   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:05.989302   721   770 I AT      : AT read start
10-17 14:48:05.989448   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:05.989494   721   753 D RIL     : p_response->success = 1
10-17 14:48:05.989521   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:05.989544   721   753 D RIL     : strLength = 6
10-17 14:48:05.989568   721   753 D RIL     : line = <
10-17 14:48:05.989568   721   753 D RIL     : OK
10-17 14:48:05.989568   721   753 D RIL     : >
10-17 14:48:05.989596   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:05.989644   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:05.989708   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c3f0 p=0x7f978571f0 
10-17 14:48:05.989749   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:48:05.989774   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:05.989961  1450  1606 D RILJ    : [9576]< OEM_HOOK_RAW [B@d989068 [SUB0]
10-17 14:48:07.458273   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185271/0
10-17 14:48:07.731892  1450  1450 D RILJ    : [9577]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:07.733937   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:07.734008   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9160, pRI=0x7f9784c6f0, p=0x7f978572d0, pUCI=0x0
10-17 14:48:07.734040   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978572d0 dispatched to RIL_ATCI_PROXY
10-17 14:48:07.734158   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:07.734196   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:07.734195   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:07.734226   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:07.734232   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978572d0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:07.734264   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:07.734265   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:07.734294   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:07.734296   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:07.734323   721   753 D RIL     : radioState:10
10-17 14:48:07.734333   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:07.734359   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:07.734362   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:07.734395   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:07.734398   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:07.734424   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:07.734425   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:07.734451   721   753 I AT      : AT write start
10-17 14:48:07.734463   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:07.734486   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:07.734521   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:07.734556   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:07.734564   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:07.734588   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:07.734632   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:07.734623   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:07.734657   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:07.734714   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:07.734759   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:07.734806   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:07.734884   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:07.734930   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:07.734955   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:07.734994   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:07.735017   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:07.735052   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:07.742302   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:07.742375   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:07.742441   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:07.742481   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:07.742578   721   770 I AT      : AT read end: 6
10-17 14:48:07.742615   721   770 D AT      : AT< OK
10-17 14:48:07.742644   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:07.742683   721   770 I AT      : AT read start
10-17 14:48:07.742722   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:07.742757   721   753 D RIL     : p_response->success = 1
10-17 14:48:07.742784   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:07.742816   721   753 D RIL     : strLength = 6
10-17 14:48:07.742843   721   753 D RIL     : line = <
10-17 14:48:07.742843   721   753 D RIL     : OK
10-17 14:48:07.742843   721   753 D RIL     : >
10-17 14:48:07.742869   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:07.742915   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:07.742982   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f978572d0 
10-17 14:48:07.743016   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9160
10-17 14:48:07.743039   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:07.743176  1450  1606 D RILJ    : [9577]< OEM_HOOK_RAW [B@e655c81 [SUB0]
10-17 14:48:08.277574  1450  1450 D RILJ    : [9578]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:08.281729   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:08.281813   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda760, pRI=0x7f9784c810, p=0x7f978565b0, pUCI=0x0
10-17 14:48:08.281848   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f978565b0 dispatched to RIL_ATCI_PROXY
10-17 14:48:08.282002   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:08.282000   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:08.282048   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:08.282086   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:08.282095   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:08.282112   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:08.282160   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:08.282161   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:08.282192   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:08.282197   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:08.282233   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:08.282236   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f978565b0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:08.282262   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:08.282272   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:08.282300   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:08.282303   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:08.282328   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:08.282331   721   753 D RIL     : radioState:10
10-17 14:48:08.282369   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:08.282376   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:08.282395   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:08.282407   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:08.282433   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:08.282434   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:08.282460   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:08.282464   721   753 I AT      : AT write start
10-17 14:48:08.282500   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:08.282526   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:08.282556   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:08.282783   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:08.282844   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:08.282893   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:08.283006   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:08.283089   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:08.283123   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:08.283162   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:08.290600   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:08.290697   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:08.290769   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:08.290813   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:08.291082   721   770 I AT      : AT read end: 6
10-17 14:48:08.291147   721   770 D AT      : AT< OK
10-17 14:48:08.291178   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:08.291220   721   770 I AT      : AT read start
10-17 14:48:08.292792   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:08.292898   721   753 D RIL     : p_response->success = 1
10-17 14:48:08.292934   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:08.292970   721   753 D RIL     : strLength = 6
10-17 14:48:08.293012   721   753 D RIL     : line = <
10-17 14:48:08.293012   721   753 D RIL     : OK
10-17 14:48:08.293012   721   753 D RIL     : >
10-17 14:48:08.293058   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:08.293147   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:08.293342   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c810 p=0x7f978565b0 
10-17 14:48:08.293387   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:48:08.293416   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:08.293651  1450  1606 D RILJ    : [9578]< OEM_HOOK_RAW [B@1de126 [SUB0]
10-17 14:48:10.717653   721   760 I RILC    : NUMBER:1
10-17 14:48:10.717711   721   760 I RILC    : arg len:14
10-17 14:48:10.717747   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:48:10.717850   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:48:10.717906   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978569a0 dispatched to RIL_CMD_PROXY_1
10-17 14:48:10.718052   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:10.718083   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:10.718128   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:10.718124   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:10.718160   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:10.718163   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:48:10.718195   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c300 p=0x7f978569a0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:48:10.718201   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:10.718229   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:10.718234   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:48:10.718269   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:48:10.718271   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:10.718299   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:10.718299   721   751 D RIL     : radioState:10
10-17 14:48:10.718343   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:10.718349   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:48:10.718369   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:10.718397   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:48:10.718406   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:10.718429   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:10.718428   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:10.718459   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:48:10.718471   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:10.718483   721   751 I AT      : AT write start
10-17 14:48:10.718497   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:10.718543   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:10.718568   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:10.718597   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:10.718607   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:10.718625   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:10.719641   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:10.719712   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:10.719761   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:48:10.719847   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:48:10.719919   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:10.719990   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:10.720015   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:10.721642   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:48:10.721728   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:10.721796   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:48:10.721975   721   768 I AT      : AT read end: 40
10-17 14:48:10.722019   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:10.722048   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:10.722083   721   768 I AT      : AT read start
10-17 14:48:10.722585   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:10.722658   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:48:10.722700   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:10.722770   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:48:10.722808   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:10.722899   721   768 I AT      : AT read end: 6
10-17 14:48:10.722931   721   768 D AT      : AT< OK
10-17 14:48:10.722958   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:48:10.723000   721   768 I AT      : AT read start
10-17 14:48:10.724420   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:10.724468   721   751 D RIL     : requestQueryThermal success
10-17 14:48:10.724499   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:10.724528   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:48:10.724567   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:48:10.724623   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c300 p=0x7f978569a0 
10-17 14:48:10.724661   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6a20
10-17 14:48:10.724685   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:12.458549   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185275/0
10-17 14:48:15.118512  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:15.122336  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:16.656742  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:48:16.660316  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:48:16.660474  1450  1450 D RILJ    : [9579]> SCREEN_STATE: false [SUB0]
10-17 14:48:16.663003  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:48:16.663654  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:48:16.663786  1450  1450 D RILJ    : [9580]> SCREEN_STATE: false [SUB1]
10-17 14:48:16.663863   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:48:16.663918   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9140, pRI=0x7f9784c960, p=0x7f97856bd0, pUCI=0x0
10-17 14:48:16.663949   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c960 p=0x7f97856bd0 dispatched to RIL_CMD_PROXY_3
10-17 14:48:16.664116   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:16.664155   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:16.664197   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:16.664212   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:16.664227   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:16.664267   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:16.664273   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:16.664298   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:16.664334   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:16.664343   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:16.664358   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:16.664406   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:16.664431   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:16.664468   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:16.664491   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:16.664530   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:16.664553   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:16.664595   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:16.664619   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:16.664673   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:16.664699   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:16.664754   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:16.668471   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:16.668552   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c960 p=0x7f97856bd0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:16.668585   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:16.668616   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:16.668640   721   749 D RIL     : radioState:10
10-17 14:48:16.668691   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.668718   721   749 D AT      : AT> AT+CREG=1
10-17 14:48:16.668742   721   749 I AT      : AT write start
10-17 14:48:16.668825   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:16.668944   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.668997   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.669046   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:16.669148   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:16.669286   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:48:16.669364   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cda8a0, pRI=0x7f9784c9c0, p=0x7f97856c40, pUCI=0x0
10-17 14:48:16.669398   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c9c0 p=0x7f97856c40 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:16.669523   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:16.669558   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:16.669596   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:16.669621   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:16.669665   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:16.669691   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:16.669694   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:16.669725   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:16.669762   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:16.669791   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:16.669824   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c9c0 p=0x7f97856c40 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:16.669854   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:16.669884   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:16.669909   721   755 D RIL     : radioState:0
10-17 14:48:16.669944   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:16.669971   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:16.669995   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:16.670042   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.670069   721   755 D AT      : AT> AT+CREG=1
10-17 14:48:16.670092   721   755 I AT      : AT write start
10-17 14:48:16.670177   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:16.670202   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:16.670239   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:16.670263   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:16.670299   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:16.670323   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:16.670362   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:16.670386   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:16.670545   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:16.670578   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:16.670617   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:16.670641   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:16.670751   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.670806   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.670858   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:16.671427   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:16.676538   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:16.676614   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:16.676678   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:16.676720   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.676825   721   766 I AT      : AT read end: 6
10-17 14:48:16.676867   721   766 D AT      : AT< OK
10-17 14:48:16.676896   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:16.676941   721   766 I AT      : AT read start
10-17 14:48:16.678681   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:16.678774   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:16.678854   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:16.678896   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.683534   721   772 I AT      : AT read end: 6
10-17 14:48:16.683598   721   772 D AT      : AT< OK
10-17 14:48:16.683628   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:16.683695   721   772 I AT      : AT read start
10-17 14:48:16.683751   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.683808   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.683836   721   749 D AT      : AT> AT+CGREG=1
10-17 14:48:16.683863   721   749 I AT      : AT write start
10-17 14:48:16.683977   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.684015   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.684040   721   755 D AT      : AT> AT+CGREG=1
10-17 14:48:16.684063   721   755 I AT      : AT write start
10-17 14:48:16.684187   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.684239   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.684288   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:16.684367   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:16.686751   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.686824   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.686873   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:16.686951   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:16.691906   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:16.691969   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:16.692034   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:16.692076   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.692182   721   772 I AT      : AT read end: 6
10-17 14:48:16.692220   721   772 D AT      : AT< OK
10-17 14:48:16.692248   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:16.692296   721   772 I AT      : AT read start
10-17 14:48:16.692359   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.692402   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.692428   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:48:16.692467   721   755 I AT      : AT write start
10-17 14:48:16.692590   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.692594   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:16.692637   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.692642   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:16.692681   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:16.692696   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:16.692735   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.692757   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:16.692813   721   766 I AT      : AT read end: 6
10-17 14:48:16.692845   721   766 D AT      : AT< OK
10-17 14:48:16.692873   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:16.692911   721   766 I AT      : AT read start
10-17 14:48:16.692984   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.693019   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.693043   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:48:16.693064   721   749 I AT      : AT write start
10-17 14:48:16.693187   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.693232   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.693280   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:16.693357   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:16.693783   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:16.693840   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:16.693903   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:16.693944   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.694039   721   772 I AT      : AT read end: 6
10-17 14:48:16.694077   721   772 D AT      : AT< OK
10-17 14:48:16.694105   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:16.694144   721   772 I AT      : AT read start
10-17 14:48:16.694188   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.694226   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.694275   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:48:16.694320   721   755 I AT      : AT write start
10-17 14:48:16.694460   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.694505   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.694551   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:16.694630   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:48:16.694850   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:16.694904   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:16.694963   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:16.695003   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.695089   721   766 I AT      : AT read end: 6
10-17 14:48:16.695125   721   766 D AT      : AT< OK
10-17 14:48:16.695151   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:16.695189   721   766 I AT      : AT read start
10-17 14:48:16.695237   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.695281   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.695308   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:48:16.695335   721   749 I AT      : AT write start
10-17 14:48:16.695455   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.695498   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.695543   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:16.695621   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:48:16.695904   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:16.695956   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:16.696013   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:16.696052   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.696139   721   772 I AT      : AT read end: 6
10-17 14:48:16.696177   721   772 D AT      : AT< OK
10-17 14:48:16.696205   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:16.696241   721   772 I AT      : AT read start
10-17 14:48:16.696295   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.696343   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.696368   721   755 D AT      : AT> AT+CEREG=1
10-17 14:48:16.696390   721   755 I AT      : AT write start
10-17 14:48:16.696500   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.696542   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.696584   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:16.696657   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:16.696927   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:16.696986   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:16.697046   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:16.697085   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.697173   721   766 I AT      : AT read end: 6
10-17 14:48:16.697206   721   766 D AT      : AT< OK
10-17 14:48:16.697232   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:16.697266   721   766 I AT      : AT read start
10-17 14:48:16.697322   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.697371   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.697399   721   749 D AT      : AT> AT+CEREG=1
10-17 14:48:16.697421   721   749 I AT      : AT write start
10-17 14:48:16.697533   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.697575   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.697621   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:16.697918   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:16.697974   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:16.698033   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:16.698073   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.698158   721   772 I AT      : AT read end: 6
10-17 14:48:16.698193   721   772 D AT      : AT< OK
10-17 14:48:16.698230   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:16.698276   721   772 I AT      : AT read start
10-17 14:48:16.698315   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:16.698352   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:16.698391   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:16.698462   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c9c0 p=0x7f97856c40 
10-17 14:48:16.698494   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda8a0
10-17 14:48:16.698518   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:16.698724  1450  1609 D RILJ    : [9580]< SCREEN_STATE  [SUB1]
10-17 14:48:16.701082   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:16.709243   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:16.709311   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:16.709375   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:16.709415   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.709514   721   766 I AT      : AT read end: 6
10-17 14:48:16.709552   721   766 D AT      : AT< OK
10-17 14:48:16.709581   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:16.709625   721   766 I AT      : AT read start
10-17 14:48:16.709722   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:16.709764   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:16.709802   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:16.709871   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c960 p=0x7f97856bd0 
10-17 14:48:16.709901   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9140
10-17 14:48:16.709925   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:16.710027  1450  1606 D RILJ    : [9579]< SCREEN_STATE  [SUB0]
10-17 14:48:16.934975  1450  1450 D RILJ    : [9581]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:16.936808   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:16.936894   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaac0, pRI=0x7f9784ca50, p=0x7f97857420, pUCI=0x0
10-17 14:48:16.936929   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784ca50 p=0x7f97857420 dispatched to RIL_ATCI_PROXY
10-17 14:48:16.937049   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:16.937069   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:16.937093   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:16.937095   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:16.937128   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784ca50 p=0x7f97857420 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:16.937138   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:16.937157   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:16.937161   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:16.937189   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:16.937199   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:16.937213   721   753 D RIL     : radioState:10
10-17 14:48:16.937221   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:16.937251   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:16.937258   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:16.937281   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:16.937282   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:16.937308   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:16.937322   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:16.937332   721   753 I AT      : AT write start
10-17 14:48:16.937345   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:16.937381   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:16.937404   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:16.937449   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:16.937459   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:16.937475   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:16.937520   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:16.937523   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:16.937547   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:16.937612   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:16.937660   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:16.937710   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:16.937793   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:16.937854   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:16.937891   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:16.937929   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:16.937967   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:16.945445   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:16.945526   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:16.945594   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:16.945637   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:16.945746   721   770 I AT      : AT read end: 6
10-17 14:48:16.945793   721   770 D AT      : AT< OK
10-17 14:48:16.945822   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:16.945860   721   770 I AT      : AT read start
10-17 14:48:16.945909   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:16.945947   721   753 D RIL     : p_response->success = 1
10-17 14:48:16.945986   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:16.946011   721   753 D RIL     : strLength = 6
10-17 14:48:16.946035   721   753 D RIL     : line = <
10-17 14:48:16.946035   721   753 D RIL     : OK
10-17 14:48:16.946035   721   753 D RIL     : >
10-17 14:48:16.946062   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:16.946107   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:16.946182   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784ca50 p=0x7f97857420 
10-17 14:48:16.946213   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:48:16.946238   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:16.946482  1450  1606 D RILJ    : [9581]< OEM_HOOK_RAW [B@b6a167 [SUB0]
10-17 14:48:17.084199  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.086291  1450  1515 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.086428  1450  1515 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.087871  1450  2351 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.088049  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.120263  1450  4234 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.120383  1450  4234 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.126413  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.126530  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.132195  1450  1683 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.132313  1450  1683 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.144982  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.146957  1450  1752 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.147069  1450  1752 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.147921  1450 23534 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.148077  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.162400  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.163958  1450 20008 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.164071  1450 20008 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.164804  1450  4234 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.165028  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.181709  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.183490  1450  1807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.183607  1450  1807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.184382  1450  1683 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.184551  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.198107  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.199844  1450  1752 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.199972  1450  1752 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.200737  1450 23534 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.200964  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.286227  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.289956  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.290377  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.296633  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:48:17.299769  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:48:17.299928  1450  1450 D RILJ    : [9582]> SCREEN_STATE: true [SUB0]
10-17 14:48:17.302599  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:48:17.303233   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:48:17.303328   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cdaaa0, pRI=0x7f9784c150, p=0x7f97857500, pUCI=0x0
10-17 14:48:17.303365   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857500 dispatched to RIL_CMD_PROXY_3
10-17 14:48:17.303496   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:17.303497   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:17.303543   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:17.303573   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:17.303577   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:17.303599   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:17.303608   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:17.303647   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:17.303662   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:17.303673   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:17.303718   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:17.303769   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:17.303826   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:17.303853   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:17.303895   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:17.303929   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:17.304369   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:17.304817   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:17.305330   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:17.305420   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:17.305450  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:48:17.305498   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:17.305539   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.305575  1450  1450 D RILJ    : [9583]> SCREEN_STATE: true [SUB1]
10-17 14:48:17.305583   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c150 p=0x7f97857500 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.305621   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.305661   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:17.305688   721   749 D RIL     : radioState:10
10-17 14:48:17.305768   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.305813   721   749 D AT      : AT> AT+CREG=3
10-17 14:48:17.305841   721   749 I AT      : AT write start
10-17 14:48:17.306007   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:17.306055   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:17.309507   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:48:17.309648   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9360, pRI=0x7f9784c540, p=0x7f97857c00, pUCI=0x0
10-17 14:48:17.309706   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c540 p=0x7f97857c00 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:17.309858   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:17.309927   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:17.309961   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:17.309987   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:17.309994   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:17.310035   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:17.310064   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:17.310063   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:17.310095   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:17.310145   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:17.310147   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:17.310196   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:17.310218   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:17.310232   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:17.310274   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:17.310340   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:17.310369   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:17.310420   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:17.310422   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:17.310454   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:17.310705   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:17.310851   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:17.310998   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c540 p=0x7f97857c00 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:17.311048   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.311089   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:17.311116   721   755 D RIL     : radioState:0
10-17 14:48:17.311169   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.311198   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.311231   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.311295   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.311332   721   755 D AT      : AT> AT+CREG=3
10-17 14:48:17.311357   721   755 I AT      : AT write start
10-17 14:48:17.311693   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.311814   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.311877   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.311999   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:17.312715   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.312844   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.312922   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.313062   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:17.321081   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:48:17.321181   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:48:17.321262   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:48:17.321306   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.321358   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.321402   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.321456   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.321495   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.321543   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:48:17.321585   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:48:17.321639   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:48:17.321679   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.321724   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.321765   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.321814   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.321855   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.322038   721   771 I AT      : AT read end: 36
10-17 14:48:17.322070   721   765 I AT      : AT read end: 36
10-17 14:48:17.322106   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:17.322106   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:17.322143   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:17.322152   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:17.322192   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:17.322191   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:17.322231   721   771 D RIL     : NW state changed: normal case
10-17 14:48:17.322239   721   765 D RIL     : NW state changed: normal case
10-17 14:48:17.322270   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:48:17.322270   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:48:17.322304   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:48:17.322303   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:17.322338   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:48:17.322340   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:48:17.322401   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:48:17.322401   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:48:17.322439   721   765 D RIL     : bCREGType3Support=1
10-17 14:48:17.322441   721   771 D RIL     : bCREGType3Support=1
10-17 14:48:17.322469   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:48:17.322474   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:48:17.322497   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:48:17.322503   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:48:17.322578   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:48:17.322578   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:48:17.322612   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.322612   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.322679   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43720
10-17 14:48:17.322714   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43730
10-17 14:48:17.322841   721   771 I AT      : AT read start
10-17 14:48:17.322928   721   772 I AT      : AT read end: 6
10-17 14:48:17.322967   721   772 D AT      : AT< OK
10-17 14:48:17.322977  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:48:17.322982  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:48:17.323000   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.323053   721   772 I AT      : AT read start
10-17 14:48:17.323145   721   765 D RILC    : s_last_wake_timeout_info: 0x7f94e43720, cancel
10-17 14:48:17.323191   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43780
10-17 14:48:17.323231   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43790
10-17 14:48:17.323295   721   765 I AT      : AT read start
10-17 14:48:17.323465   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.323552   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.323588   721   755 D AT      : AT> AT+CGREG=3
10-17 14:48:17.323614   721   755 I AT      : AT write start
10-17 14:48:17.323828   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.323874   721   766 I AT      : AT read end: 6
10-17 14:48:17.323898   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.323907   721   766 D AT      : AT< OK
10-17 14:48:17.323937   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.323948   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.323982   721   766 I AT      : AT read start
10-17 14:48:17.324038   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:17.324051   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.324102   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.324130   721   749 D AT      : AT> AT+CGREG=3
10-17 14:48:17.324155   721   749 I AT      : AT write start
10-17 14:48:17.324337  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:48:17.324489  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:48:17.324713  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:48:17.324825  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:48:17.325166   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.325245   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.325310   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.325403   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:17.326263  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.326381  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.326455  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:48:17.326527  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:48:17.326675  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:48:17.326823  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:48:17.326929  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:48:17.326979  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:48:17.327022  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:48:17.327069  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:48:17.327107  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:48:17.327263  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:48:17.327461  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:48:17.327573  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:48:17.327649  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:48:17.327967  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:48:17.328906  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.329093  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.329177  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:48:17.330639  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:48:17.330826  1450  1450 D RILJ    : [9584]> OPERATOR [SUB1]
10-17 14:48:17.331689   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.331804   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.331891   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.331939   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.332429   721   772 I AT      : AT read end: 6
10-17 14:48:17.332539   721   772 D AT      : AT< OK
10-17 14:48:17.332574   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.332619   721   772 I AT      : AT read start
10-17 14:48:17.332681   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.332738   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.332768   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:48:17.332804   721   755 I AT      : AT write start
10-17 14:48:17.333556   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.333668   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.333746   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.333792   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.333937   721   766 I AT      : AT read end: 6
10-17 14:48:17.333994   721   766 D AT      : AT< OK
10-17 14:48:17.334027   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.334087   721   766 I AT      : AT read start
10-17 14:48:17.334182   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.334238   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.334269   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:48:17.334293   721   749 I AT      : AT write start
10-17 14:48:17.334524   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.334641   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.334725   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.334827   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:17.336396   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.336469   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.336524   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.336618   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:17.342248   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.342325   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.342391   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.342434   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.345498   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.345574   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.345636   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.345676   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.345971   721   766 I AT      : AT read end: 6
10-17 14:48:17.346043   721   766 D AT      : AT< OK
10-17 14:48:17.346078   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.346129   721   766 I AT      : AT read start
10-17 14:48:17.346175   721   772 I AT      : AT read end: 6
10-17 14:48:17.346213   721   772 D AT      : AT< OK
10-17 14:48:17.346214   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.346249   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.346258   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.346288   721   749 D AT      : AT> AT+ECSQ
10-17 14:48:17.346294   721   772 I AT      : AT read start
10-17 14:48:17.346313   721   749 I AT      : AT write start
10-17 14:48:17.346364   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.346402   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.346440   721   755 D AT      : AT> AT+ECSQ
10-17 14:48:17.346464   721   755 I AT      : AT write start
10-17 14:48:17.346867   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.346924   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.346924   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.346973   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.346984   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.347099   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:48:17.347547   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.347676   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:48:17.347936  1450  1450 D RILJ    : [9585]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:48:17.348544   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:48:17.348649   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf93a0, pRI=0x7f9784c660, p=0x7f97857d50, pUCI=0x0
10-17 14:48:17.348684   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784c660 p=0x7f97857d50 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:17.348795   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:17.348833   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:17.348868   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:17.348883   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:17.348897   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:17.348942   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:17.348947   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:17.348970   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:17.349019   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:17.349046   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:17.349084   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:17.349139   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:17.349165   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:17.349396   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:17.349443   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:17.349478   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:17.349631   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:17.349678   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:17.349724   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:17.349750   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:17.350281  1450  1450 D RILJ    : [9586]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:48:17.351450   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:48:17.351553   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9460, pRI=0x7f9784c7b0, p=0x7f97857f80, pUCI=0x0
10-17 14:48:17.351589   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c660 p=0x7f97857d50 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.351619   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD2_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.351651   721   760 D RILC-MTK: Request pRI=0x7f9784c7b0 to RIL_CMD2_PROXY_3 is busy. total:2 requests pending
10-17 14:48:17.353041  1450  1450 D RILJ    : [9587]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:48:17.354775   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:48:17.354891   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9540, pRI=0x7f9784cab0, p=0x7f97857ff0, pUCI=0x0
10-17 14:48:17.354957   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c660 p=0x7f97857d50 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.354989   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784c7b0 p=0x7f97857f80 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.354914   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:48:17.355027   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD2_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.355054   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.355061   721   760 D RILC-MTK: Request pRI=0x7f9784cab0 to RIL_CMD2_PROXY_3 is busy. total:3 requests pending
10-17 14:48:17.355138   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:48:17.355183   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.355241   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.355282   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.355334   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.355374   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.355625   721   766 I AT      : AT read end: 43
10-17 14:48:17.355670   721   766 D AT      : AT< +ECSQ: 43,99,-271,1,1,1,1,3,32767
10-17 14:48:17.355702   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 43,99,-271,1,1,1,1,3,32767
10-17 14:48:17.355745   721   766 D AT      : AT< OK
10-17 14:48:17.355773   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.355817   721   766 I AT      : AT read start
10-17 14:48:17.355893   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.356104   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:48:17.356158   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:48:17.356198   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.356279   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.356309   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:48:17.356332   721   749 I AT      : AT write start
10-17 14:48:17.356741   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.356834   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.356906   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.357001   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:48:17.357002   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:36
10-17 14:48:17.357060   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.357135   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/9
10-17 14:48:17.357194   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.357247   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.357290   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.357338   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.357386   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.357677  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:17.357804  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:48:17.357889  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:48:17.357954   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:48:17.357980  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:48:17.358021   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9bc0, pRI=0x7f9784cb10, p=0x7f97858140, pUCI=0x0
10-17 14:48:17.358057   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784c660 p=0x7f97857d50 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.358087   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784c7b0 p=0x7f97857f80 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.358116   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cab0 p=0x7f97857ff0 is queued in RIL_CMD2_PROXY_3
10-17 14:48:17.358149   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD2_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.358182   721   760 D RILC-MTK: Request pRI=0x7f9784cb10 to RIL_CMD2_PROXY_3 is busy. total:4 requests pending
10-17 14:48:17.358761   721   772 I AT      : AT read end: 42
10-17 14:48:17.358840   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:48:17.358876   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:48:17.358908   721   772 D AT      : AT< OK
10-17 14:48:17.358934   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.358990   721   772 I AT      : AT read start
10-17 14:48:17.359385   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.359478   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:48:17.359517   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:48:17.359549   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.359577   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:48:17.359600   721   755 I AT      : AT write start
10-17 14:48:17.359789   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.359861   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.359914   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.360001   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:48:17.360592   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.360637  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:48:17.360680   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.360731  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:48:17.360753   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.360795   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.361019  1450  1450 D RILJ    : [9588]> OPERATOR [SUB0]
10-17 14:48:17.361071   721   766 I AT      : AT read end: 6
10-17 14:48:17.361112   721   766 D AT      : AT< OK
10-17 14:48:17.361144   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.361201   721   766 I AT      : AT read start
10-17 14:48:17.361295   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.361346   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.361372   721   749 D AT      : AT> AT+CEREG=3
10-17 14:48:17.361397   721   749 I AT      : AT write start
10-17 14:48:17.362616   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.362614   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.362686   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.362690   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.362741   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.362767   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.362809   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.363084   721   772 I AT      : AT read end: 6
10-17 14:48:17.363138   721   772 D AT      : AT< OK
10-17 14:48:17.363149  1450  1450 D RILJ    : [9589]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:48:17.363168   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.363222   721   772 I AT      : AT read start
10-17 14:48:17.363308   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.363372   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.363419   721   755 D AT      : AT> AT+CEREG=3
10-17 14:48:17.363444   721   755 I AT      : AT write start
10-17 14:48:17.364282   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:48:17.364346   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9be0, pRI=0x7f9784cb40, p=0x7f978581b0, pUCI=0x0
10-17 14:48:17.364382   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cb40 p=0x7f978581b0 dispatched to RIL_CMD_PROXY_3
10-17 14:48:17.364481   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:17.364521   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:17.364567   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:17.364575   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:17.364596   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:17.364633   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:17.364641   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:17.364659   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:17.364714   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:17.364742   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:17.364784   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:17.364815   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:17.364818   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:17.364852   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:17.364896   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:17.364922   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:17.362826   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:17.365156  1450  1450 D RILJ    : [9590]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:48:17.365476   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:17.366387   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:17.366435   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:17.366594   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:17.366742  1450  1450 D RILJ    : [9591]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:48:17.366853   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.366917   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.366981   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.367078   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:17.367550   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:48:17.367631   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9c00, pRI=0x7f9784cbd0, p=0x7f97858290, pUCI=0x0
10-17 14:48:17.367788   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cb40 p=0x7f978581b0 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.367820   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.367860   721   760 D RILC-MTK: Request pRI=0x7f9784cbd0 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:48:17.367906   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:48:17.367957   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9c80, pRI=0x7f9784cc30, p=0x7f97858300, pUCI=0x0
10-17 14:48:17.367988   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cb40 p=0x7f978581b0 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.368017   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cbd0 p=0x7f97858290 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.368046   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.368078   721   760 D RILC-MTK: Request pRI=0x7f9784cc30 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:48:17.368402  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.368517  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:48:17.368613   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:48:17.368677   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9ca0, pRI=0x7f9784cd20, p=0x7f97858370, pUCI=0x0
10-17 14:48:17.368680  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:48:17.368713   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cb40 p=0x7f978581b0 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.368744   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784cbd0 p=0x7f97858290 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.368755  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -271 1 1
10-17 14:48:17.368772   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f97858300 is queued in RIL_CMD_PROXY_3
10-17 14:48:17.368795  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.368803   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:17.368835   721   760 D RILC-MTK: Request pRI=0x7f9784cd20 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:48:17.371125   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.371228   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.371313   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.371359   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.371419   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.371463   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.371525   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.371567   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.371714   721   766 I AT      : AT read end: 6
10-17 14:48:17.371715   721   772 I AT      : AT read end: 6
10-17 14:48:17.371773   721   766 D AT      : AT< OK
10-17 14:48:17.371773   721   772 D AT      : AT< OK
10-17 14:48:17.371806   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.371806   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.371866   721   772 I AT      : AT read start
10-17 14:48:17.371867   721   766 I AT      : AT read start
10-17 14:48:17.371954   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.371954   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.372000   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:17.372001   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.372049   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.372059   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.372129   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f97857500 
10-17 14:48:17.372130   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c540 p=0x7f97857c00 
10-17 14:48:17.372171   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:48:17.372171   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9360
10-17 14:48:17.372208   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:17.372208   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.372245   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784cb40 p=0x7f978581b0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.372245   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784c660 p=0x7f97857d50 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:17.372279   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.372279   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.372313   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:48:17.372314   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:48:17.372342   721   755 D RIL     : radioState:0
10-17 14:48:17.372341   721   749 D RIL     : radioState:10
10-17 14:48:17.372382   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372384   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.372383  1450  1606 D RILJ    : [9582]< SCREEN_STATE  [SUB0]
10-17 14:48:17.372417   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372421   721   749 D AT      : AT> AT+COPS?
10-17 14:48:17.372448   721   749 I AT      : AT write start
10-17 14:48:17.372448   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372482   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372531   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:17.372558   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:17.372595   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.372646   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c660 p=0x7f97857d50 
10-17 14:48:17.372681   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf93a0
10-17 14:48:17.372713  1450  1609 D RILJ    : [9583]< SCREEN_STATE  [SUB1]
10-17 14:48:17.372734   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:17.372765   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c7b0 p=0x7f97857f80 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:17.372799   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.372827   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:48:17.372852   721   755 D RIL     : radioState:0
10-17 14:48:17.372888   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372915   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372940   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.372966   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.373004   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:17.373032   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:17.373030  1450  1609 D RilRequest: [9584]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:17.373079   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.373144   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97857f80 
10-17 14:48:17.373177   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9460
10-17 14:48:17.373208   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:17.373239   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cab0 p=0x7f97857ff0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:17.373269   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.373299   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:48:17.373325   721   755 D RIL     : radioState:0
10-17 14:48:17.373363   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.373377  1450  1609 D RilRequest: [9585]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:17.373393   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.373425   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.373454   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:17.373491   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:17.373519   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:17.373576   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.373642   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cab0 p=0x7f97857ff0 
10-17 14:48:17.373684   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9540
10-17 14:48:17.373678   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.373721   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:17.373750   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.373753   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cb10 p=0x7f97858140 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:17.373787   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.373811   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.373818   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:48:17.373844   721   755 D RIL     : radioState:0
10-17 14:48:17.373882   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.373909   721   755 D AT      : AT> AT+COPS?
10-17 14:48:17.373906   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:17.373940   721   755 I AT      : AT write start
10-17 14:48:17.374201  1450  1609 D RilRequest: [9586]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:17.375498  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:48:17.375598  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:48:17.375607   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.375638  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:17.375661   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.375711  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:48:17.375713   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:17.375752  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:17.375782  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:17.375802   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:48:17.375859  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:48:17.376014   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:48:17.376069   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.376143   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:48:17.376187   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.376236   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.376278   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.376323   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.376361   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.376476   721   766 I AT      : AT read end: 30
10-17 14:48:17.376516   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:48:17.376545   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:48:17.376580   721   766 D AT      : AT< OK
10-17 14:48:17.376606   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.376646   721   766 I AT      : AT read start
10-17 14:48:17.376718   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.376762   721   749 D RIL     : Get operator code 25020
10-17 14:48:17.376822   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:48:17.376859   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:48:17.376889   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.376950   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.377023   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb40 p=0x7f978581b0 
10-17 14:48:17.377065   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9be0
10-17 14:48:17.377097   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.377227   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784cbd0 p=0x7f97858290 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.377284   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.377318   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:48:17.377317  1450  1606 D RILJ    : [9588]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:48:17.377351   721   749 D RIL     : radioState:10
10-17 14:48:17.377412   721   749 D RIL     : request gprs reg state: normal case
10-17 14:48:17.377456   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.377486   721   749 D AT      : AT> AT+CGREG?
10-17 14:48:17.377511   721   749 I AT      : AT write start
10-17 14:48:17.377798   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:48:17.377795   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.377886   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.377965   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.377992   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.378052   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:17.378063   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:48:17.378106   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.378160   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:17.378201   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:17.378249   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:17.378291   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.378402   721   772 I AT      : AT read end: 18
10-17 14:48:17.378450   721   772 D AT      : AT< +COPS: 0
10-17 14:48:17.378482   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:48:17.378518   721   772 D AT      : AT< OK
10-17 14:48:17.378543   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:17.378585   721   772 I AT      : AT read start
10-17 14:48:17.378662   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:17.378715   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:17.378766   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:17.378856   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cb10 p=0x7f97858140 
10-17 14:48:17.378893   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9bc0
10-17 14:48:17.378919   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:17.379584   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:48:17.379674   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.379746   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:48:17.379788   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.379902   721   766 I AT      : AT read end: 44
10-17 14:48:17.379947   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:48:17.380057   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:48:17.380096   721   766 I AT      : AT read start
10-17 14:48:17.380318   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.380381   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.380453   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.380495   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.380610   721   766 I AT      : AT read end: 6
10-17 14:48:17.380647   721   766 D AT      : AT< OK
10-17 14:48:17.380676   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.380722   721   766 I AT      : AT read start
10-17 14:48:17.380777   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.380825   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:17.380856   721   749 E RIL     : The value in the field <lac> :0
10-17 14:48:17.380883   721   749 D RIL     : cid: 3583
10-17 14:48:17.381127   721   749 E RIL     : The value of act: 3
10-17 14:48:17.381158   721   749 D RIL     : cause_type: 0
10-17 14:48:17.381183   721   749 D RIL     : reject_cause: 0
10-17 14:48:17.381231   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.381268   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:48:17.381292   721   749 I AT      : AT write start
10-17 14:48:17.381448   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.381502   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.381551   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.381642   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:48:17.382636   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:48:17.382710   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.382788   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:48:17.382839   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.382954   721   766 I AT      : AT read end: 19
10-17 14:48:17.383004   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:48:17.383034   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:48:17.383141   721   766 I AT      : AT read start
10-17 14:48:17.383376   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.383438   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.383515   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.383567   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.383670   721   766 I AT      : AT read end: 6
10-17 14:48:17.383714   721   766 D AT      : AT< OK
10-17 14:48:17.383744   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.383782   721   766 I AT      : AT read start
10-17 14:48:17.383921   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.383994   721   749 E RIL     : rid: 0
10-17 14:48:17.384035   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:48:17.384077   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:48:17.384105   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:48:17.384131   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:48:17.384160   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.384216   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.384302   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97858290 
10-17 14:48:17.384336   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c00
10-17 14:48:17.384366   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.384397   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784cc30 p=0x7f97858300 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.384426   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.384457   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:48:17.384482   721   749 D RIL     : radioState:10
10-17 14:48:17.384519   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.384507  1450  1606 D RILJ    : [9589]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:48:17.384552   721   749 D AT      : AT> AT+CREG?
10-17 14:48:17.384577   721   749 I AT      : AT write start
10-17 14:48:17.384765   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.384828   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.384880   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.384967   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:17.385731   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:48:17.385799   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.385868   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:48:17.385915   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.386024   721   766 I AT      : AT read end: 38
10-17 14:48:17.386067   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:48:17.386099   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:48:17.386136   721   766 I AT      : AT read start
10-17 14:48:17.386259   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:2
10-17 14:48:17.386314   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 2 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.386378   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 2/2 bytes of frame to /dev/pts/3
10-17 14:48:17.386421   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.386471   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:4
10-17 14:48:17.386510   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 4 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.386556   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 4/4 bytes of frame to /dev/pts/3
10-17 14:48:17.386597   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.386701   721   766 I AT      : AT read end: 6
10-17 14:48:17.386740   721   766 D AT      : AT< OK
10-17 14:48:17.386769   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.386812   721   766 I AT      : AT read start
10-17 14:48:17.386951   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.387003   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:17.387031   721   749 E RIL     : The value in the field <lac> :127
10-17 14:48:17.387059   721   749 D RIL     : cid: 3583
10-17 14:48:17.387084   721   749 E RIL     : The value of act: 3
10-17 14:48:17.387107   721   749 D RIL     : cause_type: 0
10-17 14:48:17.387142   721   749 D RIL     : reject_cause: 0
10-17 14:48:17.387202   721   749 E RIL     : rid: 0
10-17 14:48:17.387233   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:48:17.387263   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:48:17.387290   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:48:17.387315   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:48:17.387345   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:48:17.387378   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.387438   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.387524   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cc30 p=0x7f97858300 
10-17 14:48:17.387557   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9c80
10-17 14:48:17.387590   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.387622   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cd20 p=0x7f97858370 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.387653   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.387680   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:48:17.387704   721   749 D RIL     : radioState:10
10-17 14:48:17.387741   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.387769   721   749 D AT      : AT> AT+COPS?
10-17 14:48:17.387757  1450  1606 D RILJ    : [9590]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:48:17.387963   721   749 I AT      : AT write start
10-17 14:48:17.388184   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.388242  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:48:17.388273   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.388307  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:48:17.388325   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.388400  1450  1609 D RILJ    : [9587]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:48:17.388415   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:17.375898  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:17.388643  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:17.388736  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:48:17.388877  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:48:17.388922  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:48:17.396099   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:48:17.396187   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.396404   721   766 I AT      : AT read end: 24
10-17 14:48:17.396427   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:48:17.396451   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:48:17.396481   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:48:17.396477   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.396527   721   766 I AT      : AT read start
10-17 14:48:17.396542   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.396583   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.396681   721   766 I AT      : AT read end: 6
10-17 14:48:17.396711   721   766 D AT      : AT< OK
10-17 14:48:17.396719   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.396740   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.396760   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.396777   721   766 I AT      : AT read start
10-17 14:48:17.396848   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.396900   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.396949   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.397030   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cd20 p=0x7f97858370 
10-17 14:48:17.397068   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9ca0
10-17 14:48:17.397097   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:17.397294  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:48:17.397446  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:48:17.397540  1450  1606 D RILJ    : [9591]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:48:17.401694  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.401799  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:48:17.401886  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:48:17.401941  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:48:17.402007  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:17.402914  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:17.412698  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.412797  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:48:17.412890  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:48:17.412939  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:48:17.412985  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:48:17.413032  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:48:17.413069  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:48:17.413114  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:48:17.413208  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:48:17.419409  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.422425  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.422578  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:48:17.422639  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:48:17.422748  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:48:17.422842  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:48:17.422894  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:48:17.422946  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:48:17.422980  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.423050  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:48:17.423116  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:48:17.423194  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:48:17.423282  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:48:17.423312  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:48:17.423468  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:48:17.423514  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:48:17.423560  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.423631  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:48:17.423672  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:17.423702  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:17.423750  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:48:17.423796  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:48:17.423804  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:48:17.424918  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:17.427159  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:48:17.427257  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:48:17.427299  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:48:17.427481  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:48:17.427664  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:48:17.427963  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:48:17.428047  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:48:17.428114  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:48:17.428171  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:48:17.428339  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:48:17.428411  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:48:17.428486  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:48:17.428594  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428648  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428696  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428737  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428780  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428823  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428864  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428907  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.428983  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.429031  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:17.429069  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:48:17.429106  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:48:17.429141  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:48:17.429200  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:48:17.430715  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:48:17.431533  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.431672  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:48:17.432389  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:48:17.433300  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:48:17.432
10-17 14:48:17.433432  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:48:17.434087  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.434219  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.434361  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:48:17.434419  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:48:17.434477  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.434748  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:48:17.435448   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.435550   909  7313 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:17.435774   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=4
10-17 14:48:17.436182   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144335Europe/Samara(1,290,14400,0,1476701015) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.436458   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.436662   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.436866   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144625Europe/Samara(1,290,14400,0,1476701185) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.437049   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144817Europe/Samara(1,290,14400,0,1476701297) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.437099   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:48:17.437154   909  7313 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:17.437277   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.437382   909  7313 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:17.437494   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.437709   909  7313 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:17.437858   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.438056   909  7313 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:17.438241   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.438357   909  7313 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:17.438557   909  7313 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:17.438775   909  7313 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:17.439019  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:17.439195  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:17.439266  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:17.439307  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:17.439352  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:48:17.439380  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:17.442311  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:17.442634   909  7313 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:17.445583  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:48:17.445714  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:17.445902  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:48:17.449170  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.458823   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185315/0
10-17 14:48:17.464118  1450 23534 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:48:17.465319  1450 23534 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:48:17.470367  1450  1683 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:48:17.471764  1450  1683 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:48:17.476334   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:48:17.688075  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.689348  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.689647  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.706108  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.707797  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.708750  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.715234  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.716865  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.717731  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.723820  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.724997  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.725829  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.750119  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.765402  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.765837  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.797910  1450  1634 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:17.798793  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:17.803246  1450  1683 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.809079  1450 29539 D DCT     : [0]phoneSubId = 1
10-17 14:48:17.809380  1450 29539 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:17.815811  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.817961  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.826750  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:48:17.827193  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.831391  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:17.834536  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:48:17.839062   909  1551 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:17.839425   909  1551 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:17.840781  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:17.840989  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:48:17.851709   909  1512 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:17.852073   909  1512 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:17.854785  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:17.855041  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:48:17.855390  1450  1450 D RILJ    : [9592]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:48:17.858467  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:17.860190   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:48:17.860265  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:17.860307   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cf9d20, pRI=0x7f9784cd80, p=0x7f978583e0, pUCI=0x0
10-17 14:48:17.860347   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f978583e0 dispatched to RIL_CMD_PROXY_3
10-17 14:48:17.860473   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:17.860472   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:17.860523   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:17.860561   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:17.860556   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:17.860596   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:17.860649   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:17.860709   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:17.860737   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:17.861147   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:17.861230   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:17.861286   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:17.861322   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:17.861357   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cd80 p=0x7f978583e0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:17.861392   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:17.861425   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:48:17.861454   721   749 D RIL     : radioState:10
10-17 14:48:17.861499   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:48:17.861547   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:48:17.861581   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.861610   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:48:17.861636   721   749 I AT      : AT write start
10-17 14:48:17.861817   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:17.861844   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:17.861824   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:17.861884   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:17.861887   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:17.861930   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:17.861945   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:17.861946   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:17.861968   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:17.862013   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:17.862010   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:17.862045   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:17.862123   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:17.863113   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:17.863448   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:17.863547   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:17.863626   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:17.863716   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:17.863770   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:17.864242   721   766 I AT      : AT read end: 6
10-17 14:48:17.864334   721   766 D AT      : AT< OK
10-17 14:48:17.864371   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:17.864362  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:48:17.864438   721   766 I AT      : AT read start
10-17 14:48:17.864747   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:17.864820   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:17.864911   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:17.865003   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cd80 p=0x7f978583e0 
10-17 14:48:17.865051   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9d20
10-17 14:48:17.865086   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:17.865371  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:48:17.865515  1450  1606 D RILJ    : [9592]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:48:17.869402  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:17.869512  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:48:17.869646  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.869716  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.870386   909  2707 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.870466   909  2707 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:17.870810   909  2707 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:17.874237  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:17.874351  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:48:17.874478  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.874490  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.874565  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.875124   909  1190 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.875201   909  1190 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:17.875488   909  1190 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:17.879481  1450  2351 D DCT     : [0]phoneSubId = 1
10-17 14:48:17.879665  1450  2351 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:17.884290  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:17.884490  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:48:17.894001  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:17.895623  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:17.896019  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:17.899498  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:48:17.899619  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:48:17.900425  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:48:17.900545  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:48:17.900604  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:48:17.900655  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:48:17.934414  1450 23534 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:17.936758  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:17.964128  1450  4234 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.964281  1450  4234 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.984013  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.988509  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:17.988593  1450 29539 D DCT     : [0]phoneSubId = 1
10-17 14:48:17.988720  1450 29539 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:17.990393  1450 23534 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:17.990560  1450 23534 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:17.995475  1450 20008 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:17.995712  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:17.997797  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:18.000700  1450  4234 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:18.002129  1450  4234 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:18.009199  1450  1634 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:18.009341  1450  1634 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:18.013830  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:18.014377  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:18.019787  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:18.022086  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:18.027131  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:48:18.027566  1450  1683 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:18.027658  1450  1683 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:18.028003  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:18.028426  1450  1634 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:18.028563  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:18.146951  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:48:18.150395  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:18.150521  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:48:18.153099   909  7313 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:18.153650   909  7313 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:18.155410  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:18.155565  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:48:18.159269   909  1632 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:18.159567   909  1632 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:18.166559  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:18.166717  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:48:18.167024  1450  1450 D RILJ    : [9593]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:48:18.171826   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:48:18.171938   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cda900, pRI=0x7f9784cde0, p=0x7f97856540, pUCI=0x0
10-17 14:48:18.171987   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 dispatched to RIL_CMD_PROXY_3
10-17 14:48:18.172099   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:18.172102   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:18.172151   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:18.172188   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:18.172196   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:18.172242   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:18.172270   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:18.172313   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:18.172340   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:18.172673   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:18.172737   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:18.172790   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:18.172810   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:18.172985   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:18.173022   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cde0 p=0x7f97856540 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:18.173056   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:18.173089   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:48:18.173130   721   749 D RIL     : radioState:10
10-17 14:48:18.173175   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:48:18.173207   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:48:18.173210   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:18.173244   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:18.173245   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:18.173273   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:48:18.173290   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:18.173299   721   749 I AT      : AT write start
10-17 14:48:18.173315   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:18.173357   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:18.173383   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:18.173424   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:18.173454   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:18.173499   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:18.173488   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:18.173528   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:18.173549   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:18.173605   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:18.173701   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:18.175121  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:48:18.177195  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:18.177270  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:48:18.177472  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:18.177557  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:18.178154   909   923 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:18.178285   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:18.178558   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:18.179692  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:18.179914  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:48:18.182207   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:18.182297   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:18.182387   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:18.182436   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:18.182712   721   766 I AT      : AT read end: 6
10-17 14:48:18.182766   721   766 D AT      : AT< OK
10-17 14:48:18.182797   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:18.182846   721   766 I AT      : AT read start
10-17 14:48:18.183099   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:18.183103  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:18.183154   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:18.183228  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:18.183206   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:18.183609   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cde0 p=0x7f97856540 
10-17 14:48:18.183647   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda900
10-17 14:48:18.183675   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:18.183711   909  1551 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:18.183814   909  1551 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:18.184052   909  1551 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:18.184389  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:48:18.184481  1450  1606 D RILJ    : [9593]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:48:18.194296  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:18.194426  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:48:18.321193  1450  1450 D RILJ    : [9594]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:18.322988   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43780 
10-17 14:48:18.323037   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43720
10-17 14:48:18.323065   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43730
10-17 14:48:18.323422   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43780 reset to NULL
10-17 14:48:18.323477   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43780
10-17 14:48:18.323505   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43790
10-17 14:48:18.323805   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:18.323873   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaaa0, pRI=0x7f9784c150, p=0x7f97856bd0, pUCI=0x0
10-17 14:48:18.323908   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c150 p=0x7f97856bd0 dispatched to RIL_ATCI_PROXY
10-17 14:48:18.324014   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:18.324033   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:18.324053   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:18.324061   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:18.324095   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:18.324103   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:18.324105   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:18.324125   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:18.324135   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:18.324156   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c150 p=0x7f97856bd0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:18.324180   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:18.324186   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:18.324209   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:18.324218   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:18.324244   721   753 D RIL     : radioState:10
10-17 14:48:18.324245   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:18.324270   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:18.324287   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:18.324307   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:18.324318   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.324352   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:18.324376   721   753 I AT      : AT write start
10-17 14:48:18.324469   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:18.324495   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:18.324558   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:18.324847   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:18.324879   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:18.324908   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:18.324907   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:18.324964   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:18.325089   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:18.325134   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:18.325155   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:18.325167   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:18.325211   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:18.325544   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:18.332547   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:18.332622   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:18.332691   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:18.332733   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:18.332883   721   770 I AT      : AT read end: 6
10-17 14:48:18.332928   721   770 D AT      : AT< OK
10-17 14:48:18.332961   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:18.333005   721   770 I AT      : AT read start
10-17 14:48:18.333051   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.333088   721   753 D RIL     : p_response->success = 1
10-17 14:48:18.333125   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:18.333148   721   753 D RIL     : strLength = 6
10-17 14:48:18.333170   721   753 D RIL     : line = <
10-17 14:48:18.333170   721   753 D RIL     : OK
10-17 14:48:18.333170   721   753 D RIL     : >
10-17 14:48:18.333199   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:18.333246   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:18.333317   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f97856bd0 
10-17 14:48:18.333357   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:48:18.333382   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:18.333640  1450  1606 D RILJ    : [9594]< OEM_HOOK_RAW [B@f9a4b14 [SUB0]
10-17 14:48:18.616789  1450  1450 D RILJ    : [9595]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:18.618628   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:18.618699   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784c240, p=0x7f97856cb0, pUCI=0x0
10-17 14:48:18.618735   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f97856cb0 dispatched to RIL_ATCI_PROXY
10-17 14:48:18.618830   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:18.618831   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:18.618851   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:18.618871   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:18.618877   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:18.618917   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:18.618923   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:18.618924   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:18.618925   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:18.618942   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:18.618974   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:18.619034   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:18.619116   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:18.619133   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:18.619185   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:18.619236   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:18.619287   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:18.619375   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:18.619395   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:18.619413   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:18.619460   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:18.619461   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:18.619513   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:18.619576   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:18.619622   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f97856cb0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:18.619653   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:18.619681   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:18.619705   721   753 D RIL     : radioState:10
10-17 14:48:18.619746   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:18.619778   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.619804   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:18.619828   721   753 I AT      : AT write start
10-17 14:48:18.620001   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:18.620057   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:18.620104   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:18.620188   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:18.627645   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:18.627722   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:18.627792   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:18.627840   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:18.627948   721   770 I AT      : AT read end: 6
10-17 14:48:18.627997   721   770 D AT      : AT< OK
10-17 14:48:18.628027   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:18.628070   721   770 I AT      : AT read start
10-17 14:48:18.628107   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.628140   721   753 D RIL     : p_response->success = 1
10-17 14:48:18.628168   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:18.628191   721   753 D RIL     : strLength = 6
10-17 14:48:18.628214   721   753 D RIL     : line = <
10-17 14:48:18.628214   721   753 D RIL     : OK
10-17 14:48:18.628214   721   753 D RIL     : >
10-17 14:48:18.628241   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:18.628293   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:18.628366   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f97856cb0 
10-17 14:48:18.628409   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:48:18.628436   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:18.628599  1450  1606 D RILJ    : [9595]< OEM_HOOK_RAW [B@d0a3fbd [SUB0]
10-17 14:48:18.836467  1450  1450 D RILJ    : [9596]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:18.838441   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:18.838529   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9160, pRI=0x7f9784c4b0, p=0x7f978570a0, pUCI=0x0
10-17 14:48:18.838564   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c4b0 p=0x7f978570a0 dispatched to RIL_ATCI_PROXY
10-17 14:48:18.838672   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:18.838681   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:18.838713   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:18.838743   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:18.838756   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:18.838795   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:18.838820   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:18.838860   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:18.838885   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:18.838920   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:18.838943   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:18.838980   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:18.839004   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:18.839051   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:18.839075   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:18.839115   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:18.839141   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:18.839140   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:18.839173   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:18.839220   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:18.839224   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:18.839271   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:18.839311   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:18.839343   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:18.839374   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c4b0 p=0x7f978570a0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:18.839403   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:18.839431   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:18.839454   721   753 D RIL     : radioState:10
10-17 14:48:18.839493   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:18.839522   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.839546   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:18.839569   721   753 I AT      : AT write start
10-17 14:48:18.839714   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:18.839764   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:18.839811   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:18.839892   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:18.847422   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:18.847566   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:18.847642   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:18.847694   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:18.847825   721   770 I AT      : AT read end: 6
10-17 14:48:18.847865   721   770 D AT      : AT< OK
10-17 14:48:18.847893   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:18.847933   721   770 I AT      : AT read start
10-17 14:48:18.847982   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:18.848028   721   753 D RIL     : p_response->success = 1
10-17 14:48:18.848055   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:18.848078   721   753 D RIL     : strLength = 6
10-17 14:48:18.848103   721   753 D RIL     : line = <
10-17 14:48:18.848103   721   753 D RIL     : OK
10-17 14:48:18.848103   721   753 D RIL     : >
10-17 14:48:18.848132   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:18.848179   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:18.848254   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c4b0 p=0x7f978570a0 
10-17 14:48:18.848288   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9160
10-17 14:48:18.848313   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:18.848462  1450  1606 D RILJ    : [9596]< OEM_HOOK_RAW [B@5f6e9b2 [SUB0]
10-17 14:48:19.276126  1450  1450 D RILJ    : [9597]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:19.280179   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:19.280259   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda760, pRI=0x7f9784c510, p=0x7f978563f0, pUCI=0x0
10-17 14:48:19.280292   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c510 p=0x7f978563f0 dispatched to RIL_ATCI_PROXY
10-17 14:48:19.280397   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:19.280431   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:19.280467   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:19.280473   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:19.280497   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:19.280611   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:19.280642   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:19.280681   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:19.280704   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:19.280721   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:19.280747   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:19.280765   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:19.280814   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:19.280846   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:19.280889   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c510 p=0x7f978563f0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:19.280986   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:19.280989   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:19.281020   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:19.281028   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:19.281057   721   753 D RIL     : radioState:10
10-17 14:48:19.281100   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:19.281101   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:19.281110   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:19.281136   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:19.281137   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.281167   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:19.281182   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:19.281189   721   753 I AT      : AT write start
10-17 14:48:19.281234   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:19.281258   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:19.281293   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:19.281382   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:19.281526   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:19.281576   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:19.281628   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:19.281710   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:19.290502   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:19.290626   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:19.290709   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:19.290765   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:19.291764   721   770 I AT      : AT read end: 6
10-17 14:48:19.291829   721   770 D AT      : AT< OK
10-17 14:48:19.291865   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:19.291911   721   770 I AT      : AT read start
10-17 14:48:19.292091   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.292153   721   753 D RIL     : p_response->success = 1
10-17 14:48:19.292184   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:19.292213   721   753 D RIL     : strLength = 6
10-17 14:48:19.292237   721   753 D RIL     : line = <
10-17 14:48:19.292237   721   753 D RIL     : OK
10-17 14:48:19.292237   721   753 D RIL     : >
10-17 14:48:19.292267   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:19.292323   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:19.292409   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c510 p=0x7f978563f0 
10-17 14:48:19.292442   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:48:19.292468   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:19.292912  1450  1606 D RILJ    : [9597]< OEM_HOOK_RAW [B@701ed03 [SUB0]
10-17 14:48:19.505096  1450  1450 D RILJ    : [9598]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:19.510086   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:19.510238   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdabc0, pRI=0x7f9784c360, p=0x7f978567e0, pUCI=0x0
10-17 14:48:19.510291   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f978567e0 dispatched to RIL_ATCI_PROXY
10-17 14:48:19.510452   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:19.510504   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:19.510548   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:19.510561   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:19.510583   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:19.510627   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:19.510651   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:19.510650   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:19.510656   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:19.510704   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:19.510751   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:19.510795   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:19.510851   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:19.510887   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:19.511023   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:19.511055   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:19.511050   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:19.511089   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:19.511128   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:19.511185   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:19.511206   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:19.511220   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:19.511247   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f978567e0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:19.511260   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:19.511283   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:19.511290   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:19.511322   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:19.511354   721   753 D RIL     : radioState:10
10-17 14:48:19.511406   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:19.511449   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.511485   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:19.511513   721   753 I AT      : AT write start
10-17 14:48:19.511756   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:19.511839   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:19.511897   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:19.512010   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:19.519981   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:19.520121   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:19.520236   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:19.520289   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:19.520488   721   770 I AT      : AT read end: 6
10-17 14:48:19.520551   721   770 D AT      : AT< OK
10-17 14:48:19.520627   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:19.520684   721   770 I AT      : AT read start
10-17 14:48:19.521726   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.521820   721   753 D RIL     : p_response->success = 1
10-17 14:48:19.521852   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:19.521880   721   753 D RIL     : strLength = 6
10-17 14:48:19.521907   721   753 D RIL     : line = <
10-17 14:48:19.521907   721   753 D RIL     : OK
10-17 14:48:19.521907   721   753 D RIL     : >
10-17 14:48:19.521943   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:19.522014   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:19.522099   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f978567e0 
10-17 14:48:19.522154   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdabc0
10-17 14:48:19.522183   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:19.522668  1450  1606 D RILJ    : [9598]< OEM_HOOK_RAW [B@55b0480 [SUB0]
10-17 14:48:19.648455  1450  1450 D RILJ    : [9599]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:19.651920   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:19.652026   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784c3f0, p=0x7f97857110, pUCI=0x0
10-17 14:48:19.652068   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f97857110 dispatched to RIL_ATCI_PROXY
10-17 14:48:19.652227   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:19.652227   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:19.652274   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:19.652277   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:19.652317   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c3f0 p=0x7f97857110 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:19.652319   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:19.652318   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:19.652352   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:19.652357   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:19.652394   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:19.652396   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:19.652399   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:19.652424   721   753 D RIL     : radioState:10
10-17 14:48:19.652429   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:19.652469   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:19.652500   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:19.652504   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.652529   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:19.652533   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:19.652559   721   753 I AT      : AT write start
10-17 14:48:19.652570   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:19.652596   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:19.652635   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:19.652660   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:19.652662   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:19.652694   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:19.652740   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:19.652732   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:19.652772   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:19.652869   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:19.652945   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:19.652999   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:19.653089   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:19.653154   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:19.653184   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:19.653228   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:19.654611   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:19.654722   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:19.654805   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:19.654861   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:19.655021   721   770 I AT      : AT read end: 6
10-17 14:48:19.655088   721   770 D AT      : AT< OK
10-17 14:48:19.655123   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:19.655179   721   770 I AT      : AT read start
10-17 14:48:19.655239   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:19.655281   721   753 D RIL     : p_response->success = 1
10-17 14:48:19.655309   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:19.655332   721   753 D RIL     : strLength = 6
10-17 14:48:19.655356   721   753 D RIL     : line = <
10-17 14:48:19.655356   721   753 D RIL     : OK
10-17 14:48:19.655356   721   753 D RIL     : >
10-17 14:48:19.655385   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:19.655438   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:19.655520   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c3f0 p=0x7f97857110 
10-17 14:48:19.655563   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:48:19.655590   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:19.655843  1450  1606 D RILJ    : [9599]< OEM_HOOK_RAW [B@e201ab9 [SUB0]
10-17 14:48:20.442047  1450  1450 D RILJ    : [9600]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:20.449887   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:20.450096   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaaa0, pRI=0x7f9784c6f0, p=0x7f978571f0, pUCI=0x0
10-17 14:48:20.450221   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978571f0 dispatched to RIL_ATCI_PROXY
10-17 14:48:20.450393   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:20.450393   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:20.450469   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:20.450515   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:20.450531   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:20.450517   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:20.450550   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:20.450605   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:20.450617   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:20.450632   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:20.450670   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:20.450704   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:20.450737   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:20.450742   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:20.450789   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c6f0 p=0x7f978571f0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:20.450801   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:20.450827   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:20.450826   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:20.450868   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:20.450889   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:20.450984   721   753 D RIL     : radioState:10
10-17 14:48:20.450984   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:20.451045   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:20.451086   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:20.451117   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:20.451144   721   753 I AT      : AT write start
10-17 14:48:20.452239   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:20.452368   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:20.452443   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:20.452613   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:20.452764   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:20.452764   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:20.452826   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:20.452907   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:20.452903   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:20.452964   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:20.460133   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:20.460238   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:20.460320   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:20.460368   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:20.460530   721   770 I AT      : AT read end: 6
10-17 14:48:20.460608   721   770 D AT      : AT< OK
10-17 14:48:20.460644   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:20.460703   721   770 I AT      : AT read start
10-17 14:48:20.460764   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:20.460816   721   753 D RIL     : p_response->success = 1
10-17 14:48:20.460844   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:20.460869   721   753 D RIL     : strLength = 6
10-17 14:48:20.461099   721   753 D RIL     : line = <
10-17 14:48:20.461099   721   753 D RIL     : OK
10-17 14:48:20.461099   721   753 D RIL     : >
10-17 14:48:20.461178   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:20.461260   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:20.461373   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c6f0 p=0x7f978571f0 
10-17 14:48:20.461426   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaaa0
10-17 14:48:20.461459   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:20.461847  1450  1606 D RILJ    : [9600]< OEM_HOOK_RAW [B@fe5eefe [SUB0]
10-17 14:48:20.705459  1450  1450 D RILJ    : [9601]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:20.710113   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:20.710222   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda760, pRI=0x7f9784c960, p=0x7f978565b0, pUCI=0x0
10-17 14:48:20.710266   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c960 p=0x7f978565b0 dispatched to RIL_ATCI_PROXY
10-17 14:48:20.710371   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:20.710418   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:20.710418   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:20.710458   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:20.710501   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:20.710501   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:20.710522   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:20.710531   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:20.710558   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:20.710604   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:20.710628   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:20.710749   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:20.710848   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:20.710975   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c960 p=0x7f978565b0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:20.710997   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:20.711017   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:20.711026   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:20.711048   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:20.711073   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:20.711076   721   753 D RIL     : radioState:10
10-17 14:48:20.711095   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:20.711103   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:20.711121   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:20.711144   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:20.711153   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:20.711157   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:20.711207   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:20.711212   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:20.711233   721   753 I AT      : AT write start
10-17 14:48:20.711253   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:20.712543   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:20.712645   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:20.712726   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:20.712771   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:20.713717   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:20.713860   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:20.721629   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:20.721744   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:20.721851   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:20.721907   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:20.722055   721   770 I AT      : AT read end: 6
10-17 14:48:20.722123   721   770 D AT      : AT< OK
10-17 14:48:20.722162   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:20.722217   721   770 I AT      : AT read start
10-17 14:48:20.722913   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:20.722999   721   753 D RIL     : p_response->success = 1
10-17 14:48:20.723032   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:20.723061   721   753 D RIL     : strLength = 6
10-17 14:48:20.723090   721   753 D RIL     : line = <
10-17 14:48:20.723090   721   753 D RIL     : OK
10-17 14:48:20.723090   721   753 D RIL     : >
10-17 14:48:20.723124   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:20.723191   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:20.723296   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c960 p=0x7f978565b0 
10-17 14:48:20.723335   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda760
10-17 14:48:20.723370   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:20.723717  1450  1606 D RILJ    : [9601]< OEM_HOOK_RAW [B@a2c565f [SUB0]
10-17 14:48:20.732561   721   760 I RILC    : NUMBER:1
10-17 14:48:20.732636   721   760 I RILC    : arg len:14
10-17 14:48:20.732675   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:48:20.732841   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:48:20.732923   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c150 p=0x7f97856bd0 dispatched to RIL_CMD_PROXY_1
10-17 14:48:20.733067   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:20.733120   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:20.733161   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:20.733167   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:20.733179   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:20.733184   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:20.733209   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:48:20.733209   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:20.733250   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784c150 p=0x7f97856bd0 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:48:20.733270   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:20.733294   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:48:20.733299   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:20.733333   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:48:20.733361   721   751 D RIL     : radioState:10
10-17 14:48:20.733361   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:20.733398   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:20.733412   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:48:20.733445   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:20.733464   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:48:20.733472   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:20.733498   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:20.733526   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:20.733530   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:48:20.733561   721   751 I AT      : AT write start
10-17 14:48:20.733594   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:20.733625   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:20.733689   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:20.733720   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:20.733787   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:20.733853   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:20.733882   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:20.733909   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:20.733976   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:20.734040   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:48:20.734053   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:20.734085   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:20.734147   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:48:20.741706   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:48:20.741891   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:20.741989   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:48:20.742043   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:20.742103   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:48:20.742147   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:20.742220   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:48:20.742263   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:20.742399   721   768 I AT      : AT read end: 46
10-17 14:48:20.742451   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:20.742483   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:20.742543   721   768 D AT      : AT< OK
10-17 14:48:20.742637   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:48:20.742678   721   768 I AT      : AT read start
10-17 14:48:20.742746   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:20.742799   721   751 D RIL     : requestQueryThermal success
10-17 14:48:20.742834   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:20.742865   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:48:20.742908   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:48:20.742975   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784c150 p=0x7f97856bd0 
10-17 14:48:20.743016   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9d00
10-17 14:48:20.743058   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:20.864450  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:21.175550  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:21.197149  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:21.197575  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:21.331789  1450  1450 D RILJ    : [9602]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:21.349306   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:21.349422   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cda960, pRI=0x7f9784c240, p=0x7f978572d0, pUCI=0x0
10-17 14:48:21.349466   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f978572d0 dispatched to RIL_ATCI_PROXY
10-17 14:48:21.349595   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:21.349595   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:21.349634   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:21.349652   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:21.349657   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:21.349692   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c240 p=0x7f978572d0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:21.349684   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:21.349705   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:21.349721   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:21.349726   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:21.349764   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:21.349764   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:21.349793   721   753 D RIL     : radioState:10
10-17 14:48:21.349818   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:21.349836   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:21.349845   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:21.349867   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:21.349882   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:21.349894   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:21.349917   721   753 I AT      : AT write start
10-17 14:48:21.350027   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:21.350058   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:21.350098   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:21.350126   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:21.350271   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:21.350341   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:21.350354   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:21.350395   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:21.350401   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:21.350445   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:21.350475   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:21.350508   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:21.350517   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:21.350545   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:21.350593   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:21.350617   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:21.359028   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:21.359245   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:21.359398   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:21.359500   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:21.361247   721   770 I AT      : AT read end: 6
10-17 14:48:21.361399   721   770 D AT      : AT< OK
10-17 14:48:21.361446   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:21.361532   721   770 I AT      : AT read start
10-17 14:48:21.361679   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:21.361749   721   753 D RIL     : p_response->success = 1
10-17 14:48:21.361788   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:21.361820   721   753 D RIL     : strLength = 6
10-17 14:48:21.361859   721   753 D RIL     : line = <
10-17 14:48:21.361859   721   753 D RIL     : OK
10-17 14:48:21.361859   721   753 D RIL     : >
10-17 14:48:21.361900   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:21.361977   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:21.362092   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c240 p=0x7f978572d0 
10-17 14:48:21.362156   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda960
10-17 14:48:21.362201   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:21.362568  1450  1606 D RILJ    : [9602]< OEM_HOOK_RAW [B@3abe8ac [SUB0]
10-17 14:48:21.421652  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:21.461981  1450  1515 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:21.462539  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:21.482778  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:21.492781  1450 21807 D DCT     : [0]phoneSubId = 1
10-17 14:48:21.493101  1450 21807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:22.002681   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:48:22.002793   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:48:22.002875   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:48:22.002925   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:22.003056   721   765 I AT      : AT read end: 37
10-17 14:48:22.003150   721   765 D AT      : AT< +ECSQ: 42,99,-276,1,1,1,1,3,32767
10-17 14:48:22.003182   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 42,99,-276,1,1,1,1,3,32767
10-17 14:48:22.003230   721   765 D RIL     : Nw URC:+ECSQ: 42,99,-276,1,1,1,1,3,32767
10-17 14:48:22.003311   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:48:22.003350   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:48:22.003381   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:22.003445   721   765 I AT      : AT read start
10-17 14:48:22.003887  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:48:22.004156  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:48:22.004243  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -276 1 1
10-17 14:48:22.004288  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:22.459307   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185329/0
10-17 14:48:25.120005  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:25.120496  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.BATTERY_CHANGED
10-17 14:48:25.278894  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:48:25.282456  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB0]
10-17 14:48:25.282708  1450  1450 D RILJ    : [9603]> SCREEN_STATE: false [SUB0]
10-17 14:48:25.285750  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:48:25.286593   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:48:25.286689   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf9240, pRI=0x7f9784c810, p=0x7f97857340, pUCI=0x0
10-17 14:48:25.286730   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c810 p=0x7f97857340 dispatched to RIL_CMD_PROXY_3
10-17 14:48:25.286882   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.286902   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.286920   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.286975   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.286979   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:25.287007   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.287055   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.287059   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.287068   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.287086   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.287104   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c810 p=0x7f97857340 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.287131   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.287138   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.287156   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.287169   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:25.287202   721   749 D RIL     : radioState:10
10-17 14:48:25.287267   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.287275   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.287295   721   749 D AT      : AT> AT+CREG=1
10-17 14:48:25.287319   721   749 I AT      : AT write start
10-17 14:48:25.287335   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.287338   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.287398   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.287453   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.287462   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.287484   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.287519   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.287545   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.287583   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.287608   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.287862   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.290341   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.290406   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.290456   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.290541   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:25.290784  1450  1450 D RILJ    : defaultDisplayState: 1, isDevicePlugged: false [SUB1]
10-17 14:48:25.291021  1450  1450 D RILJ    : [9604]> SCREEN_STATE: false [SUB1]
10-17 14:48:25.293032   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:48:25.293128   721   760 I RILC-MTK: create request 61: pRequest=0x7f94ce6aa0, pRI=0x7f9784ca50, p=0x7f97856690, pUCI=0x0
10-17 14:48:25.293168   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784ca50 p=0x7f97856690 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.293283   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.293300   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.293319   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.293346   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.293364   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.293378   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.293409   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.293416   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.293456   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.293471   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.293488   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.293488   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.293502   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.293526   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784ca50 p=0x7f97856690 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.293557   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.293558   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.293586   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.293549   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.293632   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:25.293887   721   755 D RIL     : radioState:0
10-17 14:48:25.293699   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.293929   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.293960   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.293969   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.293985   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.294022   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.294048   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.294083   721   755 D AT      : AT> AT+CREG=1
10-17 14:48:25.294108   721   755 I AT      : AT write start
10-17 14:48:25.294212   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.294256   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.294269   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.294302   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.294309   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.294362   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.294446   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:25.297986   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.298060   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.298127   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.298185   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.298284   721   766 I AT      : AT read end: 6
10-17 14:48:25.298324   721   766 D AT      : AT< OK
10-17 14:48:25.298352   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.298390   721   766 I AT      : AT read start
10-17 14:48:25.298430   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.298495   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.298523   721   749 D AT      : AT> AT+CGREG=1
10-17 14:48:25.298546   721   749 I AT      : AT write start
10-17 14:48:25.298680   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.298733   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.298826   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.298900   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:25.298910   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.298957   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.299018   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.299063   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.299817   721   772 I AT      : AT read end: 6
10-17 14:48:25.299861   721   772 D AT      : AT< OK
10-17 14:48:25.299890   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.299935   721   772 I AT      : AT read start
10-17 14:48:25.300037   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.300091   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.300117   721   755 D AT      : AT> AT+CGREG=1
10-17 14:48:25.300141   721   755 I AT      : AT write start
10-17 14:48:25.300319   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.300375   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.300428   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.300507   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:25.301105   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.301173   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.301244   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.301295   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.301346   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.301389   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.301443   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.301481   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.301591   721   766 I AT      : AT read end: 6
10-17 14:48:25.301638   721   766 D AT      : AT< OK
10-17 14:48:25.301666   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.301706   721   766 I AT      : AT read start
10-17 14:48:25.301892   721   772 I AT      : AT read end: 6
10-17 14:48:25.301933   721   772 D AT      : AT< OK
10-17 14:48:25.301962   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.302003   721   772 I AT      : AT read start
10-17 14:48:25.302058   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.302102   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.302128   721   755 D AT      : AT> AT+ECSQ=0
10-17 14:48:25.302149   721   755 I AT      : AT write start
10-17 14:48:25.302633   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.302699   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.302725   721   749 D AT      : AT> AT+ECSQ=0
10-17 14:48:25.302750   721   749 I AT      : AT write start
10-17 14:48:25.302900   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.302900   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.302962   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.302961   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.303016   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.303098   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:25.303172   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.303249   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:25.305046   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.305116   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.305187   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.305232   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.305279   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.305321   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.305369   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.305408   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.305503   721   766 I AT      : AT read end: 6
10-17 14:48:25.305504   721   772 I AT      : AT read end: 6
10-17 14:48:25.305548   721   772 D AT      : AT< OK
10-17 14:48:25.305548   721   766 D AT      : AT< OK
10-17 14:48:25.305579   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.305579   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.305620   721   772 I AT      : AT read start
10-17 14:48:25.305629   721   766 I AT      : AT read start
10-17 14:48:25.305690   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.305725   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.305749   721   755 D AT      : AT> AT+PSBEARER=0
10-17 14:48:25.305771   721   755 I AT      : AT write start
10-17 14:48:25.305798   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.305831   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.305855   721   749 D AT      : AT> AT+PSBEARER=0
10-17 14:48:25.305877   721   749 I AT      : AT write start
10-17 14:48:25.305901   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.305947   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.305981   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.305992   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.306018   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.306069   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:48:25.306146   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.306237   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:48:25.307547   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.307607   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.307672   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.307711   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.307821   721   772 I AT      : AT read end: 6
10-17 14:48:25.307855   721   772 D AT      : AT< OK
10-17 14:48:25.307883   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.307922   721   772 I AT      : AT read start
10-17 14:48:25.307967   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.308017   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.308044   721   755 D AT      : AT> AT+CEREG=1
10-17 14:48:25.308096   721   755 I AT      : AT write start
10-17 14:48:25.308226   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.308242   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.308277   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.308284   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.308332   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.308334   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.308378   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.308408   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:25.308480   721   766 I AT      : AT read end: 6
10-17 14:48:25.308522   721   766 D AT      : AT< OK
10-17 14:48:25.308549   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.308584   721   766 I AT      : AT read start
10-17 14:48:25.308623   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.308680   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.308713   721   749 D AT      : AT> AT+CEREG=1
10-17 14:48:25.308735   721   749 I AT      : AT write start
10-17 14:48:25.308847   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.308898   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.308946   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.309556   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.309615   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.309677   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.309720   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.309814   721   772 I AT      : AT read end: 6
10-17 14:48:25.309853   721   772 D AT      : AT< OK
10-17 14:48:25.309881   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.309923   721   772 I AT      : AT read start
10-17 14:48:25.309960   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.309996   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.310035   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.310100   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ca50 p=0x7f97856690 
10-17 14:48:25.310131   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:48:25.310156   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.310627  1450  1609 D RILJ    : [9604]< SCREEN_STATE  [SUB1]
10-17 14:48:25.311121   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:25.312576   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.312643   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.312708   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.312750   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.312869   721   766 I AT      : AT read end: 6
10-17 14:48:25.312910   721   766 D AT      : AT< OK
10-17 14:48:25.312938   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.312974   721   766 I AT      : AT read start
10-17 14:48:25.313018   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.313066   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.313107   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.313173   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c810 p=0x7f97857340 
10-17 14:48:25.313203   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9240
10-17 14:48:25.313228   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:25.313327  1450  1606 D RILJ    : [9603]< SCREEN_STATE  [SUB0]
10-17 14:48:25.534739  1450  1450 D RILJ    : [9605]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:25.536674   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:25.536759   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cc3ee0, pRI=0x7f9784c210, p=0x7f97856930, pUCI=0x0
10-17 14:48:25.536794   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856930 dispatched to RIL_ATCI_PROXY
10-17 14:48:25.536900   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.536906   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.536936   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.536950   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.536939   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.536980   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.536981   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.537028   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.537060   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.537073   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.537092   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:25.537098   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.537124   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c210 p=0x7f97856930 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:25.537131   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.537155   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.537186   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.537193   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:25.537226   721   753 D RIL     : radioState:10
10-17 14:48:25.537246   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.537263   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:25.537271   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.537294   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:25.537313   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.537320   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:25.537334   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:25.537340   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.537353   721   753 I AT      : AT write start
10-17 14:48:25.537367   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:25.537441   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.537466   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.537502   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.537526   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.537631   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.537683   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.537733   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:25.537814   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:25.539563   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:25.539644   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:25.539716   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:25.539758   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.539944   721   770 I AT      : AT read end: 6
10-17 14:48:25.539999   721   770 D AT      : AT< OK
10-17 14:48:25.540031   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:25.540072   721   770 I AT      : AT read start
10-17 14:48:25.540143   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:25.540175   721   753 D RIL     : p_response->success = 1
10-17 14:48:25.540218   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:25.540242   721   753 D RIL     : strLength = 6
10-17 14:48:25.540264   721   753 D RIL     : line = <
10-17 14:48:25.540264   721   753 D RIL     : OK
10-17 14:48:25.540264   721   753 D RIL     : >
10-17 14:48:25.540291   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.540336   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.540400   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c210 p=0x7f97856930 
10-17 14:48:25.540447   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc3ee0
10-17 14:48:25.540473   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.540632  1450  1606 D RILJ    : [9605]< OEM_HOOK_RAW [B@21ea975 [SUB0]
10-17 14:48:25.671143  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.672961  1450  1511 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.673089  1450  1511 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.674008  1450  1634 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:25.674194  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:25.692980  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.693084  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.698731  1450 29539 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.698861  1450 29539 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.706871  1450  1752 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.706999  1450  1752 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.723368  1450 23534 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.725677  1450  1683 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.725809  1450  1683 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.731355  1450  1515 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:25.731552  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:25.743132  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB0]
10-17 14:48:25.749449  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB0]
10-17 14:48:25.749647  1450  1450 D RILJ    : [9606]> SCREEN_STATE: true [SUB0]
10-17 14:48:25.752934  1450  1450 D RILJ    : onDisplayChanged: displayId = 0 [SUB1]
10-17 14:48:25.753487   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: SCREEN_STATE length:16
10-17 14:48:25.753595   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cf91e0, pRI=0x7f9784c840, p=0x7f97856fc0, pUCI=0x0
10-17 14:48:25.753634   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c840 p=0x7f97856fc0 dispatched to RIL_CMD_PROXY_3
10-17 14:48:25.753731   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.753775   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.753822   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.753851   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.753866  1450  1450 D RILJ    : defaultDisplayState: 2, isDevicePlugged: false [SUB1]
10-17 14:48:25.753890   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.753916   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.753957   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.753984   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.754009  1450  1450 D RILJ    : [9607]> SCREEN_STATE: true [SUB1]
10-17 14:48:25.754190   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:25.754242   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.754248   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.754278   721   749 D RILC-MTK: SCREEN_STATE pRI=0x7f9784c840 p=0x7f97856fc0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.754283   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.754311   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.754330   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.754344   721   749 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:25.754357   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.754371   721   749 D RIL     : radioState:10
10-17 14:48:25.754396   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.754420   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.754435   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.754460   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.754467   721   749 D AT      : AT> AT+CREG=3
10-17 14:48:25.754490   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.754492   721   749 I AT      : AT write start
10-17 14:48:25.754726   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.754795   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.754869   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.754968   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:25.755269   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.755306   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.755465   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.755497   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.755657   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.755691   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.756233   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: SCREEN_STATE length:16
10-17 14:48:25.756306   721   760 I RILC-MTK: create request 61: pRequest=0x7f94cdabc0, pRI=0x7f9784cae0, p=0x7f978573b0, pUCI=0x0
10-17 14:48:25.756338   721   760 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cae0 p=0x7f978573b0 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.756430   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.756466   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.756506   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.756512   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.756537   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.756569   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.756589   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.756601   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.756639   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.756644   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.756666   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.756702   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.756741   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.756790   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.756825   721   755 D RILC-MTK: SCREEN_STATE pRI=0x7f9784cae0 p=0x7f978573b0 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.756856   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.756887   721   755 D RIL     : onRequest: SCREEN_STATE, datalen = 4
10-17 14:48:25.756912   721   755 D RIL     : radioState:0
10-17 14:48:25.756951   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.756977   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.757003   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.757054   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.757086   721   755 D AT      : AT> AT+CREG=3
10-17 14:48:25.757110   721   755 I AT      : AT write start
10-17 14:48:25.757273   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.757334   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.757386   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.757475   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:25.758451   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.758523   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.758583   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.758610   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.758649   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.758673   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.758712   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.758737   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.763010   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:36
10-17 14:48:25.763113   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 2 to /dev/pts/2
10-17 14:48:25.763194   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/2
10-17 14:48:25.763239   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.763298   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.763339   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.763426   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.763468   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.763731   721   766 I AT      : AT read end: 6
10-17 14:48:25.763794   721   766 D AT      : AT< OK
10-17 14:48:25.763811   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:7, ctrl:239, len:36
10-17 14:48:25.763828   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.763870   721   766 I AT      : AT read start
10-17 14:48:25.763874   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 36 byte frame received on channel 7 to /dev/pts/8
10-17 14:48:25.763611   721   765 I AT      : AT read end: 36
10-17 14:48:25.763949   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 36/36 bytes of frame to /dev/pts/8
10-17 14:48:25.763954   721   765 D AT      : AT< +CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:25.763983   721   765 D AT      : RIL_URC_READER Enter processLine:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:25.763993   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.764028   721   765 D RIL     : Nw URC:+CREG: 1,"1B5C","00000DFF",3,0,0
10-17 14:48:25.764041   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.764061   721   765 D RIL     : NW state changed: normal case
10-17 14:48:25.764079   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.764090   721   765 D RIL     : The URC is "1B5C","00000DFF",3,0,0
10-17 14:48:25.764121   721   765 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:25.764130   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.764149   721   765 D RIL     : onNetworkStateChanged() , stat=1 , is_cs=1
10-17 14:48:25.764167   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.764199   721   765 D RIL     : +creg urc <ci>: 3583
10-17 14:48:25.764232   721   765 D RIL     : bCREGType3Support=1
10-17 14:48:25.764239   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.764259   721   765 D RIL     : now +creg urc <cause_type>: 0
10-17 14:48:25.764284   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.764284   721   765 D RIL     : now +creg urc <cause>: 0
10-17 14:48:25.764313   721   749 D AT      : AT> AT+CGREG=3
10-17 14:48:25.764337   721   749 I AT      : AT write start
10-17 14:48:25.764367   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:48:25.764395   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.764458   721   765 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e433c0
10-17 14:48:25.764481   721   771 I AT      : AT read end: 36
10-17 14:48:25.764493   721   765 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e433d0
10-17 14:48:25.764510   721   771 D AT      : AT< +CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:25.764537   721   771 D AT      : RIL_URC2_READER Enter processLine:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:25.764578   721   771 D RIL     : Nw URC:+CREG: 0,"0000","0FFFFFFF",0,0,0
10-17 14:48:25.764588   721   765 I AT      : AT read start
10-17 14:48:25.764610   721   771 D RIL     : NW state changed: normal case
10-17 14:48:25.764639   721   771 D RIL     : The URC is "0000","0FFFFFFF",0,0,0
10-17 14:48:25.764671   721   771 D RIL     : convertRegState() uiRegState=0 , uiRet=0 
10-17 14:48:25.764701   721   771 D RIL     : onNetworkStateChanged() , stat=0 , is_cs=1
10-17 14:48:25.764709   721   772 I AT      : AT read end: 6
10-17 14:48:25.764741   721   772 D AT      : AT< OK
10-17 14:48:25.764748   721   771 D RIL     : +creg urc <ci>: 268435455
10-17 14:48:25.764768   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.764783   721   771 D RIL     : bCREGType3Support=1
10-17 14:48:25.764805   721   772 I AT      : AT read start
10-17 14:48:25.764810   721   771 D RIL     : now +creg urc <cause_type>: 0
10-17 14:48:25.764837   721   771 D RIL     : now +creg urc <cause>: 0
10-17 14:48:25.764895   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.764913   721   771 I RILC    : RIL_SOCKET_2 UNSOLICITED: UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED length:64
10-17 14:48:25.764943   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.764941   721   771 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.764972   721   755 D AT      : AT> AT+CGREG=3
10-17 14:48:25.764995   721   755 I AT      : AT write start
10-17 14:48:25.765006   721   771 D RILC    : s_last_wake_timeout_info: 0x7f94e433c0, cancel
10-17 14:48:25.765041   721   771 D RILC    : internalRequestTimedCallback malloc p_info: 0x7f94e43900
10-17 14:48:25.765073   721   771 D RILC    : internalRequestTimedCallback malloc p_info->event: 0x7f94e43910
10-17 14:48:25.765130   721   771 I AT      : AT read start
10-17 14:48:25.765147   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.765206   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.765258   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.765351   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:25.765411  1450  1606 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {1, 1b5c, dff, 3, 0} [SUB0]
10-17 14:48:25.765641   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.765701   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.765753   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.765847   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:25.765937  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:48:25.766176  1450  1609 V RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED {0, 0, fffffff, 0, 0} [SUB1]
10-17 14:48:25.766179  1450  1450 D GsmSST  : [GsmSST0] onNetworkStateChangeResult state:1 lac:7004 cid:3583 Act:3 cause:0
10-17 14:48:25.766393  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:48:25.766497   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.766563   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.766644   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.766688   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.769007   721   772 I AT      : AT read end: 6
10-17 14:48:25.769060   721   772 D AT      : AT< OK
10-17 14:48:25.769089   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.769134   721   772 I AT      : AT read start
10-17 14:48:25.769194  1450  1450 D PhoneFactory: calculatePreferredNetworkType: phoneSubId = 1 networkType = 1
10-17 14:48:25.769312  1450  1450 D GsmSST  : [GsmSST0] pollState RadioState is RADIO_ON, currentNetworkMode= 1
10-17 14:48:25.769492  1450  1450 D RILJ    : [9608]> OPERATOR [SUB0]
10-17 14:48:25.769552   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.769621   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.769650   721   755 D AT      : AT> AT+ECSQ=1
10-17 14:48:25.769674   721   755 I AT      : AT write start
10-17 14:48:25.769788   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.769852   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.769925   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.769997   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.771292   721   766 I AT      : AT read end: 6
10-17 14:48:25.771270  1450  1450 D RILJ    : [9609]> DATA_REGISTRATION_STATE [SUB0]
10-17 14:48:25.771359   721   766 D AT      : AT< OK
10-17 14:48:25.771393   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.771453   721   766 I AT      : AT read start
10-17 14:48:25.771566   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.771622   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.771675   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.771676   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OPERATOR length:8
10-17 14:48:25.771740   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9120, pRI=0x7f9784cba0, p=0x7f978563f0, pUCI=0x0
10-17 14:48:25.771774   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784cba0 p=0x7f978563f0 dispatched to RIL_CMD_PROXY_3
10-17 14:48:25.771773   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 10
10-17 14:48:25.771887   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.771891   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.771922   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.771963   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.771968   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.771972   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.771990   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.772014   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.772036   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.772044   721   749 D AT      : AT> AT+ECSQ=1
10-17 14:48:25.772063   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.772069   721   749 I AT      : AT write start
10-17 14:48:25.772101   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.772149   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.772176   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.772375   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.772455   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.772483   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.773599   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.773663   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.773714   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.773739   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.773780   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.773805   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.773951   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.774021   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.774077   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.774174   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:25.774285   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.774336   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.774419   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.774471   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.774624   721   772 I AT      : AT read end: 6
10-17 14:48:25.774699   721   772 D AT      : AT< OK
10-17 14:48:25.774733   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.774786   721   772 I AT      : AT read start
10-17 14:48:25.774811  1450  1450 D RILJ    : [9610]> VOICE_REGISTRATION_STATE [SUB0]
10-17 14:48:25.775016   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.775085   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.775115   721   755 D AT      : AT> AT+ECSQ
10-17 14:48:25.775138   721   755 I AT      : AT write start
10-17 14:48:25.775166   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:48:25.775224   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cf9300, pRI=0x7f9784ce10, p=0x7f978567e0, pUCI=0x0
10-17 14:48:25.775258   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cba0 p=0x7f978563f0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.775287   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:25.775305   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.775321   721   760 D RILC-MTK: Request pRI=0x7f9784ce10 to RIL_CMD_PROXY_3 is busy. total:2 requests pending
10-17 14:48:25.775356   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.775410   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.775447   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.775495   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 8
10-17 14:48:25.775493   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.775571   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.775612   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.775858   721   766 I AT      : AT read end: 6
10-17 14:48:25.775912   721   766 D AT      : AT< OK
10-17 14:48:25.775947   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.775989   721   766 I AT      : AT read start
10-17 14:48:25.776042   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.776118   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.776147   721   749 D AT      : AT> AT+ECSQ
10-17 14:48:25.776170   721   749 I AT      : AT write start
10-17 14:48:25.776893   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.776977   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.777032   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.777120   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 8
10-17 14:48:25.777220   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:34
10-17 14:48:25.777272   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 34 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.777366   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 34/34 bytes of frame to /dev/pts/9
10-17 14:48:25.777410   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.777583   721   772 I AT      : AT read end: 34
10-17 14:48:25.777630   721   772 I AT      : AT read start
10-17 14:48:25.777950   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:2
10-17 14:48:25.778039   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 2 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.778132   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 2/2 bytes of frame to /dev/pts/9
10-17 14:48:25.778179   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.778240   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.778281   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.778340   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.778384   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.780015   721   772 I AT      : AT read end: 8
10-17 14:48:25.780036   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:37
10-17 14:48:25.780091   721   772 D AT      : AT< +ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:48:25.780108   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.780122   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+ECSQ: 255,255,1,1,1,1,1,0,32767
10-17 14:48:25.780164   721   772 D AT      : AT< OK
10-17 14:48:25.780190   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.780197   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/3
10-17 14:48:25.780249   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.780248   721   772 I AT      : AT read start
10-17 14:48:25.780312   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.780354   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.780415   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.780421   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.780464   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.780485   721   755 E RIL     : Recevice an invalid value from modem for <rxlevel>
10-17 14:48:25.780533   721   755 E RIL     : updateSignalStrength ERROR: -1
10-17 14:48:25.780595   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.780624   721   755 D AT      : AT> AT+PSBEARER=1
10-17 14:48:25.780655   721   755 I AT      : AT write start
10-17 14:48:25.781006  1450  1450 D RILJ    : [9611]> QUERY_NETWORK_SELECTION_MODE [SUB0]
10-17 14:48:25.780846   721   766 I AT      : AT read end: 43
10-17 14:48:25.781116   721   766 D AT      : AT< +ECSQ: 42,99,-276,1,1,1,1,3,32767
10-17 14:48:25.781157   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+ECSQ: 42,99,-276,1,1,1,1,3,32767
10-17 14:48:25.781202   721   766 D AT      : AT< OK
10-17 14:48:25.781230   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.781282   721   766 I AT      : AT read start
10-17 14:48:25.781422   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.781449   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.781519   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.781545   721   749 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:48:25.781581   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.781591   721   749 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:48:25.781621   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.781683   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 14
10-17 14:48:25.781754   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.781791   721   749 D AT      : AT> AT+PSBEARER=1
10-17 14:48:25.781816   721   749 I AT      : AT write start
10-17 14:48:25.782319   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.782406   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.782487   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.782948   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:48:25.783099   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cf9340, pRI=0x7f9784ce40, p=0x7f97856cb0, pUCI=0x0
10-17 14:48:25.783153   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cba0 p=0x7f978563f0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.783213   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784ce10 p=0x7f978567e0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.783248   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:25.783289   721   760 D RILC-MTK: Request pRI=0x7f9784ce40 to RIL_CMD_PROXY_3 is busy. total:3 requests pending
10-17 14:48:25.783529   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 14
10-17 14:48:25.783706   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.783773   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.783875   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.783927   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.784266   721   772 I AT      : AT read end: 6
10-17 14:48:25.784395   721   772 D AT      : AT< OK
10-17 14:48:25.784442   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.784509   721   772 I AT      : AT read start
10-17 14:48:25.784717   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.784847   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.784884   721   755 D AT      : AT> AT+CEREG=3
10-17 14:48:25.784913   721   755 I AT      : AT write start
10-17 14:48:25.786098   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.786230   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.786308   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.786425   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 11
10-17 14:48:25.789092   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.789216   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.789389   721   766 I AT      : AT read end: 6
10-17 14:48:25.789455   721   766 D AT      : AT< OK
10-17 14:48:25.789489   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.789536   721   766 I AT      : AT read start
10-17 14:48:25.789867   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.789948   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.790014   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.790057   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.790209   721   772 I AT      : AT read end: 6
10-17 14:48:25.790266   721   772 D AT      : AT< OK
10-17 14:48:25.790298   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.790347   721   772 I AT      : AT read start
10-17 14:48:25.790444   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.790519   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.790548   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.790619   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.790671   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.790757   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784cae0 p=0x7f978573b0 
10-17 14:48:25.790806   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdabc0
10-17 14:48:25.790838   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.791159  1450  1609 D RILJ    : [9607]< SCREEN_STATE  [SUB1]
10-17 14:48:25.793090  1450  4234 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.793785   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.793908   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.793969   721   749 D AT      : AT> AT+CEREG=3
10-17 14:48:25.794008   721   749 I AT      : AT write start
10-17 14:48:25.795157  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.795286  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.795656   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.795726   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.795789   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.795909   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:25.796097  1450  1807 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:25.796256  1450  1807 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:25.796823  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.796979  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_NETWORK_STATE_CHANGED
10-17 14:48:25.797067  1450  1450 D GsmSST  : [GsmSST1] onNetworkStateChangeResult state:0 lac:0 cid:268435455 Act:0 cause:0
10-17 14:48:25.797150  1450  1450 I use-Rlog/RLOG-GSM: clear dontUpdateNetworkStateFlag
10-17 14:48:25.797204  1450  1450 D GsmSST  : [GsmSST1] unknown lac:0 or cid:268435455
10-17 14:48:25.797553   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:48:25.797643   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9b80, pRI=0x7f9784cea0, p=0x7f978570a0, pUCI=0x0
10-17 14:48:25.797684   721   760 D RILC-MTK: 1:OPERATOR pRI=0x7f9784cba0 p=0x7f978563f0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.797714   721   760 D RILC-MTK: 2:DATA_REGISTRATION_STATE pRI=0x7f9784ce10 p=0x7f978567e0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.797762   721   760 D RILC-MTK: 3:VOICE_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856cb0 is queued in RIL_CMD_PROXY_3
10-17 14:48:25.797793   721   760 D RILC-MTK: **** the last executed cmd for RIL_CMD_PROXY_3 is SCREEN_STATE ****
10-17 14:48:25.797826   721   760 D RILC-MTK: Request pRI=0x7f9784cea0 to RIL_CMD_PROXY_3 is busy. total:4 requests pending
10-17 14:48:25.798184  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.798435  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.798552  1450  1450 D GsmSST  : [GsmSST1] Invalid subId, return invalid networkType
10-17 14:48:25.798623  1450  1450 D GsmSST  : [GsmSST1] pollState RadioState is RADIO_OFF, currentNetworkMode= -1
10-17 14:48:25.798757  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:48:25.798852  1450  1450 D GsmSST  : [GsmSST1] updateLocatedPlmn(),previous plmn= null ,update to: null
10-17 14:48:25.798923  1450  1450 D GsmSST  : [GsmSST1] mLastCsNetworkType=0, mLastPsNetworkType= 0, mNewSS VoiceRadioTechnology= 0, mSS VoiceRadioTechnology= 0, mNewSS DataRadioTechnology= 0, mSS DataRadioTechnology= 0
10-17 14:48:25.798961  1450  1450 D GsmSST  : [GsmSST1] pollStateDone(): don't change network type and wait for new event
10-17 14:48:25.798997  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=0
10-17 14:48:25.799036  1450  1450 D GsmSST  : [GsmSST1] set service state as POWER_OFF
10-17 14:48:25.799069  1450  1450 D PHONE   : [ServiceState] setNullState=3
10-17 14:48:25.799202  1450  1450 D GsmSST  : [GsmSST1] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 0 Ril Data Regist state: 0 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: -1 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:48:25.799319  1450  1450 D GsmSST  : [GsmSST1] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:false,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:false
10-17 14:48:25.799398  1450  1450 D GsmSST  : [GsmSST1] explict_update_spn trigger to refresh SPN
10-17 14:48:25.799448  1450  1450 D GsmSST  : [GsmSST1] No matched EONS and No CPHS ONS
10-17 14:48:25.799745  1450  1450 D GsmSST  : [GsmSST1] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=false getVoiceRegState()=3 getDataRegState()3
10-17 14:48:25.803523   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.803612   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.803722   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.803742   721   766 I AT      : AT read end: 6
10-17 14:48:25.803771   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.803786   721   766 D AT      : AT< OK
10-17 14:48:25.803823   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.803876   721   766 I AT      : AT read start
10-17 14:48:25.803934   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.803982   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.804029   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.804107   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c840 p=0x7f97856fc0 
10-17 14:48:25.804139   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf91e0
10-17 14:48:25.804174   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.804207   721   749 D RILC-MTK: OPERATOR pRI=0x7f9784cba0 p=0x7f978563f0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.804236   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.804265   721   749 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:48:25.804291   721   749 D RIL     : radioState:10
10-17 14:48:25.804329   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.804323  1450  1606 D RILJ    : [9606]< SCREEN_STATE  [SUB0]
10-17 14:48:25.804364   721   749 D AT      : AT> AT+COPS?
10-17 14:48:25.804386   721   749 I AT      : AT write start
10-17 14:48:25.804587   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.804668   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.804724   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.804828   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:25.805561  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.805724  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.805794  1450  1450 D GsmSST  : [GsmSST1] updateAllOpertorInfo with realPlmn:null
10-17 14:48:25.806928  1450  1450 D GsmSST  : [GsmSST1] old:3 ,mPsRegState:1,new:3
10-17 14:48:25.807143  1450  1450 D RILJ    : [9612]> OPERATOR [SUB1]
10-17 14:48:25.809067  1450  1450 D RILJ    : [9613]> DATA_REGISTRATION_STATE [SUB1]
10-17 14:48:25.809332   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: OPERATOR length:8
10-17 14:48:25.809387   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:48:25.809432   721   760 I RILC-MTK: create request 22: pRequest=0x7f94cf9be0, pRI=0x7f9784ced0, p=0x7f97856c40, pUCI=0x0
10-17 14:48:25.809452   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.809468   721   760 D RILC-MTK: OPERATOR pRI=0x7f9784ced0 p=0x7f97856c40 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.809578   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.809578   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.809623   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.809655   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.809661   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.809671   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.809686   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.809717   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.809736   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.809742   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.809744   721   766 I AT      : AT read end: 24
10-17 14:48:25.809781   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:48:25.809799   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.809806   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.809818   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:48:25.809828   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.809856   721   766 I AT      : AT read start
10-17 14:48:25.809872   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.809946   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.809975   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.810016   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.810027   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:48:25.810062   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.810088   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.810152   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.810224   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.810270   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.810321   721   755 D RILC-MTK: OPERATOR pRI=0x7f9784ced0 p=0x7f97856c40 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.810342   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.810355   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.810391   721   755 D RIL     : onRequest: OPERATOR, datalen = 0
10-17 14:48:25.810417   721   755 D RIL     : radioState:0
10-17 14:48:25.810471   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.810471   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.810502   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.810525   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.810533   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.810562   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.810611   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:25.810642   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.810700   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.810762   721   766 I AT      : AT read end: 6
10-17 14:48:25.810774   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784ced0 p=0x7f97856c40 
10-17 14:48:25.810796   721   766 D AT      : AT< OK
10-17 14:48:25.810812   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9be0
10-17 14:48:25.810826   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.810837   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.811311   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.811410   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.811414  1450  1609 D RilRequest: [9612]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:25.811500   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.810875   721   766 I AT      : AT read start
10-17 14:48:25.811545   721   749 D RIL     : Get operator code 25020
10-17 14:48:25.811582   721   749 D RIL     : Get ril_nw_nitzName_mutex in the getOperatorNamesFromNumericCode
10-17 14:48:25.811624   721   749 D RIL     : Return NITZ Operator Name: 25020 Tele2 , lname length: 5, sname length: 0
10-17 14:48:25.811677   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.811743   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.811813  1450  1450 D RILJ    : [9614]> VOICE_REGISTRATION_STATE [SUB1]
10-17 14:48:25.811838   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cba0 p=0x7f978563f0 
10-17 14:48:25.811883   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9120
10-17 14:48:25.811914   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.811947   721   749 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784ce10 p=0x7f978567e0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.811979   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.812011   721   749 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:48:25.812037   721   749 D RIL     : radioState:10
10-17 14:48:25.812069  1450  1606 D RILJ    : [9608]< OPERATOR {Tele2, Tele2, 25020} [SUB0]
10-17 14:48:25.812091   721   749 D RIL     : request gprs reg state: normal case
10-17 14:48:25.812133   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.812162   721   749 D AT      : AT> AT+CGREG?
10-17 14:48:25.812189   721   749 I AT      : AT write start
10-17 14:48:25.812696   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: DATA_REGISTRATION_STATE length:8
10-17 14:48:25.812786   721   760 I RILC-MTK: create request 21: pRequest=0x7f94cc36c0, pRI=0x7f9784c540, p=0x7f97856e70, pUCI=0x0
10-17 14:48:25.812823   721   760 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c540 p=0x7f97856e70 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.812943   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.812984   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.813028   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.813039   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.813066   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.813104   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.813111   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.813135   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.813173   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.813227   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.813234   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.813264   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.813265   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.813303   721   755 D RILC-MTK: DATA_REGISTRATION_STATE pRI=0x7f9784c540 p=0x7f97856e70 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.813306   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.813338   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.813374   721   755 D RIL     : onRequest: DATA_REGISTRATION_STATE, datalen = 0
10-17 14:48:25.813401   721   755 D RIL     : radioState:0
10-17 14:48:25.813446   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.813460   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.813474   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.813492   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.813500   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.813529   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.813538   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.813563   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.813564   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:25.813595   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.813605   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.813633   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.813640   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.813672   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.813699   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.813697   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c540 p=0x7f97856e70 
10-17 14:48:25.813734   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cc36c0
10-17 14:48:25.813759   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.813875   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.813935   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.813987   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.814079   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 10
10-17 14:48:25.814623  1450  1609 D RilRequest: [9613]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:25.814938  1450  1450 D RILJ    : [9615]> QUERY_NETWORK_SELECTION_MODE [SUB1]
10-17 14:48:25.815195   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: VOICE_REGISTRATION_STATE length:8
10-17 14:48:25.815293   721   760 I RILC-MTK: create request 20: pRequest=0x7f94cda8a0, pRI=0x7f9784c660, p=0x7f97857420, pUCI=0x0
10-17 14:48:25.815333   721   760 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c660 p=0x7f97857420 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.815449   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.815499   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.815500   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.815535   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.815576   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.815585   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.815607   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.815655   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.815661   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.815702   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.815707   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.815730   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.815771   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.815811   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.816521   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.816582   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.816635   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.816662   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.816706   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.816735   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.816777   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:25.816810   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.816845   721   755 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784c660 p=0x7f97857420 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.816876   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.816908   721   755 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:48:25.816902  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:25.816939   721   755 D RIL     : radioState:0
10-17 14:48:25.816990   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.817009  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:48:25.817017   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.817044   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.817069   721   755 I RIL     : isWfcSupport: 0
10-17 14:48:25.817105   721   755 D         : IMS: IMS_isRilRequestFromIms, socket_id = 1 
10-17 14:48:25.817136   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.817186   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.817201   721   760 D RILC    : SOCKET RIL_SOCKET_2 REQUEST: QUERY_NETWORK_SELECTION_MODE length:8
10-17 14:48:25.817255   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c660 p=0x7f97857420 
10-17 14:48:25.817256   721   760 I RILC-MTK: create request 45: pRequest=0x7f94cf9360, pRI=0x7f9784c9c0, p=0x7f97857490, pUCI=0x0
10-17 14:48:25.817294   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda8a0
10-17 14:48:25.817295   721   760 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c9c0 p=0x7f97857490 dispatched to RIL_CMD2_PROXY_3
10-17 14:48:25.817414   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:25.817446   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:25.817486   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:25.817495   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:25.817519   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:25.817510  1450  1609 D RilRequest: [9614]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
10-17 14:48:25.817567   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:25.817619   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:25.817646   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:25.817688   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:25.817701   721   755 D RILC-MTK: proxy id:7, proxyName: RIL_CMD2_PROXY_3
10-17 14:48:25.817708   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:25.817734   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:25.817745   721   755 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784c9c0 p=0x7f97857490 execute on RIL_CMD2_PROXY_3 using channel 7
10-17 14:48:25.817775   721   755 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.817785   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:25.817794   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:25.817807   721   755 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:48:25.817833   721   755 D RIL     : radioState:0
10-17 14:48:25.817833   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:25.817838   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:25.817864   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:25.817879   721   755 D AT      : AT send on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.817903   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:25.817906   721   755 D AT      : AT> AT+COPS?
10-17 14:48:25.817933   721   755 I AT      : AT write start
10-17 14:48:25.817955   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:25.817981   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:25.818014   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:25.818098   537   716 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.818155   537   716 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.818205   537   716 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 8
10-17 14:48:25.818295   537   716 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 8 with length 9
10-17 14:48:25.818314  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:48:25.818492  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -276 1 1
10-17 14:48:25.818546  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.818638  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_OPERATOR
10-17 14:48:25.818686  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult cancelPollState due to RADIO_NOT_AVAILABLE
10-17 14:48:25.818719  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:25.819517  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_OPERATOR
10-17 14:48:25.819684  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:48:25.819739  1450  1450 D UiccController: isValidCardIndex index = 0
10-17 14:48:25.822233   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:44
10-17 14:48:25.822308   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 44 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.822439   721   766 I AT      : AT read end: 44
10-17 14:48:25.822478   721   766 D AT      : AT< +CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:48:25.822508   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CGREG: 3,1,"1B5C","00000DFF",3,"CC",0,0
10-17 14:48:25.822545   721   766 I AT      : AT read start
10-17 14:48:25.822759   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 44/44 bytes of frame to /dev/pts/3
10-17 14:48:25.822813   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.822868   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.822910   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.823113   721   766 I AT      : AT read end: 6
10-17 14:48:25.823159   721   766 D AT      : AT< OK
10-17 14:48:25.823188   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.823234   721   766 I AT      : AT read start
10-17 14:48:25.823293   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.823348   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:25.823377   721   749 E RIL     : The value in the field <lac> :0
10-17 14:48:25.823406   721   749 D RIL     : cid: 3583
10-17 14:48:25.823433   721   749 E RIL     : The value of act: 3
10-17 14:48:25.823459   721   749 D RIL     : cause_type: 0
10-17 14:48:25.823484   721   749 D RIL     : reject_cause: 0
10-17 14:48:25.823525   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.823551   721   749 D AT      : AT> AT+PSBEARER?
10-17 14:48:25.823577   721   749 I AT      : AT write start
10-17 14:48:25.823595   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.823651   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.823723   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.823766   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.823814   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.823904   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 13
10-17 14:48:25.824169   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:12
10-17 14:48:25.824218   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 12 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.824342   721   772 I AT      : AT read end: 12
10-17 14:48:25.824380   721   772 D AT      : AT< +COPS: 0
10-17 14:48:25.824414   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:+COPS: 0
10-17 14:48:25.824449   721   772 I AT      : AT read start
10-17 14:48:25.824950   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 12/12 bytes of frame to /dev/pts/9
10-17 14:48:25.825015   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.825159   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:8, ctrl:239, len:6
10-17 14:48:25.825208   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 8 to /dev/pts/9
10-17 14:48:25.825316   721   772 I AT      : AT read end: 6
10-17 14:48:25.825355   721   772 D AT      : AT< OK
10-17 14:48:25.825387   721   772 D AT      : RIL_CMD2_READER_1 Enter processLine:OK
10-17 14:48:25.825429   721   772 I AT      : AT read start
10-17 14:48:25.825486   721   755 D AT      : response received on RIL_CMD2_READER_1, tid:547980383296
10-17 14:48:25.825536   721   755 D RILC    : RequestComplete, RIL_SOCKET_2
10-17 14:48:25.825582   721   755 E RILC    : Send Response to RIL_SOCKET_2
10-17 14:48:25.825656   721   755 D RILC-MTK: proxyLoop free  pRI=0x7f9784c9c0 p=0x7f97857490 
10-17 14:48:25.825692   721   755 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9360
10-17 14:48:25.825722   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:25.826123  1450  1609 D RILJ    : responseInts numInts=1 [SUB1]
10-17 14:48:25.826209  1450  1609 D RILJ    : responseInts response[0]=0 [SUB1]
10-17 14:48:25.826299  1450  1609 D RILJ    : [9615]< QUERY_NETWORK_SELECTION_MODE {0} [SUB1]
10-17 14:48:25.826645   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/9
10-17 14:48:25.826740   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.826805   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:19
10-17 14:48:25.826847   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 19 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.827027   721   766 I AT      : AT read end: 19
10-17 14:48:25.827068   721   766 D AT      : AT< +PSBEARER: 2, 2
10-17 14:48:25.827102   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+PSBEARER: 2, 2
10-17 14:48:25.827149   721   766 I AT      : AT read start
10-17 14:48:25.827252   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 19/19 bytes of frame to /dev/pts/3
10-17 14:48:25.827305   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.827364   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.827406   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.827641   721   766 I AT      : AT read end: 6
10-17 14:48:25.827683   721   766 D AT      : AT< OK
10-17 14:48:25.827714   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.827770   721   766 I AT      : AT read start
10-17 14:48:25.827858   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.827917   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.828100   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.828176   721   749 E RIL     : rid: 0
10-17 14:48:25.828205   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:48:25.828253   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:48:25.828282   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:48:25.828308   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:48:25.828341   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.828410   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.828505   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce10 p=0x7f978567e0 
10-17 14:48:25.828541   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9300
10-17 14:48:25.828530  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:25.828578   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.828609   721   749 D RILC-MTK: VOICE_REGISTRATION_STATE pRI=0x7f9784ce40 p=0x7f97856cb0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.828625  1450  1450 D TelephonyManager: getTelephonyProperty prop value= Tele2
10-17 14:48:25.828641   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.828670   721   749 D RIL     : onRequest: VOICE_REGISTRATION_STATE, datalen = 0
10-17 14:48:25.828694   721   749 D RIL     : radioState:10
10-17 14:48:25.828691  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName= Tele2 [SUB0]
10-17 14:48:25.828692  1450  1606 D RILJ    : [9609]< DATA_REGISTRATION_STATE {1, 1b5c, dff, 2, 0, 6} [SUB0]
10-17 14:48:25.828745   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.828746  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorLong use lookFromNetwork
10-17 14:48:25.828776   721   749 D AT      : AT> AT+CREG?
10-17 14:48:25.828802   721   749 I AT      : AT write start
10-17 14:48:25.829699   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.829769   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.829822   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.829909   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:25.833449  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:25.833544  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 
10-17 14:48:25.833622  1450  1450 D RILJ    : lookupOperatorNameFromNetwork numeric= 25020,subId= 1,nitzOperatorNumeric= 25020,nitzOperatorName=  [SUB0]
10-17 14:48:25.833669  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: OperatorShort use lookupOperatorNameFromNetwork
10-17 14:48:25.833706  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_OPERATOR: Tele2, 
10-17 14:48:25.833749  1450  1450 D GsmSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= 25020 ,update to: 25020
10-17 14:48:25.833792  1450  1450 D GsmSST  : [GsmSST0] opNames.length  ==3
10-17 14:48:25.833831  1450  1450 D GsmSST  : [GsmSST0] setmcc ==250
10-17 14:48:25.833949  1450  1450 D PhoneNumberUtils: setOpNamesMcc persist.sys.opmcc ==250
10-17 14:48:25.837704  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.838523   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:38
10-17 14:48:25.838617   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 38 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.838772   721   766 I AT      : AT read end: 38
10-17 14:48:25.838827   721   766 D AT      : AT< +CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:48:25.838859   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+CREG: 3,1,"1B5C","00000DFF",3,0,0
10-17 14:48:25.838900   721   766 I AT      : AT read start
10-17 14:48:25.838983   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 38/38 bytes of frame to /dev/pts/3
10-17 14:48:25.839038   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.839097   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.839140   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.839262   721   766 I AT      : AT read end: 6
10-17 14:48:25.839303   721   766 D AT      : AT< OK
10-17 14:48:25.839336   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.839394   721   766 I AT      : AT read start
10-17 14:48:25.839463   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.839532   721   749 D RIL     : convertRegState() uiRegState=1 , uiRet=1 
10-17 14:48:25.839565   721   749 E RIL     : The value in the field <lac> :127
10-17 14:48:25.839595   721   749 D RIL     : cid: 3583
10-17 14:48:25.839622   721   749 E RIL     : The value of act: 3
10-17 14:48:25.839647   721   749 D RIL     : cause_type: 0
10-17 14:48:25.839672   721   749 D RIL     : reject_cause: 0
10-17 14:48:25.839735   721   749 E RIL     : rid: 0
10-17 14:48:25.839765   721   749 D RIL     : RestrictedStateChanged: 0
10-17 14:48:25.839775  1450  1752 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.839800   721   749 D RIL     : isSimInserted(): rid: 0, sim_inserted_status: 1
10-17 14:48:25.839831   721   749 D RIL     : isSimInserted(): pivotSim = 1 ,1
10-17 14:48:25.839855  1450  1752 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.839859   721   749 D RIL     : isSimInserted(): simInserted = 1
10-17 14:48:25.839897   721   749 D RIL     : convertToRilRegState() uiRegState=1 , uiRet=1 
10-17 14:48:25.839933   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.839996   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.840083   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784ce40 p=0x7f97856cb0 
10-17 14:48:25.840118   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9340
10-17 14:48:25.840154   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:25.840191   721   749 D RILC-MTK: QUERY_NETWORK_SELECTION_MODE pRI=0x7f9784cea0 p=0x7f978570a0 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:25.840220   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:25.840248   721   749 D RIL     : onRequest: QUERY_NETWORK_SELECTION_MODE, datalen = 0
10-17 14:48:25.840273   721   749 D RIL     : radioState:10
10-17 14:48:25.840314   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.840348   721   749 D AT      : AT> AT+COPS?
10-17 14:48:25.840342  1450  1606 D RILJ    : [9610]< VOICE_REGISTRATION_STATE {1, 1b5c, dff, 2, , , , , , , , , , 0} [SUB0]
10-17 14:48:25.840380   721   749 I AT      : AT write start
10-17 14:48:25.840422   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.840550   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:25.840591   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:25.840654   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:25.840746   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 9
10-17 14:48:25.840485   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.841765  1450 20008 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:25.841948  1450 20008 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:25.842822   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:24
10-17 14:48:25.844460   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 24 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.844672   721   766 I AT      : AT read end: 24
10-17 14:48:25.844726   721   766 D AT      : AT< +COPS: 0,2,"25020",3
10-17 14:48:25.844758   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:+COPS: 0,2,"25020",3
10-17 14:48:25.844800   721   766 I AT      : AT read start
10-17 14:48:25.844886   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 24/24 bytes of frame to /dev/pts/3
10-17 14:48:25.844942   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.845005   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:25.845045   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:25.845167   721   766 I AT      : AT read end: 6
10-17 14:48:25.845207   721   766 D AT      : AT< OK
10-17 14:48:25.845237   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:25.845285   721   766 I AT      : AT read start
10-17 14:48:25.845349   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:25.845367   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:25.845407   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:25.845420   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:25.845457   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:25.845540   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cea0 p=0x7f978570a0 
10-17 14:48:25.845574   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9b80
10-17 14:48:25.845601   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:25.845702  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.845818  1450  1606 D RILJ    : responseInts numInts=1 [SUB0]
10-17 14:48:25.845832  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_GPRS
10-17 14:48:25.845877  1450  1606 D RILJ    : responseInts response[0]=0 [SUB0]
10-17 14:48:25.845878  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:25.845913  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:25.845956  1450  1606 D RILJ    : [9611]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
10-17 14:48:25.845967  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:48:25.846002  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:25.846030  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:25.846078  1450  1450 D GsmSST  : [GsmSST1] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:48:25.846110  1450  1450 E GsmSST  : [GsmSST1] handlePollStateResult return due to (ar.userObj != mPollingContext)
10-17 14:48:25.846142  1450  1450 D GsmSST  : [GsmSST1] handleMessage msg done
10-17 14:48:25.846196  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_GPRS
10-17 14:48:25.846248  1450  1450 D GsmSST  : [GsmSST0] <mNewMaxDataCalls> 6
10-17 14:48:25.846294  1450  1450 D PHONE   : [ServiceState] setDataRegState=0
10-17 14:48:25.846381  1450  1450 D PHONE   : [ServiceState] setProprietaryDataRadioTechnology=0
10-17 14:48:25.846418  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:48:25.846464  1450  1450 D GsmSST  : [GsmSST0] handlPollStateResultMessage: GsmSST setDataRegState=0 regState=1 dataRadioTechnology=2
10-17 14:48:25.846496  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.846560  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_REGISTRATION
10-17 14:48:25.846620  1450  1450 D GsmSST  : [GsmSST0] set voice reject cause to 0
10-17 14:48:25.846686  1450  1450 D GsmSST  : [GsmSST0] EVENT_POLL_STATE_REGISTRATION mSS getRilVoiceRadioTechnology:2, regState:1, NewSS RilVoiceRadioTechnology:2, lac:7004, cid:3583
10-17 14:48:25.846784  1450  1450 D PHONE   : [ServiceState] setVoiceRegState=0
10-17 14:48:25.846815  1450  1450 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
10-17 14:48:25.846973  1450  1450 D GsmSST  : [GsmSST0] regState = 1isVoiceCapable = truemEmergencyOnly = false
10-17 14:48:25.847182  1450  1450 D GsmSST  : [GsmSST0] states.length > 3
10-17 14:48:25.847222  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.847294  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_POLL_STATE_NETWORK_SELECTION_MODE
10-17 14:48:25.847358  1450  1450 D GsmSST  : [GsmSST0] set raoming=false,mGsmRoaming= false,mDataRoaming= false
10-17 14:48:25.850527  1450  1450 D GsmSST  : [GsmSST0] mLastCsNetworkType=2, mLastPsNetworkType= 2, mNewSS VoiceRadioTechnology= 2, mSS VoiceRadioTechnology= 2, mNewSS DataRadioTechnology= 2, mSS DataRadioTechnology= 2
10-17 14:48:25.850608  1450  1450 D GsmSST  : [GsmSST0] pollStateDone(): don't change network type and wait for new event
10-17 14:48:25.850650  1450  1450 D PHONE   : [ServiceState] setDataRadioTechnology=2
10-17 14:48:25.850801  1450  1450 D GsmSST  : [GsmSST0] Poll ServiceState done:  oldSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] newSS=[0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false] oldMaxDataCalls=6 mNewMaxDataCalls=6 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
10-17 14:48:25.853064  1450  1450 D GsmSST  : [GsmSST0] pollStateDone,hasRegistered:false,hasDeregistered:false,hasGprsAttached:false,hasRilVoiceRadioTechnologyChanged:false,hasRilDataRadioTechnologyChanged:false,hasVoiceRegStateChanged:false,hasDataRegStateChanged:false,hasChanged:true,hasVoiceRoamingOn:false,hasVoiceRoamingOff:false,hasDataRoamingOn:false,hasDataRoamingOff:false,hasLocationChanged:false,hasLacChanged:false,sReceiveNitz:true
10-17 14:48:25.853366  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:48:25.853458  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:48:25.853521  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule USIM mEfSST is 06fa173c233e040040010000 set bSpnActive to true (slot 0)
10-17 14:48:25.853581  1450  1450 D SIMRecords: [SIMRecords] getDisplayRule mParentApp is com.android.internal.telephony.uicc.UiccCardApplication@ed7b064 (slot 0)
10-17 14:48:25.853765  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride (slot 0)
10-17 14:48:25.853831  1450  1450 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=Tele2 (slot 0)
10-17 14:48:25.853895  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: plmn is 25020 nLac is 7004 bLongNameRequired: true (slot 0)
10-17 14:48:25.853972  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 0 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854025  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 1 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854071  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 2 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854116  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 3 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854165  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 4 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854208  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 5 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854250  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 6 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854291  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 7 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854333  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 8 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854383  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: record number is 9 sPlmn:  nMinLAC: 65535 nMaxLAC: 65535 PnnIndex 255 (slot 0)
10-17 14:48:25.854422  1450  1450 D SIMRecords: [SIMRecords] EONS getEonsIfExist: sEons is null (slot 0)
10-17 14:48:25.854459  1450  1450 D GsmSST  : [GsmSST0] Home PLMN, get CPHS ons
10-17 14:48:25.854490  1450  1450 D GsmSST  : [GsmSST0] No matched EONS and No CPHS ONS
10-17 14:48:25.854554  1450  1450 D GsmSST  : [GsmSST0] updateSpnDisplay mVoiceCapable=true mEmergencyOnly=false mCi.getRadioState().isOn()=true getVoiceRegState()=0 getDataRegState()0
10-17 14:48:25.856076  1450  1450 D GsmSST  : [GsmSST0] updateAllOpertorInfo with spn:Tele2
10-17 14:48:25.856743  1450  1450 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:25.856903  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 25020 propVal=25020
10-17 14:48:25.857602  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: ru propVal=ru
10-17 14:48:25.858484  1450  1450 D GsmSST  : [GsmSST0] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=25020 mcc=250 prevOperatorNumeric=25020 prevMcc=250 needToFixTimeZone=false ltod=10-17 14:48:25.858
10-17 14:48:25.858689  1450  1450 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false,false
10-17 14:48:25.859443  1450  1450 D GsmSST  : [GsmSST0] Broadcasting ServiceState : 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.859617  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.859722  1450  1450 D PhoneBase: networkType=EDGE
10-17 14:48:25.859789  1450  1450 D PhoneBase: isVideoEnabled: false
10-17 14:48:25.859857  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.860119  1450  1450 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad} phondId=0 subId=1
10-17 14:48:25.860976   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.861137   909  7315 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:25.861336   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: logSSC.length=5 next=0
10-17 14:48:25.861756   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.862207   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.862674   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144625Europe/Samara(1,290,14400,0,1476701185) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.863149   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144817Europe/Samara(1,290,14400,0,1476701297) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.863625   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144825Europe/Samara(1,290,14400,0,1476701305) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.863741   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: ----------------
10-17 14:48:25.863803   909  7315 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:25.863966   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.864095   909  7315 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:25.864270   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.phone binder=android.os.BinderProxy@6f8f485 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@65ed2da onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.864534   909  7315 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:25.864740   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.865330   909  7315 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:25.865998   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=android binder=android.telephony.PhoneStateListener$1@6b38be3 callback=android.telephony.PhoneStateListener$1@6b38be3 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.866171   909  7315 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:25.866368   909  7315 D TelephonyRegistry: notifyServiceStateForSubscriber: callback.onSSC r={callingPackage=com.google.android.googlequicksearchbox binder=android.os.BinderProxy@6ce9e1b callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@e07bbb8 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=0 events=1 canReadPhoneState=false} subId=1 phoneId=0 state=0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:25.866590   909  7315 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:25.868237  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:25.868427  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:25.868496  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:25.868533  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:25.868575  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:48:25.868621  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:25.871783  1450  1515 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.874270  1450 21807 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:25.874394  1450 21807 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:25.875310  1450  2351 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:25.875489  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:25.876617  1450  1450 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:25.877204   909  7315 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:25.883472  1450  1450 D GsmSST  : [GsmSST0] old:0 ,mPsRegState:0,new:0
10-17 14:48:25.883582  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:25.883713  1450  1450 D CallManager:  handleMessage (EVENT_SERVICE_STATE_CHANGED)
10-17 14:48:25.886288  1450  1450 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:25.900356   909   924 D TelephonyManager: getTelephonyProperty prop value= ru
10-17 14:48:25.906298  1450  1515 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:48:25.907505  1450  1515 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:48:25.913041  1450  1807 D SubscriptionController: [getActiveSubInfoList]+
10-17 14:48:25.914198  1450  1807 D SubscriptionController: [getActiveSubInfoList]- 1 infos return
10-17 14:48:25.981663  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:25.984272  1450 23534 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:25.985038  1450 23534 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.013784  1450 29539 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:26.014675  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:26.024520  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.036569  1450  4234 D DCT     : [0]phoneSubId = 1
10-17 14:48:26.037961  1450  4234 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:26.171544  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.174628  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.175009  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.184442  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.186284  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.186689  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.192752  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.195711  1450  1807 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.205524  1450  1807 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.212000  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.213540  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.214103  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.225623  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.227733  1450  1634 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.228315  1450  1634 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.237110  1450  1807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:26.237865  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:26.243719  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.250050  1450  1683 D DCT     : [0]phoneSubId = 1
10-17 14:48:26.250406  1450  1683 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:26.255672  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.256972  1450  1511 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.257765  1450  1511 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.270052  1450 21807 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:26.270586  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:26.275014  1450  2351 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.283446  1450 23534 D DCT     : [0]phoneSubId = 1
10-17 14:48:26.283690  1450 23534 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:26.297336  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:48:26.299466  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:26.299584  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:48:26.302784   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.303313   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.305797  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:26.306662  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:48:26.306909  1450  1511 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.307027  1450  1511 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.310139   909   920 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.311253   909   920 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.314491  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:26.314789  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:48:26.315497  1450  1450 D RILJ    : [9616]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:48:26.318856   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:48:26.318949   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94cda900, pRI=0x7f9784cbd0, p=0x7f97856690, pUCI=0x0
10-17 14:48:26.319035   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cbd0 p=0x7f97856690 dispatched to RIL_CMD_PROXY_3
10-17 14:48:26.319150   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:26.319147   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:26.319204   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:26.319205   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:26.319238   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:26.319286   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:26.319305   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:26.319312   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:26.319357   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:26.319360   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:26.319387   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:26.319431   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:26.319460   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:26.319471   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:26.319492   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784cbd0 p=0x7f97856690 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:26.319514   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:26.319522   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:26.319555   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:48:26.319567   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:26.319581   721   749 D RIL     : radioState:10
10-17 14:48:26.319593   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:26.319624   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:48:26.319629   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:26.319659   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,0
10-17 14:48:26.319690   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:26.319716   721   749 D AT      : AT> AT+EFD=3,0
10-17 14:48:26.319740   721   749 I AT      : AT write start
10-17 14:48:26.320150   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:26.320256   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:26.320319   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:26.320359   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:26.320410   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:26.320427   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:26.320463   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:26.320494   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:26.320538   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:26.320567   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:26.321597  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_OFF
10-17 14:48:26.323865  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:26.323955  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:48:26.324152  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.324238  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.324840   909  1631 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.324993   909  1631 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.325289   909  1631 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.326650  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:26.326816  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:48:26.326974  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.327047  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.327704   909   919 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.327883   909   919 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.328755   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:26.328834   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:26.328915   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:26.328972   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:26.329050   909   919 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.331012   721   766 I AT      : AT read end: 6
10-17 14:48:26.331068   721   766 D AT      : AT< OK
10-17 14:48:26.331101   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:26.331155   721   766 I AT      : AT read start
10-17 14:48:26.331256   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:26.331294   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:26.331344   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:26.331428   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784cbd0 p=0x7f97856690 
10-17 14:48:26.331481   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94cda900
10-17 14:48:26.331512   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:26.332744  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:48:26.332881  1450  1606 D RILJ    : [9616]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:48:26.335125  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_OFF
10-17 14:48:26.335266  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_OFF
10-17 14:48:26.345347  1450  1752 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.345642  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.348327  1450  4234 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.348491  1450  4234 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.349197  1450  1450 D CAT     : StkAppService: StkAppService onStart sim id: 0, op: 24, Bundle[{op=24}]
10-17 14:48:26.349341  1450  1450 D CAT     : StkAppService: StkAppService onStart mPhone: Handler (com.android.internal.telephony.PhoneProxy) {be7672}, mPhoneStateChangeReg: true
10-17 14:48:26.350635  1450  2326 D CAT     : StkAppInstaller: Init thread
10-17 14:48:26.350741  1450  2326 D CAT     : StkAppService: handleMessage opcode[24], sim id[0]
10-17 14:48:26.350799  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:48:26.350834  1450  2326 D CAT     : StkAppService: Need to send IDLE SCREEN Available event to SIM
10-17 14:48:26.351654  1450  1634 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.351865  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:26.353845  1450 29539 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.354175  1450 29539 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.368714  1450  1515 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.368837  1450  1515 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.382428  1450  1752 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:26.383153  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:26.385723  1450  1511 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.388013  1450 29539 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.388227  1450 29539 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.389202  1450 21807 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.389382  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 3 getDataRegState() : 3
10-17 14:48:26.389675  1450  1634 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.394772  1450  1807 D DCT     : [0]phoneSubId = 1
10-17 14:48:26.396179  1450  1807 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:26.403029  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:26.404477  1450  1752 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:26.404888  1450  1752 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:26.412991  1450  1511 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:26.413508  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:26.418280  1450 21807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:26.422822  1450  1515 D DCT     : [0]phoneSubId = 1
10-17 14:48:26.423410  1450  1515 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:26.665126  1450  1450 D GsmSST  : [GsmSST0] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:48:26.666538  1450  1450 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:26.666625  1450  1450 D DCT     : [0]stopNetStatPoll
10-17 14:48:26.667925   909  1553 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.668210   909  1553 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.669209  1450  1450 D DCT     : [0]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={[[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , ]} mWaitingApnsPermanentFailureCountDown=1 mApnSetting={[ApnSettingV3] TELE2 Internet, 386, 25020, internet.tele2.ru, , , , , , -1, default | supl, IP, IP, true, 0, 0, 0, false, 0, 0, 0, 0, , } mReason=dataDisabled mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:26.669329  1450  1450 D DCT     : [0]overall state is IDLE
10-17 14:48:26.670446   909   923 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.670711   909   923 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.672429  1450  1450 D FdManager: [GDCT][phoneId0]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:26.672572  1450  1450 D FdManager: [GDCT][phoneId0]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:48:26.672764  1450  1450 D RILJ    : [9617]> RIL_REQUEST_SET_FD_MODE [SUB0]
10-17 14:48:26.675225   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: RIL_REQUEST_SET_FD_MODE length:20
10-17 14:48:26.675334   721   760 I RILC-MTK: create request 2061: pRequest=0x7f94ce6aa0, pRI=0x7f9784c7b0, p=0x7f97857500, pUCI=0x0
10-17 14:48:26.675405   721   760 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c7b0 p=0x7f97857500 dispatched to RIL_CMD_PROXY_3
10-17 14:48:26.675518   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:26.675563   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:26.675814   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:26.675850   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:26.675893   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:26.675917   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:26.675954   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:26.675977   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:26.676019   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:26.676051   721   749 D RILC-MTK: proxy id:1, proxyName: RIL_CMD_PROXY_3
10-17 14:48:26.676084   721   749 D RILC-MTK: RIL_REQUEST_SET_FD_MODE pRI=0x7f9784c7b0 p=0x7f97857500 execute on RIL_CMD_PROXY_3 using channel 1
10-17 14:48:26.676115   721   749 D RILC    : callOnRequest for new vendor ril
10-17 14:48:26.676145   721   749 D RIL     : onRequest: RIL_REQUEST_SET_FD_MODE, datalen = 16
10-17 14:48:26.676172   721   749 D RIL     : radioState:10
10-17 14:48:26.676223   721   749 D RIL     : requestSetFDMode:args_num=2
10-17 14:48:26.676263   721   749 D RIL     : requestSetFDMode:cmd=AT+EFD=3,1
10-17 14:48:26.676300   721   749 D AT      : AT send on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:26.676313   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:26.676332   721   749 D AT      : AT> AT+EFD=3,1
10-17 14:48:26.676364   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:26.676365   721   749 I AT      : AT write start
10-17 14:48:26.676426   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:26.676436   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:26.676459   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:26.676506   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:26.676510   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:26.676536   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:26.676554   537   709 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:26.676612   537   709 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:26.676666   537   709 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 3
10-17 14:48:26.676755   537   709 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 3 with length 11
10-17 14:48:26.676961  1450  1450 D GsmSST  : [GsmSST1] BroadcastReceiver: android.intent.action.SCREEN_ON
10-17 14:48:26.676963   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:26.677024   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:26.677069   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:26.679318   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:26.679394   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:26.679452   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:26.683373  1450  1450 D DCT     : [1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:26.683522  1450  1450 D DCT     : [1]stopNetStatPoll
10-17 14:48:26.683941  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.684182  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.684667   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:3, ctrl:239, len:6
10-17 14:48:26.684752   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 3 to /dev/pts/3
10-17 14:48:26.684839   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/3
10-17 14:48:26.684899   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:26.685050   721   766 I AT      : AT read end: 6
10-17 14:48:26.685103   721   766 D AT      : AT< OK
10-17 14:48:26.685135   721   766 D AT      : RIL_CMD_READER_1 Enter processLine:OK
10-17 14:48:26.685178   721   766 I AT      : AT read start
10-17 14:48:26.685232   721   749 D AT      : response received on RIL_CMD_READER_1, tid:547986625600
10-17 14:48:26.685280   721   749 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:26.685327   721   749 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:26.685415   721   749 D RILC-MTK: proxyLoop free  pRI=0x7f9784c7b0 p=0x7f97857500 
10-17 14:48:26.685454   721   749 D RILC-MTK: proxyLoop free  pRequest=0x7f94ce6aa0
10-17 14:48:26.685482   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:26.685629   909   920 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.685760   909   920 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.686188   909   920 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.687047  1450  1606 D RILJ    : responseInts numInts=0 [SUB0]
10-17 14:48:26.687333  1450  1606 D RILJ    : [9617]< RIL_REQUEST_SET_FD_MODE {} [SUB0]
10-17 14:48:26.687827  1450  1450 D DCT     : [1]overall state is {mApnType=xcap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cmmail mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=rcs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=fota mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=wap mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dm mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=emergency mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ims mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=cbs mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=ia mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, {mApnType=net mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}, 
10-17 14:48:26.688173  1450  1450 D DCT     : [1]overall state is IDLE
10-17 14:48:26.688432  1450  1450 D SubscriptionController: [getSubId]- numSubIds == 0, return DummySubIds slotIdx=1
10-17 14:48:26.688560  1450  1450 D SubscriptionController: getDummySubIds: slotIdx=1 return 2 DummySubIds with each subId=-3
10-17 14:48:26.689301   909  1551 D SubscriptionManager: [getPhoneId]- return dummy value, subId = -3
10-17 14:48:26.689383   909  1551 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:26.689869   909  1551 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:26.693619  1450  1450 D FdManager: [GDCT][phoneId1]onReceive: action=android.intent.action.SCREEN_ON
10-17 14:48:26.693886  1450  1450 D FdManager: [GDCT][phoneId1]fdMdEnableMode=1, 3gSimID=0, when switching to SCREEN_ON
10-17 14:48:26.764766   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43900 
10-17 14:48:26.764854   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e433c0
10-17 14:48:26.764885   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e433d0
10-17 14:48:26.765235   721   760 D RILC    : s_last_wake_timeout_info: 0x7f94e43900 reset to NULL
10-17 14:48:26.765282   721   760 D RILC    : userTimerCallback free  p_info: 0x7f94e43900
10-17 14:48:26.765309   721   760 D RILC    : userTimerCallback free  p_info->event: 0x7f94e43910
10-17 14:48:27.459495   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185371/0
10-17 14:48:28.309239  1450  1450 D RILJ    : [9618]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:28.317363   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:28.317459   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9120, pRI=0x7f9784c810, p=0x7f97857570, pUCI=0x0
10-17 14:48:28.317498   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f97857570 dispatched to RIL_ATCI_PROXY
10-17 14:48:28.317613   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:28.317666   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:28.317678   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:28.317726   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:28.317734   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:28.317739   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:28.317753   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:28.317790   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:28.317799   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:28.317817   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:28.317844   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:28.317884   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:28.317988   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:28.318030   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:28.318083   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:28.318119   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:28.318159   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:28.318166   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:28.318196   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:28.318205   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c810 p=0x7f97857570 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:28.318242   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:28.318238   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:28.318271   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:28.318279   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:28.318310   721   753 D RIL     : radioState:10
10-17 14:48:28.318368   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:28.318404   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:28.318437   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:28.318462   721   753 I AT      : AT write start
10-17 14:48:28.318700   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:28.318796   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:28.318864   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:28.318980   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:28.319495   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:28.319581   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:28.319773   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:28.326789   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:28.326910   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:28.327002   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:28.327052   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:28.327223   721   770 I AT      : AT read end: 6
10-17 14:48:28.327297   721   770 D AT      : AT< OK
10-17 14:48:28.327334   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:28.327388   721   770 I AT      : AT read start
10-17 14:48:28.327447   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:28.327495   721   753 D RIL     : p_response->success = 1
10-17 14:48:28.327526   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:28.327553   721   753 D RIL     : strLength = 6
10-17 14:48:28.327579   721   753 D RIL     : line = <
10-17 14:48:28.327579   721   753 D RIL     : OK
10-17 14:48:28.327579   721   753 D RIL     : >
10-17 14:48:28.327612   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:28.327676   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:28.327771   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c810 p=0x7f97857570 
10-17 14:48:28.327811   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9120
10-17 14:48:28.327837   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:28.330060  1450  1606 D RILJ    : [9618]< OEM_HOOK_RAW [B@42dfd0a [SUB0]
10-17 14:48:29.470660  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:29.827988  1020  1595 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:29.829467  1450  1683 D SubscriptionController: [getActiveSubIdList] simInfoSet=[0=1]
10-17 14:48:29.831557  1450  1683 D SubscriptionController: [getActiveSubIdList] X subIdArr.length=1
10-17 14:48:29.866159  1450  1450 D RILJ    : [9619]> OEM_HOOK_RAW[41542b45524654583d34] [SUB0]
10-17 14:48:29.878605   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:24
10-17 14:48:29.878723   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cf9300, pRI=0x7f9784c840, p=0x7f97857730, pUCI=0x0
10-17 14:48:29.878762   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c840 p=0x7f97857730 dispatched to RIL_ATCI_PROXY
10-17 14:48:29.878886   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:29.878886   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:29.878942   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:29.879001   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:29.878997   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:29.879038   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:29.879050   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:29.879082   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:29.879119   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:29.879137   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:29.879150   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:29.879208   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:29.879210   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:29.879211   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:29.879244   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:29.879250   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:29.879288   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c840 p=0x7f97857730 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:29.879323   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:29.879358   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 10
10-17 14:48:29.879388   721   753 D RIL     : radioState:10
10-17 14:48:29.879443   721   753 D RIL     : data = AT+ERFTX=4, length = 10
10-17 14:48:29.879477   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:29.879557   721   753 D AT      : AT> AT+ERFTX=4
10-17 14:48:29.879583   721   753 I AT      : AT write start
10-17 14:48:29.879782   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:29.879849   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:29.879881   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:29.879902   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:29.879954   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:29.879988   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:29.880006   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 11
10-17 14:48:29.880028   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:29.880824   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:29.880977   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:29.881049   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:29.881077   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:29.887649   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:29.890207   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:29.890299   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:29.890349   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:29.891433   721   770 I AT      : AT read end: 6
10-17 14:48:29.891502   721   770 D AT      : AT< OK
10-17 14:48:29.891533   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:29.891599   721   770 I AT      : AT read start
10-17 14:48:29.891651   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:29.891691   721   753 D RIL     : p_response->success = 1
10-17 14:48:29.891719   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:29.891743   721   753 D RIL     : strLength = 6
10-17 14:48:29.891769   721   753 D RIL     : line = <
10-17 14:48:29.891769   721   753 D RIL     : OK
10-17 14:48:29.891769   721   753 D RIL     : >
10-17 14:48:29.891804   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:29.891878   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:29.891965   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c840 p=0x7f97857730 
10-17 14:48:29.891997   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf9300
10-17 14:48:29.892027   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:29.893533  1450  1606 D RILJ    : [9619]< OEM_HOOK_RAW [B@a69f97b [SUB0]
10-17 14:48:30.092748  1431 27957 D TelephonyManager: getTelephonyProperty prop value= 25020
10-17 14:48:30.135221  1450  1515 D SubscriptionController: getSimStateForSlotIdx:  simState=READY ordinal=5
10-17 14:48:30.142204  1020  1595 D SubscriptionManager: getSimStateForSubscriber: simState=5 slotIdx=0
10-17 14:48:30.188790  1450  1807 D GSMPhone: [GSMPhone] getServiceState : getState() : 0 getDataRegState() : 0
10-17 14:48:30.205540  1450  1752 D DCT     : [0]phoneSubId = 1
10-17 14:48:30.205727  1450  1752 D DCT     : [0]getDataEnabled: getInt retVal=false
10-17 14:48:30.448994   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:2, ctrl:239, len:37
10-17 14:48:30.449101   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 37 byte frame received on channel 2 to /dev/pts/2
10-17 14:48:30.449189   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 37/37 bytes of frame to /dev/pts/2
10-17 14:48:30.449236   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:30.449371   721   765 I AT      : AT read end: 37
10-17 14:48:30.449426   721   765 D AT      : AT< +ECSQ: 41,99,-279,1,1,1,1,3,32767
10-17 14:48:30.449458   721   765 D AT      : RIL_URC_READER Enter processLine:+ECSQ: 41,99,-279,1,1,1,1,3,32767
10-17 14:48:30.449503   721   765 D RIL     : Nw URC:+ECSQ: 41,99,-279,1,1,1,1,3,32767
10-17 14:48:30.449574   721   765 D RILC    : callForRilVersion new vendor RIL, version: 10
10-17 14:48:30.449626   721   765 I RILC    : RIL_SOCKET_1 UNSOLICITED: UNSOL_SIGNAL_STRENGTH length:72
10-17 14:48:30.449652   721   765 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:30.449711   721   765 I AT      : AT read start
10-17 14:48:30.450115  1450  1450 D GsmSST  : [GsmSST0] handle EVENT_SIGNAL_STRENGTH_UPDATE
10-17 14:48:30.450337  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():  LastSignalStrength=SignalStrength: 22 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -273 1 1
10-17 14:48:30.450456  1450  1450 D GsmSST  : [GsmSST0] onSignalStrengthResult():new mSignalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -279 1 1
10-17 14:48:30.450688  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.450873  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.451050  1450  1450 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.451118  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.451177  1450  1450 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.451204  1450  1450 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.451252  1450  1450 D GsmSST  : [GsmSST0] notifySignalStrength: mSignalStrength.getLevel=4
10-17 14:48:30.451563  1450  1450 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@4b87ab3 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -279 1 1 sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {c76a4ad}
10-17 14:48:30.452236   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: subId=1 signalStrength=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -279 1 1
10-17 14:48:30.452336   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: logSSC.length=5 next=0
10-17 14:48:30.452830   909  1551 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144343Europe/Samara(1,290,14400,0,1476701023) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:30.453271   909  1551 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144618Europe/Samara(1,290,14400,0,1476701178) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:30.453684   909  1551 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144625Europe/Samara(1,290,14400,0,1476701185) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:30.454109   909  1551 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144817Europe/Samara(1,290,14400,0,1476701297) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported 0 0 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:30.454803   909  1551 D TelephonyRegistry: notifyServiceStateForSubscriber Time 20161017T144825Europe/Samara(1,290,14400,0,1476701305) mSubId 1 mPhoneId 0  mState 0 0 voice home data home Tele2  25020 Tele2  25020  EDGE EDGE CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false Ril Voice Regist state: 1 Ril Data Regist state: 1 mProprietaryDataRadioTechnology: 0 VoiceRejectCause: 0 DataRejectCause: -1 mCdmaNetWorkMode: 0 IsDataRoamingFromRegistration=false
10-17 14:48:30.454894   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: ----------------
10-17 14:48:30.457301   909  1551 D TelephonyRegistry: validatePhoneId: true
10-17 14:48:30.457387   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: valid phoneId=0
10-17 14:48:30.457452   909  1551 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:30.457786   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=android binder=android.telephony.PhoneStateListener$1@417f33f callback=android.telephony.PhoneStateListener$1@417f33f onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=2147483647 phoneId=-1 events=1c1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -279 1 1
10-17 14:48:30.457967   909  1551 D TelephonyRegistry: idMatch: rlt=true
10-17 14:48:30.458176   909  1551 D TelephonyRegistry: notifySignalStrengthForSubscriber: callback.onSsS r={callingPackage=com.android.systemui binder=android.os.BinderProxy@a6742a6 callback=com.android.internal.telephony.IPhoneStateListener$Stub$Proxy@6aa24e7 onSubscriptionsChangedListenererCallback=null callerUserId=0 subId=1 phoneId=0 events=111e1 canReadPhoneState=true} subId=1 phoneId=0 ss=SignalStrength: 21 99 -120 -160 -3 0 -1 99 2147483647 0 2147483647 2147483647 2147483647 gsm|lte -279 1 1
10-17 14:48:30.458539   909  1551 D TelephonyRegistry: handleRemoveListLocked: mRemoveList.size()=0
10-17 14:48:30.459198   909  1551 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.459473  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.459478   909  1551 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.459571   909  1551 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.459629   909  1551 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.459663  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.459683   909  1551 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.459716   909  1551 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.459721  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.459766  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.459817  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.459857  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.466918  1450  1450 D GsmSST  : [GsmSST0] handleMessage msg done
10-17 14:48:30.468662  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.468855  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:48:30.469073  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.469264  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.469349  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.469393  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.469442  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=22
10-17 14:48:30.469473  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.472466  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.472762  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.472871  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.472927  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.472989  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.473028  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.473073  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.473124  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.473839  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.473972  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rsrp:2147483647 snr:2147483647 rsrpIconLevel:-1 snrIconLevel:-1
10-17 14:48:30.474049  1020  1390 I use-Rlog/RLOG-GSM: getLTELevel - rssi:99 rssiIconLevel:0
10-17 14:48:30.474094  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.474151  1020  1390 D use-Rlog/RLOG-GSM: mapGsmSignalDbm() gsmRscpQdbm=1 asu=21
10-17 14:48:30.474180  1020  1390 W SignalStrength: SignalStrength get plugin
10-17 14:48:30.749915   721   760 I RILC    : NUMBER:1
10-17 14:48:30.749968   721   760 I RILC    : arg len:14
10-17 14:48:30.750002   721   760 I RILC    : ARGS[0]:THERMAL,0,-1
10-17 14:48:30.750113   721   760 D RILC    : C[locl]> QUERY_MODEM_THERMAL
10-17 14:48:30.750189   721   760 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784ca50 p=0x7f97856540 dispatched to RIL_CMD_PROXY_1
10-17 14:48:30.750317   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:30.750307   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:30.750310   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:30.750351   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:30.750358   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:30.750399   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:30.750405   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:30.750460   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:30.750516   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:30.750533   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:30.750550   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:30.750603   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:30.750629   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:30.751171   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:30.751220   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:30.751286   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:30.751319   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:30.751377   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:30.751376   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:30.751414   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:30.751462   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:30.751487   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:30.751576   721   751 D RILC-MTK: proxy id:3, proxyName: RIL_CMD_PROXY_1
10-17 14:48:30.751615   721   751 D RILC-MTK: QUERY_MODEM_THERMAL pRI=0x7f9784ca50 p=0x7f97856540 execute on RIL_CMD_PROXY_1 using channel 3
10-17 14:48:30.751653   721   751 D RILC    : callOnRequest for new vendor ril
10-17 14:48:30.751682   721   751 D RIL     : onRequest: QUERY_MODEM_THERMAL, datalen = 8
10-17 14:48:30.751707   721   751 D RIL     : radioState:10
10-17 14:48:30.751745   721   751 D RIL     : requestQueryThermal Enter,-1
10-17 14:48:30.751787   721   751 D AT      : getRILChannelCtx subsystem:1, rid:0 channelOffset:0
10-17 14:48:30.751842   721   751 D AT      : AT send on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:30.751849   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:30.751870   721   751 D AT      : AT> AT+ETHERMAL
10-17 14:48:30.751893   721   751 I AT      : AT write start
10-17 14:48:30.752068   537   712 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:30.752136   537   712 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:30.752190   537   712 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 5
10-17 14:48:30.752282   537   712 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 5 with length 12
10-17 14:48:30.759934   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:40
10-17 14:48:30.760044   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 40 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:30.760131   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 40/40 bytes of frame to /dev/pts/5
10-17 14:48:30.760177   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:30.760233   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:5, ctrl:239, len:6
10-17 14:48:30.760275   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 5 to /dev/pts/5
10-17 14:48:30.760323   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/5
10-17 14:48:30.760362   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:30.760478   721   768 I AT      : AT read end: 46
10-17 14:48:30.760521   721   768 D AT      : AT< +ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:30.760552   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:+ETHERMAL: 1, 32767,,, -1, 32767, 18
10-17 14:48:30.760585   721   768 D AT      : AT< OK
10-17 14:48:30.760610   721   768 D AT      : RIL_CMD_READER_3 Enter processLine:OK
10-17 14:48:30.760654   721   768 I AT      : AT read start
10-17 14:48:30.760770   721   751 D AT      : response received on RIL_CMD_READER_3, tid:547984544832
10-17 14:48:30.760812   721   751 D RIL     : requestQueryThermal success
10-17 14:48:30.760847   721   751 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:30.760879   721   751 D RILC    : [THERMAL] local request for THERMAL returned 
10-17 14:48:30.761178   721   751 D RILC    : [THERMAL] s_THERMAL_fd is valid strResult is  1, 32767,,, -1, 32767, 18
10-17 14:48:30.761260   721   751 D RILC-MTK: proxyLoop free  pRI=0x7f9784ca50 p=0x7f97856540 
10-17 14:48:30.761301   721   751 D RILC-MTK: proxyLoop free  pRequest=0x7f94cf93a0
10-17 14:48:30.761330   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:32.459744   537   537 D RILMUXD : [gsm0710muxd] 3897:main(): Frames received/dropped: 185376/0
10-17 14:48:32.900099  1450  1450 D RILJ    : [9620]> OEM_HOOK_RAW[41542b45524654583d312c34382c36342c3634] [SUB0]
10-17 14:48:32.902857   721   760 D RILC    : SOCKET RIL_SOCKET_1 REQUEST: OEM_HOOK_RAW length:32
10-17 14:48:32.902952   721   760 I RILC-MTK: create request 59: pRequest=0x7f94cdaac0, pRI=0x7f9784c360, p=0x7f97856fc0, pUCI=0x0
10-17 14:48:32.902992   721   760 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856fc0 dispatched to RIL_ATCI_PROXY
10-17 14:48:32.903098   721   752 I RILC-MTK: RIL_CMD_PROXY_4 wakeup
10-17 14:48:32.903090   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 wakeup
10-17 14:48:32.903096   721   750 I RILC-MTK: RIL_CMD_PROXY_2 wakeup
10-17 14:48:32.903147   721   752 I RILC-MTK: RIL_CMD_PROXY_4 sleep
10-17 14:48:32.903177   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 wakeup
10-17 14:48:32.903199   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 wakeup
10-17 14:48:32.903204   721   754 I RILC-MTK: RIL_URC2_PROXY wakeup
10-17 14:48:32.903213   721   756 I RILC-MTK: RIL_CMD2_PROXY_2 sleep
10-17 14:48:32.903210   721   749 I RILC-MTK: RIL_CMD_PROXY_3 wakeup
10-17 14:48:32.903247   721   749 I RILC-MTK: RIL_CMD_PROXY_3 sleep
10-17 14:48:32.903295   721   753 I RILC-MTK: RIL_ATCI_PROXY wakeup
10-17 14:48:32.903304   721   750 I RILC-MTK: RIL_CMD_PROXY_2 sleep
10-17 14:48:32.903360   721   748 I RILC-MTK: RIL_URC_PROXY wakeup
10-17 14:48:32.903377   721   758 I RILC-MTK: RIL_CMD2_PROXY_4 sleep
10-17 14:48:32.903445   721   754 I RILC-MTK: RIL_URC2_PROXY sleep
10-17 14:48:32.903507   721   751 I RILC-MTK: RIL_CMD_PROXY_1 wakeup
10-17 14:48:32.903529   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 wakeup
10-17 14:48:32.903535   721   751 I RILC-MTK: RIL_CMD_PROXY_1 sleep
10-17 14:48:32.903605   721   759 I RILC-MTK: RIL_ATCI2_PROXY wakeup
10-17 14:48:32.903635   721   759 I RILC-MTK: RIL_ATCI2_PROXY sleep
10-17 14:48:32.904416   721   753 D RILC-MTK: proxy id:5, proxyName: RIL_ATCI_PROXY
10-17 14:48:32.904416   721   748 I RILC-MTK: RIL_URC_PROXY sleep
10-17 14:48:32.904508   721   753 D RILC-MTK: OEM_HOOK_RAW pRI=0x7f9784c360 p=0x7f97856fc0 execute on RIL_ATCI_PROXY using channel 5
10-17 14:48:32.904543   721   753 D RILC    : callOnRequest for new vendor ril
10-17 14:48:32.904536   721   755 I RILC-MTK: RIL_CMD2_PROXY_3 sleep
10-17 14:48:32.904578   721   753 D RIL     : onRequest: OEM_HOOK_RAW, datalen = 19
10-17 14:48:32.904605   721   753 D RIL     : radioState:10
10-17 14:48:32.904652   721   753 D RIL     : data = AT+ERFTX=1,48,64,64, length = 19
10-17 14:48:32.904684   721   753 D AT      : AT send on RIL_ATCI_READER, tid:547982464064
10-17 14:48:32.904714   721   753 D AT      : AT> AT+ERFTX=1,48,64,64
10-17 14:48:32.904738   721   753 I AT      : AT write start
10-17 14:48:32.904762   721   757 I RILC-MTK: RIL_CMD2_PROXY_1 sleep
10-17 14:48:32.904986   537   713 D RILMUXD : [gsm0710muxd] 3614:poll_thread(): poll_thread select found
10-17 14:48:32.905064   537   713 D RILMUXD : [gsm0710muxd] 1045:pseudo_device_read(): Enter, LackofAtciChannel=0
10-17 14:48:32.905130   537   713 D RILMUXD : [gsm0710muxd] 657:write_frame(): Sending frame to channel 26
10-17 14:48:32.905234   537   713 D RILMUXD : [gsm0710muxd] 766:write_frame(): Write a frame on channel 26 with length 20
10-17 14:48:32.912995   537   705 D RILMUXD : [gsm0710muxd] 1643:gsm0710_base_buffer_get_frame(): Get a complete frame. ch:26, ctrl:239, len:6
10-17 14:48:32.913104   537   705 D RILMUXD : [gsm0710muxd] 2383:extract_frames(): Writing 6 byte frame received on channel 26 to /dev/pts/6
10-17 14:48:32.913213   537   705 D RILMUXD : [gsm0710muxd] 2403:extract_frames(): write() returned. Written 6/6 bytes of frame to /dev/pts/6
10-17 14:48:32.913275   537   705 D RILMUXD : [gsm0710muxd] 2408:extract_frames(): fsync() failed (-1, 22 - Invalid argument)
10-17 14:48:32.913482   721   770 I AT      : AT read end: 6
10-17 14:48:32.913578   721   770 D AT      : AT< OK
10-17 14:48:32.913615   721   770 D AT      : RIL_ATCI_READER Enter processLine:OK
10-17 14:48:32.913679   721   770 I AT      : AT read start
10-17 14:48:32.913758   721   753 D AT      : response received on RIL_ATCI_READER, tid:547982464064
10-17 14:48:32.913806   721   753 D RIL     : p_response->success = 1
10-17 14:48:32.913838   721   753 D RIL     : p_response->finalResponse = OK
10-17 14:48:32.913864   721   753 D RIL     : strLength = 6
10-17 14:48:32.913892   721   753 D RIL     : line = <
10-17 14:48:32.913892   721   753 D RIL     : OK
10-17 14:48:32.913892   721   753 D RIL     : >
10-17 14:48:32.913925   721   753 D RILC    : RequestComplete, RIL_SOCKET_1
10-17 14:48:32.913993   721   753 E RILC    : Send Response to RIL_SOCKET_1
10-17 14:48:32.914116   721   753 D RILC-MTK: proxyLoop free  pRI=0x7f9784c360 p=0x7f97856fc0 
10-17 14:48:32.914165   721   753 D RILC-MTK: proxyLoop free  pRequest=0x7f94cdaac0
10-17 14:48:32.914195   721   753 I RILC-MTK: RIL_ATCI_PROXY sleep
10-17 14:48:32.914538  1450  1606 D RILJ    : [9620]< OEM_HOOK_RAW [B@944e398 [SUB0]
